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NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Before Take-off" item count differs between passes (29 vs 5); verify nothing was dropped.

Before Every Flight
[ ]  Read Local Rules
[ ]  Check Weather
[ ]  Briefing Notices
[ ]  Check Booking Sheets
[ ]  Sign Autho Sheet
[ ]  Take Headset, and Fuel Strainer

Before Start
[ ]  Pre-flight
[ ]  Doors
[ ]  Seats
[ ]  Harness
[ ]  Headset
[ ]  (Top to Bottom, Left To Right)
[ ]  Electrics
[ ]  Ignition
[ ]  Flaps
[ ]  Fuel
[ ]  Throttle
[ ]  Prop Pitch
[ ]  Mixture
[ ]  Alt air
[ ]  Throttle friction
[ ]  Primer
[ ]  Brakes

Start Checks
[ ]  Call clear
[ ]  Look Out
[ ]  Engine Start

After Start
(ROAMIRS)
[ ]  Rpm
[ ]  Oil
[ ]  Alt air
[ ]  Mixture
[ ]  Instruments
[ ]  Radios
[ ]  Security

Taxi Checks
[ ]  Brakes
[ ]  Instruments

Before Take-off
[ ]  PARK PLANE INTO WIND
[ ]  Brakes
[ ]  Prop Blast
[ ]  Fuel
[ ]  Mixture
[ ]  Services
[ ]  Inspection Complete
[ ]  Closed
[ ]  Locked in Pos.
[ ]  Tight
[ ]  Plugged In
[ ]  Scan
[ ]  Avionics off, rotating beacon on, Master on, circuit breakers in.
[ ]  Key pos. at off
[ ]  Retracted
[ ]  Fuel Pump on 6 sec/On
[ ]  Open 1-2 cm
[ ]  (Not applicable)
[ ]  Full Mixture
[ ]  Set to QNH
[ ]  Finger Tight
[ ]  Prime a Few Times/out
[ ]  Applied
[ ]  Prop clear .... Make sure prop clear
[ ]  Start engine
[ ]  1200 rpm .... Oil press. Read in 30 seconds
[ ]  Set to QNH .... Mixture full, magnetos on
[ ]  L-R T-B .... Selected on, correct freq.
[ ]  Harness, brakes working .... Test

Taxi Checks — Instruments
[ ]  1. Compass (L-decreas R-increase)
[ ]  2. A/H Stable
[ ]  3. D.I. (Same as Compass)
[ ]  4. Turn left, ball to the right.  Turn right, ball to the left.
[ ]  5. Turn left, wings left, turn right, wings right
[ ]  6. ADF tracking
[ ]  7. Temps. & Press. In green
[ ]  8. Fuel check
[ ]  Set, Park Brake
[ ]  Check Behind
[ ]  Select fullest main tank/both/contents
[ ]  Fully rich
[ ]  Check all instruments

Engine Run Up
[ ]  Throttle .... Run Up RPM
[ ]  D.I. .... Set To Compass
[ ]  Suction .... Check 4-6
[ ]  Temps. and press. .... Normal
[ ]  Mixture .... Check till drop and back
[ ]  Prop Pitch .... Cycled
[ ]  Carburettor heat .... Check (Not more than 1.75)
[ ]  Magnetos .... One by one, Off and On
[ ]  Throttle .... Full back, and the 1200-rpm

Pre Take Off
(TO MANY CO-PILOTS GO FLY IN HEAVEN EARLY)
[ ]  Test Controls .... Correct and free movement
[ ]  Throttle and friction .... Idle and finger tight
[ ]  Trim .... For Take
[ ]  Master .... On
[ ]  Mixture .... Fully Rich
[ ]  Magnetos .... Both On
[ ]  Prop pitch .... Fully Fine
[ ]  Primer .... In And Locked
[ ]  Pressures and temps. .... All In green and in limits
[ ]  Gills .... Check Instruments
[ ]  Gyros .... Check Instruments
[ ]  Fuel .... Fuel pump on, fuel pressure
[ ]  Flaps .... Set for take-off
[ ]  Instruments .... Top to Bottom, left to Right
[ ]  Harness .... Tight and secured
[ ]  Hatches .... Closed and locked
[ ]  Electrics .... Check radio and lights

Take-Off Briefing
[ ]  Review Speeds .... Rotate, Climb and best glide
[ ]  Abort procedure .... Sufficient runway remaining
[ ]  Engine failure .... Insufficient runway, SFFF
[ ]  Departure Clearance .... Obtain and review
[ ]  Call “Ready”
[ ]  Strobes and Transponder .... S-On, T-Alt when cleared on runway
[ ]  Landing light .... On when cleared for take-off

Line up Checks
(WHEN DO FLAPS RETRACT)
[ ]  Windsock .... Stick into wind
[ ]  DI aligned .... Aligned with r/w heading
[ ]  Flaps .... Set for take-off
[ ]  Reference point .... Pick on end off runway

After Take-Off
300’ AGL
[ ]  Brakes .... Apply to stop wheels
[ ]  Undercarriage .... Retract
500’ AGL
[ ]  Brakes .... Apply
[ ]  Undercarriage .... Confirm up and locked
[ ]  Power .... Set for climb
[ ]  Pitch .... Set for climb
[ ]  Mixture .... Set for climb
[ ]  Fuel .... Fuel pump off, contents and selection
[ ]  Flaps .... Retract
[ ]  Instruments .... Check services and speeds
[ ]  Electrics .... Landing and strobes off

Pre-Manoeuvring Checks
(HASELL)
[ ]  Height .... 2000’ AGL after recovery
[ ]  Airframe .... Flaps, landing gear, brakes of, trim
[ ]  Security .... Hatches and Harnesses
[ ]  Engine .... Fuel cont. and pump on, mix. & Carb
[ ]  Location .... Contr. airspaces, towns, aerodroms etc.
[ ]  Look out .... 360* inspection turn

TOC, TOD & Field APP checks
(FREDAAS)
[ ]  Fuel .... Contents, selection
[ ]  Radios .... Correct freq.
[ ]  Engine .... Temp. and Press. (Nav. Carbheat)
[ ]  D.I. .... Set to compass
[ ]  Security .... Harnesses, doors, etc.

Downwind Checks
[ ]  Brakes .... Check for brake pressure
[ ]  Undercarriage .... Down
[ ]  Mixture .... Fully rich
[ ]  Prop Pitch .... Set for climb
[ ]  Power .... As required
[ ]  Fuel .... Fuel pump on, selection
[ ]  Flaps .... As Required
[ ]  Instruments .... Check Temps. And Press.
[ ]  Electrics .... Landing lights and strobes

Base Leg Checks
[ ]  Carbheat .... On below 2000rpm
[ ]  Power .... As Required
[ ]  Flaps .... As Required

Final APP Checks
(CUFFT)
[ ]  Carbheat .... Off
[ ]  Undercaraige .... Down and locked
[ ]  Fuel .... Fuel pump and, contents
[ ]  Flaps .... As required
[ ]  Trim .... Constant ROD

After Landing Checks
[ ]  Flaps .... Retracted
[ ]  Fuel Pump .... Off
[ ]  Landing Light .... Off
[ ]  Strobes .... Off
[ ]  Mixture .... Lean for Taxi
[ ]  Transponder .... Standby

Shut Down Checks
[ ]  Brakes .... On
[ ]  Avionics .... Off
[ ]  Magnetos .... Dead-cut check
[ ]  Mixture .... Full back
[ ]  Throttle .... Closed
[ ]  Magnetos .... Off
[ ]  Beacon .... Off
[ ]  Master .... Off
[ ]  Aircraft .... Secured

Engine Failure
(SFFF)
[ ]  Speed .... 65 Knots
[ ]  Field .... 30* inside heading
[ ]  Fault .... Find Fault
[ ]  Flaps .... Full

Engine Fire
[ ]  Engine Shutdown .... All Off
[ ]  Cabin Vent .... Closed
[ ]  Extinguish fire .... Use it
[ ]  Mayday Call .... Inform tower
[ ]  Land ASAP .... Bad luck!!!
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