Lancair 320 — L320-2 - Before Takeoff Checklist
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Before Takeoff Checklist
[ ]  Flaps .... SET
[ ]  Elevator Trim .... NEUTRAL
[ ]  Instruments .... SET
[ ]  GPS & Radios .... SET
[ ]  Fuel Totalizer .... CHECK
[ ]  Throttle .... 1800RPM
[ ]  Magnetos .... CHECK
[ ]  Prop .... CYCLE
[ ]  Oil Temp. & Press. .... CHECK
[ ]  Suction .... CHECK
[ ]  Mixture .... AS REQUIRED
[ ]  Throttle .... IDLE
[ ]  Pitot Heat .... AS REQUIRED
[ ]  Canopy Latches .... SECURE

Takeoff Checklist
[ ]  Clearance .... RECEIVED
[ ]  Time (Elapsed) .... START
[ ]  Instruments .... SET
[ ]  Transponder .... ON/ALT
[ ]  Safety (Lights, Latches, Belts) .... ON, SECURE
NOTE: Apply Full Power, Rotate at 60 - 65 KIAS, Accelerate to 90 – 100 KIAS
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