Lancair 320 — L320-5 - Emergency Checklist
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Engine Out Checklist  [EMERGENCY]
[ ]  MAX GLIDE .... 104 KIAS
[ ]  Flaps and Gear .... UP
[ ]  Landing Area .... DETERMINE

Engine Restart  [EMERGENCY]
[ ]  Magneto Switches .... ON
[ ]  Master Switch .... ON
[ ]  Aux Fuel Pump .... ON
[ ]  Prop Lever .... HIGH RPM
[ ]  Mixture .... FULL RICH
[ ]  Throttle .... ½” – 1” OPEN
[ ]  Start Button .... PRESS

Engine Secure / Landing  [EMERGENCY]
[ ]  Electrical Switches .... OFF
[ ]  Magneto Switches .... OFF
[ ]  Master Switches (3) .... OFF
[ ]  Mixture .... CUTOFF
[ ]  Canopy Latches .... UNLATCH
[ ]  Gear and Flaps (When Landing Assured) .... AS REQUIRED
[ ]  SPEED .... 70 KIAS MIN.

Emergency Gear Extension  [EMERGENCY]
[ ]  SPEED .... 90 KIAS
[ ]  Gear Circuit Breaker .... PULL
[ ]  Gear Handle .... DOWN
[ ]  Hydraulic Valve (Pilot’s Right Knee) .... MOVE DOWN TO VERTICAL POSITION
[ ]  Gear Lights .... ON, 3 GREEN
[ ]  Hydraulic Valve .... MOVE UP TO HORIZONTAL POSITION
[ ]  Gear Circuit Breaker .... PUSH IN
NOTE: If Main Gear fails to lock, yaw aircraft in direction of unlocked gear. If Nose Gear fails to lock, reduce speed to 80 - 85 KIAS, exert positive G forces until all Gear Lights illuminate.
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