Lancair 320 — L320-6 - Specs Page
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Operating Specifications - N10ZC
DIMENSIONS
[ ]  Length: 21’00 ¾”
[ ]  Width: 23’08 ½”
[ ]  Height: 5’10 ¼”
MIN. TURNING CIRCLE
[ ]  Wingtip: 31’00”
[ ]  Gear: 15’06”
[ ]  Main Gear Track: 7’03”
SPEEDS
[ ]  VA .... 143 KIAS
[ ]  Vs/Vsfe (No Stall Warning Horn) .... 70/67 KIAS
GLIDE RATIO
[ ]  1/15.8; 1,000 ft. / 2.4 NM
LOAD FACTORS
[ ]  +9.5/-4.5 G
FUEL
[ ]  100 LL, Total 41 gal., Useable 39 gal.
OIL
[ ]  Aeroshell 15W-50, 8 qt. max, 7-7.5 qt. norm.
BAGGAGE CAPACITY
[ ]  70 lbs.
WEIGHT & BALANCE
[ ]  Main Gear: Arm 76.56
[ ]  Nose Gear: Arm 32.62
[ ]  Left Seat: Arm 77.5
[ ]  Right Seat: Arm 77.5
[ ]  Wing Fuel: Arm 73.8
[ ]  Baggage: Arm 80.0
[ ]  TOTALS
[ ]  LIMITS: 1800 lb, Arm 64–69.8
NOTE: * Main and Nose Gear weights include full Header Tank Fuel and Engine Oil.
NOTE: ** Total Wing Fuel is 32 gals., 31 gal. useable. Fuel weight 6.0 lbs./gal..
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