Lancair 350 — WM_Columbia_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Speeds" item count differs between passes (6 vs 5); verify nothing was dropped.

Starting Engine
[ ]  Mixture .... FULL RICH
[ ]  Prop .... FULL POWER
[ ]  Vapor Suppression .... OFF
[ ]  Induction Heated Air .... OFF
[ ]  Strobe Lights .... ON
[ ]  Throttle .... OPEN 1”
[ ]  Crosstie .... OFF
[ ]  Bus Switches .... ON
[ ]  Primer .... PRESS
[ ]  Throttle .... OPEN 1/8”
[ ]  Prop Area .... CLEAR
[ ]  Ignition .... ENGAGE
[ ]  Oil Pressure
[ ]  Engine Instruments
[ ]  Ammeter .... SELECT AMM
[ ]  Avionics Master .... ON

Before Taxi
[ ]  Crosstie Operation .... VERIFY
[ ]  Speedbrakes .... TEST/STOW
[ ]  Flaps .... TAKEOFF
[ ]  Flight Controls .... FREE/CLEAR
[ ]  Trim .... CENTERED
[ ]  Radios .... ON/SET
[ ]  IFR Clearance .... AS REQ’D
[ ]  GPS Flight Plan .... INPUT
[ ]  Transponder .... SET CODE
[ ]  Autopilot Master .... AP/FD
[ ]  Navaids/CDI .... SET/CHECK
[ ]  Headings .... VERIFY
[ ]  Heading/Altitude/VSI Bugs .... SET
[ ]  Autopilot Test .... COMPLETE
[ ]  Fuel Gauges/ .... VERIFY/CHECK LIGHT
[ ]  Fuel Selector .... TEST/SET FULLEST
[ ]  Chart Page .... SELECT DEPARTURE
[ ]  Map Page .... SET 5-20NM
[ ]  Engine Page .... SELECT/MONITOR
[ ]  Engine Instruments
[ ]  Annunciator Panel/CO Alert .... TEST/CLEAR
[ ]  Ammeters .... CHECK
[ ]  Lights .... AS REQ’D

Before Takeoff
[ ]  Radios .... TWR/DEPX
[ ]  Doors .... CLOSE/LATCH/UNLOCKED
[ ]  Crosstie .... OFF
[ ]  Engine Runup .... 1700 RPM
[ ]  Magnetos .... CHECK 25-150 RPM DROP
[ ]  Prop .... CHECK
[ ]  Fuel Selector .... CHECK DETENT/WARN
[ ]  Flight Controls .... FREE/CLEAR
[ ]  Annunciator Panel .... TEST/CLEAR
[ ]  Door Seals .... ON
[ ]  Brakes .... OFF

Crossing Hold Short
[ ]  Lights .... AS REQUIRED
[ ]  Pitot Heat .... AS REQUIRED
[ ]  Boost Pump .... ARMED
[ ]  Flaps .... TAKEOFF
[ ]  Speedbrakes .... STOWED
[ ]  Trim .... CENTERED

After Takeoff – 500 AGL
[ ]  Flaps .... UP
[ ]  Prop .... 2500-2700 RPM
[ ]  Landing Light .... OFF
[ ]  Engine Page .... NORMALIZE
[ ]  Map Page .... SELECT

Climb – 5000 AGL
[ ]  Boost Pump .... DEARMED
[ ]  Lights .... AS REQ’D
[ ]  Mixture .... LEAN AS REQ’D
[ ]  Pitot Heat .... AS REQ’D
[ ]  Deice .... AS REQ’D
[ ]  Fuel Selector .... SWITCH TANKS

Cruise
[ ]  Boost Pump .... CHECK DEARMED
[ ]  Throttle .... AS REQ’D
[ ]  Prop .... AS REQ’D
[ ]  Mixture .... LEAN ASSIST

Speeds
NOTE: Best Angle (Vx): 80 KIAS (SL)/84 KIAS (10k MSL)
NOTE: Best Rate (Vy): 106 KIAS (SL)/93 KIAS (10k MSL)
NOTE: Maneuver (Va): 148 KIAS (3400#)/127 KIAS (2500#)
NOTE: Approach (VRef): 90 KIAS
NOTE: Stall Flaps Up (VS0): 71 KIAS
NOTE: Stall Flaps Land (VS1): 57 KIAS

Descent
[ ]  ATIS .... OBTAIN
[ ]  Altimeter .... SET
[ ]  Fuel Tank .... SELECT
[ ]  Power Settings .... ADJUST
[ ]  Engine Page .... NORMALIZE
[ ]  Mixture .... ADJUST
[ ]  Chart Page .... SELECT APPROACH

Approach
[ ]  GPS Approach .... VERIFY PROGRAMMED
[ ]  Navaids .... TUNE/VERIFY
[ ]  CDI/NAV2 .... SELECT/VERIFY
[ ]  Radios .... SET
[ ]  GPS Approach .... ACTIVATE WHEN NEEDED
[ ]  Landing Light .... ON
[ ]  Fuel Tank .... SELECT
[ ]  Boost Pump .... CHECK DEARMED
[ ]  Prop .... ADJUST
[ ]  Mixture .... ADJUST
[ ]  Seat Belts .... FASTENED

Landing
[ ]  Fuel Tank .... SELECT
[ ]  Mixture .... RICH
[ ]  Prop .... MAX RPM
[ ]  Speedbrakes .... STOWED
[ ]  Flaps .... T/O or LAND

Go-Around/Missed Approach
[ ]  Throttle .... MAX POWER
[ ]  Speedbrakes .... VERIFY STOWED
[ ]  Flaps .... SET TAKEOFF
[ ]  Positive Rate of Climb .... ESTABLISH
[ ]  Flaps .... UP
[ ]  Chart Page .... SELECT
[ ]  GPS OBS Button .... PRESS/RELEASE
[ ]  Missed Approach Instructions .... FOLLOW

Clearing Runway
[ ]  Lights .... OFF/AS REQ’D
[ ]  Flaps .... UP
[ ]  Speedbrakes .... STOW
[ ]  Door Seal .... OFF
[ ]  Pitot Heat/Deice .... OFF
[ ]  Autopilot Master .... OFF
[ ]  Time .... NOTE

EMERGENCIES — Speeds  [EMERGENCY]
NOTE: Engine Out (Flaps 0): 106 KIAS
NOTE: Engine Out (Flaps 10): 93 KIAS
NOTE: Precautionary Landing (Flaps 40): 78 KIAS
NOTE: Power-off Approach (Flaps 0): 106 KIAS
NOTE: Power-off Approach (Flaps 40): 90 KIAS

Engine Failure Below 400 AGL  [EMERGENCY]
[ ]  Airspeed .... 90 KIAS
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Ignition .... OFF
[ ]  Flaps .... LAND
[ ]  Master Switches .... OFF

Engine Failure on Takeoff Above 400 AGL  [EMERGENCY]
[ ]  Airspeed .... 106 KIAS
[ ]  Flaps .... UP
[ ]  Mixture/Throttle .... RICH/FULL OPEN
[ ]  Boost Pump .... ARMED

Engine Failure in Flight (Restart)  [EMERGENCY]
[ ]  Airspeed .... 106 KIAS
[ ]  Landing Site .... SELECT
[ ]  Fuel Selector Valve .... FULLEST TANK
[ ]  Mixture/Throttle .... RICH/FULL OPEN
[ ]  Boost Pump .... ARMED
[ ]  Ignition .... BOTH

Engine Fire in Flight  [EMERGENCY]
[ ]  Throttle .... OFF
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Heating/Ventilation System .... OFF
[ ]  Master Switches .... OFF
[ ]  Nav/Comm Bypass .... ON
[ ]  Airspeed .... 179 KIAS to Extinguish
[ ]  Landing .... POWER-OFF LANDING

Electrical Fire in Flight  [EMERGENCY]
[ ]  Heating/Ventilation Controls .... FULL OPEN
[ ]  Master Switches .... OFF
[ ]  Oxygen .... OFF
[ ]  Avionics Master .... OFF
[ ]  Trim System Switch .... OFF
[ ]  Nav/Comm Bypass .... ON
[ ]  Book Procedures .... PERFORM IF ABLE
[ ]  Landing .... PRECAUTIONARY LANDING
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