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START
[ ]  Fuel Selector .... ON
[ ]  Parking Brake .... SET
[ ]  Alternate Air .... OFF
[ ]  Fuel Boost Pump .... .AUTO
[ ]  Master Switch (BAT & ALT) .... ON
[ ]  Annunciator Lights .... TEST/HIGH
[ ]  VM1000 .... VOLTS > 11.4v
[ ]  FADEC A & B .... ON
[ ]  Ignition Key .... (L), boost pump on
[ ]  HSA .... .TEST/HIGH
[ ]  Throttle .... CHECK WOT, ¼”
[ ]  Ignition Key .... START

ENGINE FIRE DURING START  [EMERGENCY]
Engine fire during start
[ ]  1. Ignition Switch [MEMORY] .... START
NOTE: Continue turning the engine over.
NOTE: If Engine Starts:
[ ]  2. Power .... .1700 RPM (2 min.)
[ ]  3. Engine .... SHUT DOWN
NOTE: If Engine does NOT Start:
[ ]  4. Ignition Switch .... START
[ ]  5. Throttle .... .FULL FORWARD
[ ]  6. FADEC A and B PWR Switches .... .OFF
[ ]  7. Fuel Selector Valve .... OFF
[ ]  8. Cranking .... TERMINATE
[ ]  9. Ignition Switch .... .OFF
[ ]  10. Master Switch .... .OFF
[ ]  11. Airplane .... .EVACUATE
[ ]  12. Fire .... .EXTINGUISH
[ ]  13. Fire Damage .... .INSPECT

AFTER START
[ ]  Throttle .... 800-1000RPM
[ ]  VM 1000 .... .IN LIMITS
[ ]  Cockpit Rheostat switches .... SET
[ ]  Lights .... AS REQUIRED
[ ]  Avionics Master .... ON
[ ]  Flaps .... 0◦
[ ]  Transponder .... STBY
[ ]  Flight Instruments .... .CHECK/SET
[ ]  Comm/Nav Aids .... CHECK/SET
[ ]  Fuel Boost Pump .... AS REQUIRED

RUN-UP
[ ]  Fuel Boost Pump .... AUTO
[ ]  Fuel Selector .... ON
[ ]  Parking Brake .... SET
[ ]  Canopy Doors .... CLOSED/SECURE
[ ]  Throttle .... 1700RPM
[ ]  Alternate Air .... CHECK
[ ]  Fuel Boost Pump .... ON/OFF/AUTO
[ ]  Annunciator Lights .... TEST/HIGH
[ ]  HSA .... TEST/HIGH
[ ]  VM1000 .... IN LIMITS
[ ]  FADEC Power B .... CHECK
[ ]  FADEC Power A .... CHECK
[ ]  Ignition L/R .... DROP 10-150 RPM
CAUTION: FADEC CAUTION
[ ]  Throttle .... IDLE

BEFORE TAKEOFF
[ ]  Seatbelts/Harnesses .... FASTENED
[ ]  Fuel Quantity .... .VERIFY
[ ]  Flight Controls .... FREE /CORRECT
[ ]  Flight Instruments .... CHECK/SET
[ ]  Nav/Comm .... CHECK/SET
[ ]  Flaps .... 20°
[ ]  Trim .... SET for TAKEOFF
[ ]  Transponder .... ALT
[ ]  Parking Brake .... RELEASE

AFTER LANDING
[ ]  Flaps .... RETRACT
[ ]  Transponder .... STANDBY
[ ]  Lights .... .AS REQUIRED

SHUTDOWN
[ ]  Avionics Master .... .OFF
[ ]  Ignition Key .... OFF
[ ]  FADEC A & B .... .OFF
[ ]  All Light Switches .... OFF
[ ]  All Electrical Switches .... .OFF
[ ]  Master Switch .... OFF
[ ]  Parking Brake .... .AS REQUIRED

SPEEDS AND APPROACH
NOTE: Vr :55; Vx: 70 ; Vy: 80; Best Glide: 80
NOTE: Approach: Flaps 30: 65-70;
NOTE:       Flaps 20: 70-75; Flaps Up: 80-85
NOTE: Va 100 KIAS (1653 lbs) / 94 (1450 lbs)

ENGINE FAILURE AFTER TAKEOFF  [EMERGENCY]
Engine failure after takeoff
[ ]  1. Best Glide or Landing Speed (as appropriate) [MEMORY] .... ESTABLISH
[ ]  2. Flaps [MEMORY] .... AS REQUIRED
NOTE: If time permits:
[ ]  3. Ignition Switch .... OFF
[ ]  4. FADEC A and B PWR Switches .... OFF
[ ]  5. Master Switch .... OFF
[ ]  6. Throttle .... IDLE
[ ]  7. Fuel Selector Valve .... OFF
[ ]  8. Seat Belts/Shoulder Harness .... .SECURE

FORCED LANDING  [EMERGENCY]
Forced landing
[ ]  1. Establish Best Glide Attitude [MEMORY] .... 80 KIAS
[ ]  2. Radio .... MAYDAY 121.5 MHz)
[ ]  3. Transponder .... .SQUAWK 7700
[ ]  4. ELT (if off airport) .... ACTIVATE
[ ]  5. Ignition Switch .... OFF
[ ]  6. FADEC A and B PWR Switches .... OFF
[ ]  7. Fuel Boost Pump Mode Switch .... OFF
[ ]  8. Throttle .... IDLE
[ ]  9. Fuel Selector Valve .... OFF
[ ]  10. Flaps (when field is made) .... . AS REQUIRED or 30°
[ ]  11. Master Switch .... OFF
[ ]  12. Belts/ Harness .... SECURE
WARNING: WARNING: Flaps will not operate when Master Switch is off.

ENGINE FAILURE IN FLIGHT  [EMERGENCY]
Engine failure in flight
[ ]  1. Best Glide Attitude [MEMORY] .... 80 KIAS
[ ]  2. Fuel Selector Valve .... CHECK ON
[ ]  3. Throttle .... OPEN ¾ INCH
[ ]  4. Fuel Boost Pump .... ON
[ ]  5. FADEC A and B PWR Switches .... . RECYCLE SIMULTANIOUSLY
[ ]  6. Ignition Switch .... CHECK BOTH
[ ]  7. Ignition Switch (NOT Windmilling) .... START
[ ]  8. Throttle .... BEST OPERATION
[ ]  9. Repeat steps 2 – 6 prop windmilling.
[ ]  10. No Start .... Forced Landing checklist.

ENGINE PARTIAL POWER LOSS  [ABNORMAL]
Engine partial power loss
[ ]  1. Fuel Boost Pump Mode Switch .... ON
[ ]  2. Fuel Selector Valve .... CHECK ON
[ ]  3. Alternate Induction Air .... PULL ON
[ ]  4. Ignition Switch .... .CHECK R, L, BOTH
[ ]  5. LAND .... AS SOON AS PRACTICAL

ENGINE FIRE IN FLIGHT  [EMERGENCY]
Engine fire in flight
[ ]  1. Fuel Selector Valve [MEMORY] .... .OFF (lift knob to turn off)
[ ]  2. Throttle .... IDLE
[ ]  3. Cabin Heat .... OFF
[ ]  4. Fuel Boost Pump Mode Switch .... OFF
[ ]  5. FADEC A & B PWR Switches .... OFF
[ ]  6. Ignition Switch .... OFF
[ ]  7. Perform Forced Landing checklist
WARNING: WARNING : No restart.

CABIN FIRE IN FLIGHT  [EMERGENCY]
Cabin fire in flight
[ ]  1. Master Switch [MEMORY] .... .OFF
[ ]  2. FADEC PWR A Switch .... .OFF
[ ]  3. Avionics Master Switch .... OFF
[ ]  4. All Electrical Switches .... OFF (Except FADEC PWR B Switch)
WARNING: WARNING: Turning off FADEC PWR B switch when Master Switch is OFF will cause immediate loss of engine power.
[ ]  5. Cabin Heat .... OFF
[ ]  6. Fire Extinguisher .... ACTIVATE
[ ]  7. Air Vents .... OPEN TO VENT CABIN
[ ]  8. LAND .... AS SOON AS PRACTICAL

SPIN RECOVERY  [EMERGENCY]
Spin
[ ]  1. Throttle [MEMORY] .... IDLE
[ ]  2. Ailerons .... NEUTRAL
[ ]  3. Rudder .... FULL OPPOSITE DIRECTION OF SPIN
[ ]  4. Control Stick .... FORWARD
[ ]  5. Rudder .... Neutralize
[ ]  6. Recover from dive
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