Mooney M20J_MSE — mooney_m20j_checklist_mwaugh
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content_gap: Section "Before Start" item count differs between passes (165 vs 16); verify nothing was dropped.

Before Start
[ ]  Preflight .... COMPLETE
[ ]  Fuel Quantity .... ____ G
[ ]  Paperwork .... COMPLETE
[ ]  Radio Master .... OFF
[ ]  Transponder .... STAND-BY
[ ]  Mixture .... CUT-OFF
[ ]  Propeller .... HIGH
[ ]  Seats/Seat Belts .... SECURE
[ ]  Fuel Selector .... CORRECT TANK
[ ]  Briefing .... Complete
ELECTRICAL POWER ON
[ ]  Master .... ON
[ ]  Anti-Collision .... ON
[ ]  Annunciators .... TEST
[ ]  Electric Stand-by Vac. .... CHECK
[ ]  Brakes .... SET
STARTING
[ ]  Fuel Pump .... ON
[ ]  Mixture .... RICH (7 secs)
[ ]  Fuel Pump .... OFF
[ ]  Throttle .... OPEN ¼”
[ ]  Area .... CLEAR
[ ]  Engine .... START
[ ]  Mixture .... RICH
AFTER START
[ ]  Engine/Inst. .... NORMAL
[ ]  Mixture .... LEAN
[ ]  Trim .... ON
[ ]  Lights .... AS REQUIRED
[ ]  Radios .... ON/SET
[ ]  Time Out .... ______
[ ]  Autopilot .... CHECK
[ ]  Stand-by Vacuum .... CHECK
[ ]  ATIS/AWOS .... OBTAIN
[ ]  Altimeter .... SET
[ ]  Heading .... SET
TAXI CHECKS
[ ]  Brakes .... CHECK
[ ]  Flight Instruments. .... CORRECT
RUNUP
[ ]  Mixture .... RICH
[ ]  Engine .... 1900 RPM
[ ]  Magnetos .... CHECKED
[ ]  Propeller .... CHECKED
[ ]  Electrical .... CHECKED
[ ]  Vacuum .... CHECKED
BEFORE TAKEOFF
[ ]  Controls .... FREE/CORRECT
[ ]  Seats/Seat Belts .... SECURE
[ ]  Trim .... TAKEOFF
[ ]  Flaps .... TAKEOFF
[ ]  Autopilot .... OFF
[ ]  Annunciator Lts .... CHECKED
[ ]  Door/Window .... LATCHED
[ ]  Fuel Pump .... ON
[ ]  Mixture .... RICH
[ ]  Transponder .... ALT
[ ]  Pitot Heat .... AS REQUIRED
[ ]  Lights .... ON
TAKING RUNWAY
[ ]  Flaps .... Takeoff
[ ]  Heading .... RUNWAY
[ ]  Time Off .... ______
TAKEOFF
[ ]  Rotate .... 63 K
[ ]  Climb .... 85 K
[ ]  Gear .... UP (No Runway)
[ ]  Flaps .... UP
500 AGL
[ ]  Throttle .... 25”
[ ]  Propeller .... 2500 RPM
[ ]  Climb .... 100 K
CLIMB
[ ]  Gear .... UP
[ ]  Flaps .... UP
[ ]  Boost Pump .... OFF
[ ]  Power/RPM .... 25”/2500
[ ]  Mixture .... LEAN (if needed)
[ ]  Cowl Flaps .... TRAIL
CRUISE
[ ]  Power/RPM .... SET
[ ]  Cowl Flaps .... CLOSE
[ ]  Ram Air .... AS NEEDED
[ ]  Mixture .... LEAN
[ ]  Landing Light .... OFF
[ ]  Engine Inst. .... CHECK
[ ]  Ammeter .... CHECK
[ ]  Vacuum .... CHECK
APPROACH
[ ]  Seats/Belts .... SECURE
[ ]  Fuel Quantity .... ______ G
[ ]  Ram Air .... OFF
[ ]  ATIS/AWOS .... OBTAINED
[ ]  Briefing .... COMPLETE
[ ]  Radios .... SET
[ ]  Heading .... SET
[ ]  Altimeter .... SET
[ ]  Boost Pump .... ON
[ ]  Lights .... ON
FINAL APPROACH FIX
[ ]  Instruments .... NO FLAGS
[ ]  Gear .... DOWN
[ ]  Flaps .... AS REQUIRED
LANDING
[ ]  Boost Pump .... ON
[ ]  Gear .... DOWN
[ ]  Mixture .... RICH
[ ]  Propeller .... ADVANCED
[ ]  Cowl Flaps .... OPEN
[ ]  Flaps .... LANDING
APPROACH SPEEDS
[ ]  Downwind .... 100 K
[ ]  Gear/Flaps .... 80 K
[ ]  Short Final .... 71 K
SPEEDS
[ ]  VX .... 66 K
[ ]  VY .... 85 K
[ ]  Best Glide .... 90 K
[ ]  VA .... 120K
[ ]  VFE .... 115 K
[ ]  VLO (Retract) .... 105 K
[ ]  VLO (Extend) .... 130 K
[ ]  VLE .... 130 K
POWER SETTINGS
CONDITION | MP | RPM | GPH
[ ]  Takeoff .... Full | 2700 | 18
[ ]  Initial Climb .... 25” | 2500 | 14
[ ]  Cruise Climb .... 24” | 2500 | 10
[ ]  Cruise .... 24 | 2400 | 9.6
[ ]  Cruise .... 22 | 2400 | 8.2
[ ]  Cruise .... 22 | 2200 | 7.8
[ ]  Cruise .... 18 | 2200 | 6.8
[ ]  Descent .... 16 | 2200/2400 | 6.1
AFTER LANDING
[ ]  Time Down .... ______
[ ]  Flaps .... UP
[ ]  Cowl Flaps .... OPEN
[ ]  Mixture .... LEAN
[ ]  Transponder .... STANDBY
[ ]  Pitot Heat .... OFF
[ ]  Boost Pump .... OFF
[ ]  Lights .... AS REQUIRED
[ ]  Trim .... TAKEOFF
SHUTDOWN
[ ]  Radios .... OFF
[ ]  Switches .... OFF
[ ]  Mixture .... CUT-OFF
[ ]  Throttle .... CLOSE
[ ]  Magnetos .... OFF
[ ]  Master .... OFF
SECURING
[ ]  Flight Controls .... SECURE
[ ]  Window .... CLOSED
[ ]  Sun Shields .... INSTALLED
[ ]  Tie-downs .... INSTALLED
[ ]  Baggage Lights .... OFF
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