Mooney M20J_MSE — mooney_m20j_procedures_mwaugh
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

TAKEOFF
NORMAL TAKEOFF – FLAPS 15°
[ ]  Full Power .... SET
[ ]  Rotate VR 62K – Takeoff VLOF 70K .... ROTATE
[ ]  Climb VY 85K .... CLIMB
[ ]  No Runway – Positive Rate – GEAR UP .... GEAR UP
[ ]  500' AGL – 105K .... 105K
[ ]  500' AGL – 25" / 2500 RPM – Takeoff Checklist
[ ]  1000' AGL – Takeoff/Climb Checklist
MAXIMUM PERFORMACE TAKEOFF – FLAPS 15°
[ ]  Hold Brakes .... HOLD
[ ]  Full Power .... SET
[ ]  Release Brakes .... RELEASE
[ ]  Rotate VR 62K – VLOF 66K .... ROTATE
[ ]  Climb VX 66K to 50' .... CLIMB
[ ]  Climb VY 85K .... CLIMB
[ ]  No Runway – Positive Rate – GEAR UP .... GEAR UP
[ ]  500' AGL – 105K .... 105K
[ ]  500' AGL – 25" / 2500 RPM – Takeoff Checklist
[ ]  1000' AGL – Takeoff/Climb Checklist

APPROACH
NORMAL APPROACH
[ ]  Approach Checklist
[ ]  Downwind 105K (15") .... 105K (15")
[ ]  GEAR DOWN / FLAPS 30° .... GEAR DOWN / FLAPS 30°
[ ]  Descend – 80K – 2000 RPM .... 80K – 2000 RPM
[ ]  “GEAR DOWN – CHECKLIST” .... CALLED
[ ]  Base – “GUMPFF” .... CALLED
[ ]  400' AGL – “GEAR DOWN STABILIZED” .... CALLED
[ ]  Short Final – Power to IDLE – 71K .... POWER IDLE – 71K
[ ]  Touchdown 71K .... 71K
MAXIMUM PERFORMANCE APPROACH
[ ]  As Normal Approach

INSTRUMENT APPROACHES
ILS APPROACH
[ ]  Approach Checklist
[ ]  105K to Intercept (15") .... 105K (15")
[ ]  G/S Int. – GEAR DOWN .... GEAR DOWN
[ ]  G/S Intercept – “NO FLAGS” .... CALLED
[ ]  G/S Descent - 90K (15") .... 90K (15")
[ ]  “GEAR DOWN – CHECKLIST” .... CALLED
[ ]  1000' AGL “GUMPFF” .... CALLED
[ ]  400' AGL “GEAR DOWN – STABILIZED” .... CALLED
[ ]  100' ABOVE MINS “100 TO GO” .... CALLED
[ ]  “LANDING” – FLAPS 30° .... FLAPS 30°
[ ]  Short Final – POWER IDLE – 71K .... POWER IDLE – 71K
[ ]  Touchdown 71K .... 71K
NON-PRECISION APPROACH
[ ]  Approach Checklist
[ ]  105K Procedure Turn (15") .... 105K (15")
[ ]  2E – 2Miles FAF GEAR DOWN .... GEAR DOWN
[ ]  FAF – “NO FLAGS” .... CALLED
[ ]  FAF Descent – 90K (15") .... 90K (15")
[ ]  “GEAR DOWN – CHECKLIST” .... CALLED
[ ]  1000' AGL “GUMPFF” .... CALLED
[ ]  100' ABOVE MINS “100 TO GO” .... CALLED
[ ]  MDA – Level (18") .... LEVEL (18")
[ ]  Leaving MDA – FLAPS 30° .... FLAPS 30°
[ ]  400' AGL “GEAR DOWN – STABILIZED” .... CALLED
[ ]  Short Final – POWER IDLE – 71K .... POWER IDLE – 71K
[ ]  Touchdown 71K .... 71K
CIRCLE TO LAND
[ ]  Turning Final, Leaving MDA – FLAPS 25° .... FLAPS 25°
[ ]  Short Final – POWER IDLE – 71K .... POWER IDLE – 71K
[ ]  Touchdown 71K .... 71K

MISSED APPROACH
[ ]  Full Power – PITCH 85K .... FULL POWER – 85K
[ ]  FLAPS 15° .... FLAPS 15°
[ ]  Positive Rate – GEAR UP .... GEAR UP
[ ]  FLAPS 0° .... FLAPS 0°
[ ]  500' AGL – 100K .... 100K
[ ]  500' AGL - 25" / 2500 RPM .... 25" / 2500 RPM
[ ]  1000' AGL - Takeoff/Cruise Checklist
[ ]  HOLDING SPEED 90K .... 90K

STEEP TURNS
[ ]  SPEED 120K - 20" / 2300 RPM .... 120K - 20" / 2300 RPM
[ ]  50° BANK – POWER 23" - TRIM .... POWER 23" - TRIM

STALLS and SLOW FLIGHT
SLOW FLIGHT
[ ]  Clearing Turns – 105K (15") .... 105K (15")
[ ]  GEAR DOWN / FLAPS 30° .... GEAR DOWN / FLAPS 30°
[ ]  GEAR DOWN Checklist
[ ]  LEVEL FLIGHT – 65K .... 65K
[ ]  CRUISE POWER .... SET
[ ]  FLAPS 0° / SPEED 85K .... FLAPS 0° / 85K
[ ]  Positive Rate – GEAR UP .... GEAR UP
[ ]  SPEED 85K .... 85K
STALL – POWER OFF
[ ]  Clearing Turns – 105K (15") .... 105K (15")
[ ]  GEAR DOWN / FLAPS 30° .... GEAR DOWN / FLAPS 30°
[ ]  GEAR DOWN Checklist
[ ]  DESCENT – 80K .... 80K
[ ]  POWER to IDLE – Pitch to BUFFET .... POWER IDLE – BUFFET
[ ]  PITCH DOWN – FULL POWER .... PITCH DOWN – FULL POWER
[ ]  Positive Rate – GEAR UP – SPEED 85K .... GEAR UP – 85K
[ ]  FLAPS 0° / SPEED 85K .... FLAPS 0° / 85K
[ ]  SPEED 85K .... 85K
STALL – POWER ON
[ ]  Clearing Turns – 105K (15") .... 105K (15")
[ ]  POWER 13" / SPEED 70K .... POWER 13" / 70K
[ ]  POWER 21" / Pitch to BUFFET .... POWER 21" / BUFFET
[ ]  PITCH DOWN – FULL POWER .... PITCH DOWN – FULL POWER
[ ]  SPEED 85K .... 85K
[ ]  SPEED 85K .... 85K

CONFIGURATION CHECKLIST
[ ]  Fuel Selectors – ON .... ON
[ ]  Cowl Flaps – OPEN .... OPEN
[ ]  Mixtures – RICH .... RICH
[ ]  Prop – HIGH .... HIGH
[ ]  Fuel Pumps - ON .... ON
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