Mooney M20J_MSE — phil_vergese_m20j
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

INITIAL PREFLIGHT
[ ]  Mags .... OFF
[ ]  Gear Switch .... DOWN
[ ]  Master Switch .... ON
[ ]  Fuel Gauges .... NOTE QUANTITY
[ ]  Annc. Lights .... PRESS TO TEST
[ ]  Nav, Strobe, Landing Light .... ON
OUTSIDE
[ ]  Wingtip & Tail Lights .... CHECK
[ ]  Stall Horn .... TEST
INSIDE
[ ]  Nav, Strobe, Landing Light .... OFF
[ ]  Electric Gyros .... SPOOLING
[ ]  Autopilot .... TEST
[ ]  Master .... OFF
[ ]  Alternate Static .... IN
[ ]  Controls .... FREE & CORRECT
[ ]  Fuel Drain .... LEFT & RIGHT (5 sec)
[ ]  Check Drained Fuel .... OUTSIDE
RIGHT REAR
[ ]  Grab Fuel Tester & Rag
[ ]  Antennas .... CHECK
[ ]  Right Side Static Port .... CLEAR
EMPENNAGE
[ ]  Tail Tiedown .... REMOVE
[ ]  Elevator & Rudder Attach .... CHECK
[ ]  Tail Light .... SECURE
[ ]  Tail Area Frost .... REMOVE
LEFT REAR
[ ]  Left Side Static Port .... CLEAR
[ ]  Tail Cone Access Door .... SECURE
[ ]  Static System Drain .... CHECK
LEFT WING
[ ]  Wing Skins .... CHECK
[ ]  Frost .... REMOVE
[ ]  Flap & Aileron Attach Points .... CHECK
[ ]  Wing Tip .... CHECK
[ ]  Leading Edge & Stall Strip .... CHECK
[ ]  Pitot Tube .... CHECK (remove cover)
[ ]  Stall Switch .... CHECK
[ ]  Fuel Tank .... CHECK QUANTITY
[ ]  Tiedown .... REMOVE
[ ]  Left Gear & Discs (30 psi) .... CHECK
[ ]  Fuel Drain .... SAMPLE
[ ]  Tank Vent .... UNOBSTRUCTED
[ ]  Pitot System Drain .... CHECK
LEFT COWLING
[ ]  Central Drain Valve .... CLOSED
[ ]  Windshield .... CLEAN
[ ]  Cowl Fastners .... SECURE
N201UT V2.3
PROP AREA
[ ]  Propeller .... CHECK
[ ]  Alternator Belt .... CHECK
[ ]  Air Filter .... CHECK
[ ]  Ram Air Door .... CLOSED
[ ]  Landing Light .... CHECK
[ ]  Nose Gear & Discs (49 psi) .... CHECK
RIGHT COWLING
[ ]  Cowl Fastners .... SECURE
[ ]  Oil Level .... CHECK (>7 gal)
[ ]  Windshield .... CLEAN
RIGHT WING
[ ]  Fuel Drain .... SAMPLE
[ ]  Tank Vent .... UNOBSTRUCTED
[ ]  Right Gear & Discs (30 psi) .... CHECK
[ ]  Tiedown .... REMOVE
[ ]  Fuel Tank .... CHECK QUANTITY
[ ]  Leading Edge & Stall Strip .... CHECK
[ ]  Wing Skins .... CHECK
[ ]  Frost .... REMOVE
[ ]  Wing Tip .... CHECK
[ ]  Flap & Aileron Attach Points .... CHECK

PASSENGER BRIEFING
[ ]  Bathroom Check
[ ]  Cell phones OFF
[ ]  "No Step" areas
[ ]  Treat all props as live. "Clear"
NOTE: Help Spotting Planes. Best way is to look at one spot for 2-3 seconds.
NOTE: Turbulence. Uncomfortable for us, but no danger to the aircraft.
NOTE: Ears. Let me know if you feel pain. Swallow or yawn as we climb & descend
NOTE: Questions (now or in-flight). No talking during takeoff and landing
NOTE: Seatbelts at all times. No smoking.
NOTE: If there's anything I do with the airplane that makes you uncomfortable, let me know right away.
NOTE: If you feel queasy tell me right away, look outside, nearest vent. Location of airsickness bags.
INSIDE PLANE
NOTE: Don't touch the anything without asking! If seat slips on takeoff, don't grab the yoke. Rudders.
[ ]  Vents (location & operation)
NOTE: Intercom is voice activated. I do checklists aloud.
NOTE: Radio callsign. Stop talking during incoming radio traffic. Hand up.
NOTE: Door – you control it & don't slam it
NOTE: Emergency Exit procedure (through door). Other exits

BEFORE STARTING ENGINE
[ ]  Tiedowns .... REMOVED
[ ]  Cell Phones .... OFF
[ ]  Hobbs Time .... RECORD
[ ]  Passenger Brief .... COMPLETE
[ ]  Baggage Door .... CLOSED
[ ]  Seats, Seat Belts .... SECURE
[ ]  Parking Brake .... SET
[ ]  Fuel .... LOWER TANK
[ ]  Circuit Breakers .... IN
[ ]  Master .... ON
[ ]  Avionics Master .... OFF
[ ]  Gear Light / Lever .... ON / DOWN
[ ]  Autopilot .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Ram Air .... CLOSED
[ ]  Mixture .... IDLE
[ ]  Prop .... FORWARD
[ ]  Throttle .... 1/4 (Full if flooded)
[ ]  Boost Pump .... OFF
[ ]  Key .... IN SWITCH
PRIME (IF >4 HOURS)
[ ]  Boost Pump .... ON UNTIL 15
[ ]  Mixture .... RICH (5 sec)
[ ]  Mixture .... IDLE
START
[ ]  Prop Area .... CLEAR
[ ]  Mags .... START
[ ]  Mixture .... RICH
[ ]  Throttle .... 1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Fuel Pressure .... CHECK
[ ]  Mixture .... 3/4
[ ]  Avionics .... ON
[ ]  Nav Lights .... AS REQ
[ ]  ATIS/AWOS .... CHECK
[ ]  Altimiter .... SET
[ ]  Heading Indicator .... SET
TAXI
[ ]  ATC .... CLEARANCE
[ ]  Brakes .... TEST
[ ]  Turn Indicator / Ball .... CHECK
[ ]  Attitude Indicator .... CHECK
[ ]  Heading Indicator .... TRACKING
[ ]  Compass .... KNOWN HEADINGS
[ ]  Trim .... TAKEOFF
[ ]  Flaps .... TAKEOFF
[ ]  Autopilot .... OFF & HDG MODE
[ ]  Heading Bug .... TOP OF DG
[ ]  Autpilot .... ON & HDG HOLD ON
[ ]  Rotate Bug to either side
[ ]  Override Autopilot each direction
[ ]  Autopilot .... OFF

RUNUP
[ ]  Parking Brakes .... SET
[ ]  Heading Indicator .... SET
[ ]  Cowl Flaps .... OPEN
[ ]  Controls .... FREE & CORRECT
[ ]  Instruments .... CHECK
[ ]  Fuel .... FULLEST TANK
[ ]  Ram Air .... CLOSED
[ ]  Throttle .... 2000 RPM
[ ]  Mixture .... BEST POWER
[ ]  Prop .... CYCLE (3x)
[ ]  Mags .... (drop < 175, diff < 50)
[ ]  Temps / Alt / Vac / Fuel .... GREEN
[ ]  Fuel Pressure .... GREEN
[ ]  Throttle .... 1000 RPM
HOLD SHORT LINE
[ ]  Flaps .... TAKEOFF
[ ]  Trim .... ON & TAKEOFF
[ ]  Charts / Plates / Log .... READY
[ ]  COM & NAV .... FIRST FREQS
[ ]  OBS, ADF, DME .... SET
[ ]  Headset .... ON
[ ]  Flight Plan .... OPEN?
[ ]  Window & Door .... LATCH
[ ]  Time Off .... LOG
[ ]  ATC .... TOWER
CLEARED TO ACTIVE
[ ]  Boost Pump .... ON
[ ]  Landing Light .... ON
[ ]  Strobes .... ON
[ ]  Transponder .... ALT
[ ]  Pitot Heat .... ON (as req)
>1000' AGL
[ ]  Throttle .... FULL
[ ]  Prop .... 2600
[ ]  Boost Pump .... OFF
[ ]  Temps / Alt / Vac / Fuel .... GREEN
[ ]  Landing Light .... OFF
[ ]  Fuel Caps .... LOOK FOR LEAKS
CRUISE
[ ]  Throttle .... FULL
[ ]  Prop .... 2400
[ ]  Cowl Flaps .... CLOSED
[ ]  Mixture .... LEAN
[ ]  Temps / Alt / Vac / Fuel .... GREEN
[ ]  Heading Indicator .... SET
[ ]  Landing Light .... OFF
[ ]  Fuel Tank .... SWITCH?

DESCENT
[ ]  Fuel .... FULLEST TANK
[ ]  Mixture .... ENRICH
[ ]  Cowl Flaps .... CLOSED
[ ]  Ram Air .... CLOSED
[ ]  Temps / Alt / Vac / Fuel .... GREEN
[ ]  Heading Indicator .... SET
[ ]  Autopilot .... OFF
[ ]  Landing Light .... ON
CLEAR ACTIVE
[ ]  Flaps .... UP
[ ]  Boost Pump .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Transponder .... STANDBY
[ ]  Pitot Heat .... OFF
[ ]  Strobes .... OFF
SHUT DOWN
[ ]  All Switches .... OFF
[ ]  Mixture .... IDLE
[ ]  Mags .... OFF
[ ]  Master .... OFF
[ ]  Overhead Light .... OFF
[ ]  Timer .... STOPPED
[ ]  Headset .... OFF
[ ]  GPS .... OFF
[ ]  Hobbs Time .... RECORD
[ ]  Flight Plan .... CLOSED

PRE-APPROACH
[ ]  ATIS, Approach in use
[ ]  Heading Indicator .... SET
[ ]  Altimiter .... SET
[ ]  Radios .... SET & IDENT
[ ]  DME .... SET
[ ]  Marker Beacons .... TEST & AUDIO ON

APPROACH BRIEFING
[ ]  Airport, Approach & Runway
[ ]  IAF & Procedure Turn
[ ]  FAF & Final Approach Course
[ ]  Minimums .... MDA/DA & VIS
[ ]  Circling .... ALTITUDE & NOTES
[ ]  TDZE
[ ]  MAP .... How to ID?
[ ]  Missed Approach Proc .... INITIAL

IFR REQUIRED REPORTS
[ ]  Vacating assigned altitude
[ ]  Altitude change when VFR on TOP
[ ]  Unable to climb / desc 500 FPM
[ ]  Change in TAS 5% or 10 knots
[ ]  Missed Approach
[ ]  Arrival at Clearance Limit
[ ]  Arrival / leaving Holding Fix
[ ]  Loss of any Nav or Com
[ ]  Safety, including hazardous WX
WHEN NOT IN RADAR CONTACT
[ ]  Compulsory points or fixes in clearance
[ ]  FAF inbound
[ ]  ETA change greater than 3 minutes

ICING CONDITIONS  [EMERGENCY]
[ ]  Ram Air .... OFF
[ ]  Cabin Heat .... OFF
NOTE: Leave off if engine is running rough
[ ]  Pitot Heat .... ON
[ ]  Static Air .... ALTERNATE
[ ]  Change .... HDG and/or ALTITUDE

ENGINE FAILURE or ROUGH  [EMERGENCY]
[ ]  Airspeed .... 105 MPH
[ ]  Landing Field .... SELECT
[ ]  Mixture .... CHECK
[ ]  Throttle .... ADJUST
[ ]  Boost Pump .... ON
NOTE: If no restart, then turn Boost OFF
[ ]  Fuel .... OTHER TANK
[ ]  Mags .... BOTH

AIR START PROCEDURE  [EMERGENCY]
[ ]  Propeller .... FORWARD
[ ]  Mixture .... IDLE
[ ]  Fuel Pressure .... CHECK
NOTE: Boost ON if no pressure
[ ]  Throttle .... 25% FORWARD
[ ]  Mags .... BOTH
[ ]  Mixture .... SLOWLY TO FULL RICH

NO START  [EMERGENCY]
[ ]  ELT .... ARM
[ ]  Transponder .... 7700
[ ]  Radio .... 121.5
[ ]  Seat Belts .... SECURE
[ ]  Mixture .... IDLE
[ ]  Fuel .... OFF
[ ]  Mags .... OFF
[ ]  Flaps .... AS REQ
[ ]  Gear .... UP or DOWN
[ ]  Door .... AJAR
[ ]  Master .... OFF (prior to landing)

ALTERNATOR  [EMERGENCY]
STEADY ALTERNATOR WARNING LIGHT
NOTE: Indicates high voltage due to voltage regulator exceeding limits
[ ]  Avionics Master .... OFF
[ ]  Master .... OFF, then ON
[ ]  Light on again? .... Alt Field Brkr OFF
[ ]  All non-essential electrical .... OFF
[ ]  Land .... ASAP
BLINKING ALTERNATOR WARNING LIGHT
NOTE: Indicates low voltage due to alternator malfunction, belt or breaker
[ ]  ALT FIELD BREAKER .... RESET
[ ]  Light on again?
[ ]  All non-essential electrical .... OFF
[ ]  Land .... ASAP

ENGINE FIRE – IN FLIGHT  [EMERGENCY]
[ ]  Fuel .... OFF
[ ]  Throttle .... CLOSED
[ ]  Mixture .... IDLE
[ ]  Cabin Vent & Heat .... CLOSED (fwd)
[ ]  Landing Gear .... DOWN or UP
[ ]  Wing Flaps .... EXTEND

ENGINE FIRE – GROUND  [EMERGENCY]
[ ]  Mixture .... IDLE
[ ]  Fuel .... OFF
[ ]  Master .... OFF

ELECTRICAL FIRE  [EMERGENCY]
[ ]  Master Switch .... OFF
[ ]  Cabin Vent .... OPEN
[ ]  Circuit Breakers .... CHECK

GEAR RETRACTION FAIL  [EMERGENCY]
NOTE: Airspeed or squat switch failed. 3 lights on: GR SAFETY BYPASS switch, GEAR DN, IN TRANSIT. Gear horn will sound.
[ ]  Gear Bypass Btn .... HOLD
NOTE: Hold until gear retracted
[ ]  Gear horn on? .... THEN
[ ]  GEAR CONT Breaker .... OFF
NOTE: Push GEAR CONT breaker back in to extend gear.

MANUAL GEAR EXTENSION  [EMERGENCY]
[ ]  Airspeed .... 125 MPH
[ ]  Gear Circuit Breaker .... OFF
[ ]  Gear Lever .... DOWN
[ ]  Handcrank Lever .... FORWARD
[ ]  Gear Crank .... CLOCKWISE
NOTE: Crank until light / floor indicator
WARNING: Do not retract gear manually

IFR LOST COMMS  [EMERGENCY]
[ ]  Squawk .... 7600
[ ]  VFR? .... Land ASAP
ROUTE
[ ]  Last assigned by ATC
[ ]  Route ATC advised to expect
ALTITUDE – HIGHEST OF
[ ]  Last assigned by ATC
[ ]  Minimum IFR altitude
[ ]  Expected altitude in clearance
LEAVE CLEARANCE LIMIT (IAF)
[ ]  At EFC time
[ ]  If no EFC given, at ETA time
LEAVE CLEARANCE LIMIT (NOT IAF)
[ ]  At EFC time
[ ]  If no EFC given proceed to IAF and begin approach at ETA time

LIGHT GUN SIGNALS
NOTE: Color Green: Ground Takeoff / Flight Land
NOTE: Flashing Green: Ground Taxi / Flight Return to land
NOTE: Red: Ground Stop / Flight Yield and circle
NOTE: Flashing Red: Ground Taxi clear of runway / Flight Airport Unsafe
NOTE: Flashing White: Ground Return to start pt. / Flight N/A
NOTE: Red / Green: Exercise extreme caution
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