Piper PA-28-140 — Cherokee140BChecklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

PREFLIGHT
CABIN
[ ]  Papers .... A.R.O.W.
[ ]  Parking Brake .... SET
[ ]  Seat Belt Securing Control Wheel .... REMOVE
[ ]  Mags .... OFF
[ ]  Avionics .... OFF
[ ]  Circuit Breakers .... IN
[ ]  Trim .... TAKEOFF
[ ]  Prop .... CLEAR
[ ]  Master .... ON
[ ]  Fuel Gauges .... TRUE
[ ]  Flaps .... EXTEND
[ ]  Lights .... INTERIOR / EXTERIOR
[ ]  Stall Indicator .... TEST
[ ]  Master .... OFF
[ ]  Fuel Selector .... CHECK EACH POSITION, SET TO EMPTIEST TANK
RIGHT WING
[ ]  Flap .... CHECK
[ ]  Aileron .... CHECK
[ ]  Navigation Light .... CHECK
[ ]  Tiedown .... DISCONNECT
[ ]  Fuel Vent .... CHECK
[ ]  Fuel Quantity .... CHECK VISUALLY
[ ]  Fuel Filler Cap .... SECURE
[ ]  Right Fuel Tank Sump .... DRAIN
[ ]  Chock .... REMOVE
[ ]  Tire .... CHECK (24 PSI)
[ ]  Brake Assembly .... CHECK
[ ]  Main Strut .... APPROX. 4.5" EXTENSION
NOSE
[ ]  Right Engine Compartment .... CHECK
[ ]  Oil Level .... 7 QTS (under 3 HR flight), 8 QTS (extended flight)
[ ]  Oil Cap .... SECURE
[ ]  Right Engine Cowling .... SECURE
[ ]  Exhaust System .... CHECK
[ ]  Chock .... REMOVE
[ ]  Nose Strut .... APPROX. 3.25" EXTENSION
[ ]  Nose Tire .... CHECK (24 PSI)
[ ]  Landing Light .... CHECK
[ ]  Engine Air Inlets .... CLEAR
[ ]  Alternator Belt Tension .... CHECK
[ ]  Prop/Spinner .... CHECK
[ ]  Left Engine Compartment .... CHECK
[ ]  Left Engine Cowling .... SECURE
[ ]  Fuel Strainer .... DRAIN
[ ]  Windshield .... CHECK
LEFT WING
[ ]  Chock .... REMOVE
[ ]  Tire .... CHECK (24 PSI)
[ ]  Brake Assembly .... CHECK
[ ]  Main Strut .... APPROX. 4.5" EXTENSION
[ ]  Left Fuel Tank Sump .... DRAIN
[ ]  Fuel Vent .... CHECK
[ ]  Tiedown .... DISCONNECT
[ ]  Pitot/Static Tube .... CLEAR
[ ]  Fuel Quantity .... CHECK VISUALLY
[ ]  Fuel Filler Cap .... SECURE
[ ]  Navigation Light .... CHECK
[ ]  Aileron .... CHECK
[ ]  Flap .... CHECK
EMPENNAGE
[ ]  Left Stabilator .... CHECK
[ ]  Tiedown .... DISCONNECT
[ ]  Trim Tab .... CHECK
[ ]  Rudder .... CHECK
[ ]  Navigation Light .... SECURE
[ ]  Right Stabilator .... CHECK
[ ]  Antennas .... CHECK

START
[ ]  Hobbs/Tach Time .... RECORDED
[ ]  Passenger Brief .... COMPLETE
[ ]  Seat Track/Back .... LOCK
[ ]  Seat Belt /Harness .... FASTEN
[ ]  Brakes .... SET
[ ]  Beacon .... ON
[ ]  Navigation Lights .... AS REQUIRED
[ ]  Mixture .... RICH
[ ]  Throttle .... OPEN 1/4"
[ ]  Carb Heat .... OFF
[ ]  Prime .... AS REQUIRED
[ ]  Prop .... CLEAR
[ ]  Master .... ON
[ ]  Fuel Pump .... ON
[ ]  Mags .... START
[ ]  Throttle .... 1,000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Fuel Pump .... OFF
[ ]  Mixture .... LEAN

PRE-TAXI
[ ]  Flaps .... UP
[ ]  Cabin Heat & Air .... AS DESIRED
[ ]  Avionics .... ON / SET
[ ]  Transponder .... CODE / STANDBY
[ ]  Clock .... SET
[ ]  Airspeed Indicator .... CHECK
[ ]  Attitude Indicator .... SET
[ ]  Heading Indicator .... SET
[ ]  VSI .... CHECK
[ ]  ATIS/AWOS .... COPY
[ ]  Altimeter .... SET / CHECK
[ ]  Landing Light .... AS REQUIRED
[ ]  Fuel Selector .... SWITCH TO FULLEST TANK

TAXI
[ ]  Brakes .... TEST
[ ]  Attitude Indicator .... CHECK
[ ]  Turn-and-Bank Indicator .... CHECK
[ ]  Heading Indicator .... CHECK
[ ]  Magnetic Compass .... CHECK

RUN-UP
[ ]  Brakes .... SET
[ ]  Mixture .... BEST POWER
[ ]  Primer .... IN & LOCKED
[ ]  Throttle .... 1,800 RPM
[ ]  Mags (R & L) .... CHECK (175 RPM max drop, 50 RPM max differential)
[ ]  Carb Heat .... TEST
[ ]  Vacuum .... CHECK
[ ]  Ammeter .... CHECK
[ ]  Oil Pressure .... CHECK
[ ]  Oil Temperature .... CHECK
[ ]  Throttle .... 1,000 RPM

TAKEOFF
[ ]  Heading Indicator .... SET
[ ]  Avionics .... SET
[ ]  Engine Gauges .... CHECK
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Selector .... FULLEST TANK
[ ]  Fuel Pump .... ON
[ ]  Carb Heat .... OFF
[ ]  Mixture .... BEST POWER
[ ]  Trim .... TAKEOFF
[ ]  Flaps .... SET (0-25°)
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Door .... LATCHED
CLEARED FOR TAKEOFF
[ ]  Landing Light .... ON
[ ]  Transponder .... ALTITUDE
[ ]  Throttle .... FULL

AFTER TAKEOFF
[ ]  Flaps .... UP
[ ]  Fuel Pump .... OFF
[ ]  Engine Gauges .... CHECK
[ ]  Landing Light .... AS DESIRED

CRUISE
[ ]  Landing Light .... OFF
[ ]  Throttle .... SET
[ ]  Mixture .... LEAN
[ ]  Engine Gauges .... CHECK
[ ]  Heading Indicator .... SET
[ ]  Fuel Selector .... AS REQUIRED

APPROACH
[ ]  Mixture .... RICHEN AS REQUIRED
[ ]  Fuel Selector .... PROPER TANK
[ ]  Carb Heat .... AS REQUIRED
[ ]  ATIS/AWOS .... COPY
[ ]  Altimeter .... SET
[ ]  Avionics .... SET
[ ]  Heading Indicator .... SET
[ ]  Engine Gauges .... CHECK
[ ]  Brakes .... PEDAL TEST
[ ]  Seatbelt/Harness .... FASTENED
[ ]  Landing Light .... ON

LANDING
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector .... PROPER TANK
[ ]  Carb Heat .... AS REQUIRED
[ ]  Mixture .... BEST POWER
[ ]  Flaps .... AS DESIRED

AFTER LANDING
[ ]  Carb Heat .... OFF
[ ]  Mixture .... LEAN
[ ]  Flaps .... UP
[ ]  Fuel Pump .... OFF
[ ]  Landing Light .... OFF
[ ]  Transponder .... STANDBY

SHUTDOWN
[ ]  Avionics .... OFF
[ ]  Throttle .... 1,000 RPM
[ ]  Mags .... GROUNDING CHECK
[ ]  Mixture .... FULL LEAN
[ ]  Prop .... CHECK STOPPED
[ ]  Mags .... OFF
[ ]  Master .... OFF
[ ]  Lights .... OFF

SECURING
[ ]  Hobbs/Tach Time .... RECORDED
[ ]  Seat Belt Securing Control Wheel .... INSTALL
[ ]  Chocks .... INSTALL
[ ]  Tiedowns .... SECURE
[ ]  Door/Window .... CLOSED

FLOODED ENGINE  [ABNORMAL]
FLOODED ENGINE
[ ]  Mixture .... FULL LEAN
[ ]  Throttle .... FULL OPEN
[ ]  Mags .... START
WHEN ENGINE FIRES:
[ ]  Mixture .... RICH
[ ]  Throttle .... 1,000 RPM

GROUND BURNOUT  [ABNORMAL]
GROUND BURNOUT
[ ]  Mixture .... RICH
[ ]  Throttle .... 2,000 RPM
[ ]  Mixture .... LEAN TO 50 RPM DROP BELOW BEST POWER
AFTER 1 MINUTE:
[ ]  Mixture .... RICH
[ ]  Mags .... RECHECK

RADIO FAILURE  [ABNORMAL]
RADIO FAILURE
[ ]  Volume .... CHECK
[ ]  Headset Connection .... CHECK
[ ]  Audio Controls .... CHECK
[ ]  Circuit Breakers .... CHECK
[ ]  Speaker .... ON
[ ]  Hand-Held Microphone .... CHECK
[ ]  Frequency .... SWITCH
IF IFR (OR VFR IN CLASS B, C, D AIRSPACE):
[ ]  Transponder .... 7600
NOTE: If failure occurs in VFR conditions, or VFR conditions are encountered after failure, continue flight under VFR and land as soon as practicable.
VFR LANDING AT A CONTROLLED FIELD:
[ ]  Remain outside or above Class D airspace until traffic flow determined. .... CHECK
[ ]  Transmit intentions "in the blind" advising tower of aircraft type, position, altitude, and intention to land. .... CHECK
[ ]  Enter pattern, report position "in the blind", and watch for light signals from tower. .... CHECK
NOTE: If failure occurs in IFR conditions, continue flight according to the following:
ROUTE TO FLY (IN ORDER): (AVE. F)
[ ]  A – Assigned .... CHECK
[ ]  V – Vectored .... CHECK
[ ]  E – Expected .... CHECK
[ ]  F – Filed .... CHECK
ALTITUDE (HIGHEST OF FOR THE ROUTE SEGMENT BEING FLOWN): (MEA)
[ ]  M – Minimum IFR Altitude .... CHECK
[ ]  E – Expected as Advised by ATC .... CHECK
[ ]  A – Assigned by ATC .... CHECK
DESCENT FOR APPROACH:
NOTE: From enroute altitude upon reaching the IAF but not before:
[ ]  Expect-further-clearance time (if given) .... CHECK
[ ]  ETA as calculated from filed ETE .... CHECK
ATC LIGHT SIGNALS
[ ]  Steady Green - On Deck .... Cleared for Takeoff
[ ]  Steady Green - Airborne .... Cleared to Land
[ ]  Flashing Green - On Deck .... Cleared for Taxi
[ ]  Flashing Green - Airborne .... Return for Landing (to be followed by steady green)
[ ]  Steady Red - On Deck .... STOP
[ ]  Steady Red - Airborne .... Give way to other aircraft and continue circling
[ ]  Flashing Red - On Deck .... Taxi clear of runway in use
[ ]  Flashing Red - Airborne .... Airport Unsafe – DO NOT LAND
[ ]  Flashing White - On Deck .... Return to starting point on airport
[ ]  Flashing White - Airborne .... Not Applicable
[ ]  Alternating Red and Green - On Deck .... Exercise extreme caution
[ ]  Alternating Red and Green - Airborne .... Exercise extreme caution
NOTE: Acknowledge all light signals by flashing landing light and/or rocking wings.

ABORT  [EMERGENCY]
ABORT
[ ]  Throttle .... IDLE
[ ]  Brakes .... AS REQUIRED

ENGINE FAILURE IMMEDIATELY AFTER TAKEOFF  [EMERGENCY]
ENGINE FAILURE IMMEDIATELY AFTER TAKEOFF
[ ]  Airspeed .... 83 MPH (flaps UP)
[ ]  Mixture .... FULL LEAN
[ ]  Fuel Selector .... OFF
[ ]  Flaps .... DOWN (70 MPH glide)
[ ]  Master & Mags .... OFF

COMPLETE ENGINE FAILURE DURING FLIGHT  [EMERGENCY]
COMPLETE ENGINE FAILURE DURING FLIGHT
[ ]  Airspeed .... 83 MPH (flaps UP)   (Glide Ratio = 1.9 SM/1,000’ AGL)
IF AIRSTART WARRANTED:
[ ]  Carb Heat .... ON
[ ]  Mixture .... RICH
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector .... CHECK / SWITCH
[ ]  Primer .... IN & LOCKED
[ ]  Mags .... CHECK ALL
[ ]  Master .... ON

FORCED LANDING  [EMERGENCY]
FORCED LANDING
[ ]  Airspeed .... 83 MPH (flaps UP)
[ ]  Squawk .... 7700
[ ]  Emergency .... DECLARE
[ ]  ELT .... ON
[ ]  Mixture .... FULL LEAN
[ ]  Fuel Selector .... OFF
[ ]  Seatbelt/Harness .... FASTENED
[ ]  Flaps .... AS REQUIRED (70 MPH with flaps full)
[ ]  Master & Mags .... OFF
[ ]  Door .... UNLATCH

ENGINE ROUGHNESS  [EMERGENCY]
ENGINE ROUGHNESS
[ ]  Carb Heat .... ON
IF ROUGHNESS CONTINUES PAST 1 MIN:
[ ]  Carb Heat .... OFF
[ ]  Mixture .... ADJUST FOR MAX SMOOTHNESS
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector .... SWITCH
[ ]  Primer .... IN & LOCKED
[ ]  Engine Gauges .... CHECK
[ ]  Mags .... L then R then BOTH
[ ]  Mags .... SMOOTHEST SETTING
[ ]  Power .... REDUCE
[ ]  Mixture .... FULL RICH
[ ]  LAND AT NEAREST AIRPORT .... EXECUTE

HIGH OIL TEMPERATURE  [EMERGENCY]
HIGH OIL TEMPERATURE
[ ]  Power .... REDUCE
[ ]  Mixture .... RICH
[ ]  Airspeed .... INCREASE
IF HIGH TEMP PERSISTS:
[ ]  LAND AT NEAREST AIRPORT .... EXECUTE

LOSS OF OIL PRESSURE  [EMERGENCY]
LOSS OF OIL PRESSURE
[ ]  Oil Temp .... CHECK
[ ]  Power .... REDUCE
IF OIL TEMP SHOWS RISE, ENGINE FAILURE IMMINENT:
[ ]  Forced Landing .... EXECUTE
IF OIL TEMP DOES NOT SHOW RISE:
[ ]  LAND AT NEAREST AIRPORT .... EXECUTE

LOSS OF FUEL PRESSURE  [EMERGENCY]
LOSS OF FUEL PRESSURE
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector .... SWITCH

ENGINE FIRE ON GROUND  [EMERGENCY]
ENGINE FIRE ON GROUND
[ ]  Starter .... CRANK
[ ]  Mixture .... FULL LEAN
[ ]  Throttle .... OPEN
[ ]  Fuel Pump .... OFF
[ ]  Fuel Selector .... OFF

ENGINE FIRE IN FLIGHT  [EMERGENCY]
ENGINE FIRE IN FLIGHT
[ ]  Mixture .... FULL LEAN
[ ]  Fuel Selector .... OFF
[ ]  Fuel Pump .... OFF
[ ]  Master & Mags .... OFF
[ ]  Heat & Defrost .... OFF
[ ]  Airspeed .... 105 MPH
[ ]  Forced Landing .... EXECUTE

ELECTRICAL FIRE  [EMERGENCY]
ELECTRICAL FIRE
[ ]  Master .... OFF

WING FIRE  [EMERGENCY]
WING FIRE
[ ]  Navigation Lights .... OFF
[ ]  Sideslip .... AS REQUIRED
[ ]  Forced Landing .... EXECUTE

SMOKE AND FUMES IN COCKPIT  [EMERGENCY]
SMOKE AND FUMES IN COCKPIT
[ ]  Vents .... OPEN
[ ]  Heater .... OFF

HIGH AMMETER READING  [EMERGENCY]
HIGH AMMETER READING
[ ]  Master .... OFF

ZERO AMMETER READING  [EMERGENCY]
ZERO AMMETER READING
[ ]  Electrical Load .... REDUCE
[ ]  Alternator Circuit Breakers .... CHECK / RESET
[ ]  Alternator Switch .... OFF (1 min) then ON
IF AMMETER READING STILL ZERO:
[ ]  Land as soon as practicable .... EXECUTE

VACUUM SYSTEM FAILURE  [EMERGENCY]
VACUUM SYSTEM FAILURE
IF VMC:
[ ]  Attitude Indicator & Heading Indicator .... COVER
[ ]  Maintain VMC .... EXECUTE
IF IMC:
[ ]  Attitude Indicator & Heading Indicator .... COVER
[ ]  Fly using Turn-and-Bank, Altimeter, and Airspeed Indicator .... EXECUTE
[ ]  Declare EMERGENCY .... EXECUTE

INOPERATIVE TRIM  [EMERGENCY]
INOPERATIVE TRIM
[ ]  Flaps .... AS REQUIRED
[ ]  Power .... AS REQUIRED

FLAP MALFUNCTION  [EMERGENCY]
FLAP MALFUNCTION
[ ]  Flaps .... LEAVE WHERE SET

STRUCTURAL ICING  [EMERGENCY]
STRUCTURAL ICING
[ ]  Carb Heat .... ON
[ ]  Throttle .... MAX RPM
[ ]  Mixture .... BEST POWER
[ ]  Heat & Defrost .... MAX
[ ]  EXIT ICING CONDITIONS .... EXECUTE
IF LANDING WITH STRUCTURAL ICING:
[ ]  Flaps .... LEAVE UP

DOOR OPENING IN FLIGHT  [EMERGENCY]
DOOR OPENING IN FLIGHT
[ ]  FLY THE AIRPLANE [MEMORY] .... EXECUTE
[ ]  Airspeed .... 89 KIAS
[ ]  Vents .... CLOSE
[ ]  Storm Window .... OPEN
IF ONLY UPPER LATCH OPEN:
[ ]  Upper Latch .... LATCH
IF ONLY SIDE LATCH IS OPEN:
[ ]  Arm Rest .... PULL WHILE LATCHING
IF BOTH LATCHES ARE OPEN:
[ ]  Side Latch .... LATCH
[ ]  Top Latch .... LATCH

LANDING WITH A FLAT MAIN TIRE  [EMERGENCY]
LANDING WITH A FLAT MAIN TIRE
[ ]  Approach .... NORMAL
[ ]  Flaps .... 40°
[ ]  Touchdown .... GOOD TIRE FIRST
[ ]  Hold airplane off flat tire as long as possible .... EXECUTE
[ ]  Maintain directional control using good-tire brake .... EXECUTE

LANDING WITH A FLAT NOSE TIRE  [EMERGENCY]
LANDING WITH A FLAT NOSE TIRE
[ ]  Approach .... NORMAL
[ ]  Flaps .... AS REQUIRED
[ ]  Touchdown .... ON MAINS
[ ]  Hold nosewheel off ground as long as possible .... EXECUTE
WHEN NOSEWHEEL TOUCHES DOWN:
[ ]  FULL UP ELEVATOR .... EXECUTE

SPIN RECOVERY  [EMERGENCY]
SPIN RECOVERY
NOTE: Memory Aid: PARE
[ ]  Power [MEMORY] .... Idle
NOTE: (Power)
[ ]  Ailerons [MEMORY] .... Neutral
NOTE: (Ailerons)
[ ]  Rudder [MEMORY] .... Full opposite rotation direction
NOTE: (Rudder)
[ ]  Yoke [MEMORY] .... Full forward with neutral ailerons
NOTE: (Elevator)
[ ]  Rudder .... Neutral when rotation stops
[ ]  Yoke .... Pull smoothly from dive
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