Piper PA-28-140 — Jacob_Esparza_N6693W_Operating_Checklist_PA_28
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Albuquerque Sunport Frequencies" item count differs between passes (5 vs 3); verify nothing was dropped.

Preflight Inspection
INTERIOR
[ ]  Control Lock .... REMOVE
[ ]  A.R.R.O.W Documents .... ON BOARD
[ ]  Maintenance Records .... CHECK
[ ]  Magnetos .... OFF
[ ]  Mixture .... LEAN
[ ]  Avionics .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Master Switch .... ON
[ ]  Beacon .... ON
[ ]  Nav. Lights .... ON
[ ]  Landing Lights .... ON
[ ]  Fuel Gauges .... CHECK
EXTERIOR
[ ]  Go Outside
[ ]  Beacon .... CHECK
[ ]  Nav Light (Right) .... CHECK
[ ]  Landing Light .... CHECK
[ ]  Pitot Cover .... REMOVE
[ ]  Nav Light (Left) .... CHECK
[ ]  Come Back Inside
[ ]  Beacon .... OFF
[ ]  Nav Lights .... OFF
[ ]  Landing Light .... OFF
[ ]  Master Switch .... OFF
[ ]  Flaps .... DOWN
RIGHT WING
[ ]  Flap .... CHECK
[ ]  Aileron .... CHECK
[ ]  Wing Tip .... CHECK
[ ]  Leading Edge .... CHECK
[ ]  Tie Down .... REMOVE
[ ]  Fuel Sample .... AQUIRE
[ ]  Fuel Level .... VISUALLY CHECK
[ ]  Fuel Vent .... CHECK
[ ]  Right Main Gear .... CHECK
NOSE
[ ]  Windshield .... CLEAN
[ ]  Oil Level .... CHECK
[ ]  Belt .... CHECK
[ ]  Exhaust .... CHECK
[ ]  Right Cowling .... SECURE
[ ]  Spinner .... CHECK
[ ]  Propeller .... CHECK
[ ]  Air Intake .... CHECK
[ ]  Brake Fluid .... CHECK
[ ]  Left Cowling .... SECURE
[ ]  Nose Gear .... CHECK
[ ]  Chocks .... REMOVE
LEFT WING
[ ]  Left Main Gear .... CHECK
[ ]  Fuel Sample .... AQUIRE
[ ]  Fuel Vent .... CHECK
[ ]  Fuel Level .... VISUALLY CHECK
[ ]  Leading Edge .... CHECK
[ ]  Pitot Tube .... CHECK
[ ]  Tie Downs .... REMOVED
[ ]  Wing Tip .... CHECK
[ ]  Aileron .... CHECK
[ ]  Flap .... CHECK
[ ]  Left Fuselage .... CHECK
[ ]  Nav/Comm Antennas .... SECURE
EMPENNAGE
[ ]  Stabilizer .... CHECK
[ ]  Trim Tab .... CHECK
[ ]  Rudder .... CHECK
[ ]  Tie Down .... REMOVED
[ ]  Right Fuselage .... CHECK

Before Engine Start
[ ]  Preflight Inspection .... COMPLETE
[ ]  Passenger Briefing .... COMPLETE
[ ]  Seats .... ADJUST AND LOCK
[ ]  Electrical Equipment .... OFF
[ ]  Circuit Breakers .... CHECK IN
[ ]  Fuel Selector Valve .... FULLEST TANK
[ ]  Parking Brake .... SET

Engine Start
[ ]  Mixture .... FULL RICH
[ ]  Throttle .... OPEN ¼”
[ ]  Carburetor Heat .... OFF (Pushed In)
[ ]  Primer .... CYCLE 3-4 TIMES
[ ]  Primer .... LOCKED
[ ]  Master Switch .... ON
[ ]  Fuel Pump .... ON
[ ]  Verify fuel pressure then turn off fuel pump
[ ]  Anti Collision Light .... ON
[ ]  Key .... VERIFY START POSITION
[ ]  Propeller Area .... CLEAR
[ ]  Brakes .... HOLD
[ ]  Starter .... ENGAGE
[ ]  Throttle .... 800 R.P.M
[ ]  Oil Pressure .... CHECK
[ ]  Fuel Pressure .... CHECK
[ ]  Ammeter .... CHECK

After Engine Start
[ ]  Avionics .... ON
[ ]  Flaps .... CHECK TRAVEL (Down then Up)
[ ]  Weather (ATIS, AWOS, ASOS) .... CHECK
[ ]  Flight Instruments .... CHECK & SET
[ ]  ATC Clearance (If Required) .... REQUEST
[ ]  Transponder .... SET CODE, VERIFY STBY
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Brakes .... RELEASE & CHECK
[ ]  Lights .... AS REQUIRED

Run Up
[ ]  Cabin Door .... CLOSED & LATCHED
[ ]  Seats and Belts .... SECURE
[ ]  Elevator Trim .... SET FOR TAKEOFF
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector Valve .... FULLEST TANK
[ ]  Mixture .... FULL RICH
[ ]  Parking Brake/Brakes .... SET & HOLD
[ ]  Throttle .... 1800 R.P.M
[ ]  Magnetos .... CHECK
NOTE: Max drop 175 R.P.M, max difference 50 R.P.M
[ ]  Carburetor Heat .... ON
NOTE: Check for R.P.M drop of about 100 R.P.M and stays there
[ ]  Carburetor Heat .... OFF
NOTE: Verify R.P.M returns to 1800 R.P.M
[ ]  Mixture .... SET FOR TAKEOFF

Run Up (Cont’d)
[ ]  Fuel Pressure .... CHECK
[ ]  Oil Pressure .... CHECK
[ ]  Oil Temperature .... CHECK
[ ]  Ammeter .... CHECK
[ ]  Suction/Vacuum .... 4-5”Hg
[ ]  Throttle .... 1000 R.P.M
[ ]  Flight Instruments .... CHECK & SET
[ ]  Avionics .... SET

Before Takeoff
[ ]  Fuel Pump .... VERIFY ON
[ ]  Fuel Selector Valve .... VERIFY FULLEST TANK
[ ]  Nav. Lights .... AS REQUIRED
[ ]  Landing Light .... ON
[ ]  Beacon .... ON
[ ]  Window .... CLOSED
[ ]  Flaps .... AS DESIRED
[ ]  Takeoff Clearance (if required) .... REQUEST
[ ]  Transponder .... SET ALT
[ ]  Parking Brake/Brakes .... RELEASE

Albuquerque Sunport Frequencies
[ ]  ATIS .... 118.00
[ ]  Tower .... 120.30
[ ]  Clearance .... 119.20
[ ]  Departure .... 123.90 or 127.40
[ ]  Ground .... 121.90

Normal Takeoff
[ ]  Throttle .... SMOOTHLY ADVANCE TO FULL POWER
[ ]  Airspeed Indicator .... ALIVE & WELL
[ ]  Engine Instruments .... MONITOR
[ ]  Elevator Control .... ROTATE AT Vr (55 KTS)
[ ]  Normal Climb Speed .... 80 KTS
[ ]  Best Angle Vx .... 65 KTS
[ ]  Best Rate of Climb Vy .... 75 KTS
[ ]  Flaps .... RETRACT

Short Field Takeoff
[ ]  Flaps .... 25° (2nd Notch)
[ ]  Brakes .... HOLD
[ ]  Throttle .... SMOOTHLY ADVANCE TO FULL POWER
[ ]  Brakes .... RELEASE
[ ]  Airspeed Indicator .... ALIVE & WELL
[ ]  Engine Instruments .... MONITOR
[ ]  Elevator Control .... ROTATE AT Vr (55 KTS)
[ ]  Vx Climb Speed .... 65 KTS
[ ]  Flaps .... RETRACT (after obstacle clearance)

Flap Settings
[ ]  1st Notch .... 10°
[ ]  2nd Notch .... 25°
[ ]  3rd Notch .... 40°

Cruise
[ ]  Fuel Selector Valve .... FULLEST TANK
NOTE: Verify fuel pump is on before switching
[ ]  Fuel Pump .... OFF
[ ]  Lights .... AS REQUIRED
[ ]  Power .... AS NEEDED
[ ]  Mixture .... SET
[ ]  Trim .... ADJUST
[ ]  Carburetor Heat .... WHEN REQUIRED

Maneuvers
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector Valve .... FULLEST TANK
[ ]  Lights .... ON
[ ]  Mixture .... FULL RICH
[ ]  Clearing Turns .... COMPLETE
[ ]  Seat Belts .... SECURE

Before Landing
[ ]  Seats and Belts .... SECURE
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector Valve .... FULLEST TANK
[ ]  Landing Light and Beacon .... ON
[ ]  Nav. Lights .... AS REQUIRED
[ ]  Mixture .... FULL RICH
[ ]  Carburetor Heat .... WHEN REQUIRED

Normal Landing
[ ]  Flaps .... 20° (extend below 100 KTS)
[ ]  Approach Speed .... 75 KTS
[ ]  Engine Instruments .... MONITOR
[ ]  Landing Clearance (if required) .... OBTAIN

Go Around/Missed Approach
[ ]  Throttle .... FULL POWER
[ ]  Carburetor Heat .... OFF (pushed in)
[ ]  Mixture .... VERIFY RICH
[ ]  Airspeed .... MAINTAIN 80 KTS
[ ]  Flaps .... RETRACT (after positive rate of climb)
[ ]  Engine Instruments .... MONITOR

After Landing/Clear of Runway
[ ]  Contact Ground .... IF REQUIRED
[ ]  Flaps .... RETRACT
[ ]  Fuel Pump .... OFF
[ ]  Transponder .... VFR STANDBY
[ ]  Lights .... AS REQUIRED
[ ]  Carburetor Heat .... OFF
[ ]  Mixture .... FULL RICH

Shutdown
[ ]  Electrical Equipment (except anti collision light) .... OFF
[ ]  Carburetor Heat .... OFF
[ ]  Throttle .... IDLE
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Key .... REMOVE
[ ]  Avionics .... OFF
[ ]  Anti Collision Light .... OFF
[ ]  Master Switch .... OFF
[ ]  Parking Brake .... SET
[ ]  Vents .... CLOSED
[ ]  Sunshade .... INSTALL
[ ]  Trash .... REMOVED
[ ]  Yoke .... SECURE w/SEAT BELT
[ ]  Tie Downs .... SECURE
[ ]  Pitot Cover .... SECURE
[ ]  Door .... LOCKED
[ ]  Flight Plan .... CLOSED
[ ]  Discrepancies .... LOG & REPORT

Engine Failure During Takeoff Roll  [EMERGENCY]
[ ]  Throttle .... FULL IDLE
NOTE: Try to clear runway before applying full brakes
[ ]  Brakes .... APPLY FULL PRESSURE
[ ]  Flaps .... RETRACT
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Fuel Pump .... OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF

Engine Failure During Takeoff Climb  [EMERGENCY]
[ ]  Airspeed .... 70 KTS
[ ]  Best Place to Land .... AQUIRE
[ ]  Fuel Tanks .... SWITCH TANKS
[ ]  Mixture .... FULL RICH
[ ]  Carburetor Heat .... ON (if engine not yet started)
[ ]  Primer .... IN & LOCKED
IF ENGINE FAILS TO RESTART
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Flaps .... AS REQUIRED
NOTE: Prepare for an emergency landing!!

In-Flight Engine Failure  [EMERGENCY]
[ ]  Airspeed .... 70 KTS
[ ]  Best Place to Land .... AQUIRE
[ ]  Fuel Pump .... ON
[ ]  Fuel Tanks .... SWITCH TANKS
[ ]  Mixture .... FULL RICH
[ ]  Carburetor Heat .... ON (if engine not yet restarted)
[ ]  Magnetos .... BOTH
[ ]  Master Switch .... ON
[ ]  Primer .... IN & LOCKED
IF ENGINE FAILS TO RESTART
[ ]  Radios .... SET to 121.5 or Remain on ATC Freq.
[ ]  Transponder .... SET TO 7700
[ ]  Radios .... DECLARE AN EMERGENCY
NOTE: Using MAYDAY! MAYDAY! MAYDAY!
NOTE: Announce tail # - type of emergency position, color of aircraft & number of persons on board
NOTE: EXECUTE AN EMERGENCY LANDING!!

Transponder Codes
[ ]  7700 .... EMERGENCY
[ ]  7600 .... RADIO FAILURE
[ ]  7500 .... HI-JACKING

Emergency Landing  [EMERGENCY]
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Fuel Pump .... OFF
[ ]  Throttle .... IDLE
[ ]  Electrical Equipment .... OFF
[ ]  Cabin Door .... UNLATCH PRIOR TO TOUCHDOWN
[ ]  Flaps .... AS REQUIRED
[ ]  Seats and Belts .... SECURE
NOTE: Without Stalling the Airplane, Touchdown at Slowest Possible Airspeed!!

Emergency Decent  [EMERGENCY]
[ ]  Throttle .... IDLE
[ ]  Carburetor Heat .... ON
[ ]  Bank .... 45 DEGREES
[ ]  Flaps .... FULL
[ ]  Airspeed .... 95 KTS
[ ]  Fuel Pump .... ON

Engine Fire  [EMERGENCY]
[ ]  Airspeed .... 105 KTS
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Cabin Heat/Air .... CLOSE
[ ]  Master Switch .... OFF
NOTE: Prepare for an Emergency Landing!!

Electrical Fire  [EMERGENCY]
[ ]  Master Switch .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Cabin Heat/Air .... CLOSE
NOTE: Prepare for an Emergency Landing!!

Cabin Fire  [EMERGENCY]
[ ]  Cabin Heat/Air .... OFF
[ ]  Fire .... EXTINGUISH
NOTE: Prepare for an Emergency Landing!!
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