Piper PA-28-140 — pa140_chris_allen_chcklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Nose" item count differs between passes (8 vs 14); verify nothing was dropped.
content_gap: Section "Passenger Briefing" item count differs between passes (19 vs 17); verify nothing was dropped.
content_gap: Section "Speeds for Normal Operation" item count differs between passes (15 vs 14); verify nothing was dropped.

Speeds for Normal Operation
[ ]  Vx .... 64 KTS = Best Angle of Climb
[ ]  Vy .... 74 KTS = Best Rate of Climb
[ ]  Vbst l/d .... 72 KTS = Best Glide
[ ]  Vs .... 56 KTS = Stall Speed, Clean
[ ]  Vso .... 48 KTS = Stall Speed, Dirty
[ ]  Vfo .... 100 KTS = Max Flap Extension
[ ]  Va .... 112 KTS = Maneuvering Speed
[ ]  Vno .... 120 KTS = Max Structr'l Cruise
[ ]  Vne .... 148 KTS = Never Exceed

[ ]  Normal Climb Out .... 90 KTS
[ ]  Short Field T/O, Flaps 25° .... 64 KTS
[ ]  Normal Landing, Flaps Up .... 74 KTS
[ ]  Normal Landing, Flaps 40° .... 66 KTS
[ ]  Short Field, Flaps 40° .... 66 KTS

Specifications
[ ]  Maximum Gross Weight .... 2150 lbs
[ ]  Basic Empty Weight .... 1340 lbs
[ ]  Payload w/Std Fuel (36 gal) .... 594 lbs
[ ]  Payload w/Max Fuel (50 gal) .... 510 lbs
[ ]  Fuel Flow @ 75% Power .... 9 gph
[ ]  Total Fuel Capacity .... 50 gal
[ ]  Standard Fuel Capacity .... 36 gal
[ ]  Fuel Octane Rating (Blue) .... 100LL
[ ]  Oil Sump Capacity .... 8 qts
[ ]  Minimum Oil Quantity .... 2 qts
[ ]  Lycoming O-320 .... 150 hp
[ ]  Battery .... 12 V
[ ]  Positive Limit Load Factor .... 3.8g
[ ]  Negative Limit Load Factor .... 0g

Passenger Briefing
NOTE: Regulations requires the Pilot in Command to brief all passengers on the following items prior to each takeoff.
CABIN DOOR
[ ]  To open cabin door, twist upper door latch forward lift the lower latch up.
[ ]  Push door open.
SEATBACKS
[ ]  Seat backs must be secured in the upright position during takeoff and landing.
SEATBELTS
[ ]  Fasten seat belt & shoulder harness (if present) for take off & landing.
[ ]  Insert latch into buckle & pull belt snug.
[ ]  To release belt, pull up on lip of buckle.
SMOKING & ALCOHOL
[ ]  Smoking and Alcoholic Beverages are not permitted onboard the aircraft at any stage of the flight.
FIRST AID
[ ]  A First Aid kit with sick bags is located behind the Pilot's seat in the seat back in case of emergency.
FIRE EXTINGUICHER
[ ]  A Fire Extinguisher is located behind the two rear seats on the floor.
PILOT OPERATION HANDBOOK
[ ]  The Pilot's Operating Handbook is located in the copilot's seatback. The handbook (POH) shall be the authority if an inconsistency exists between this card and the Pilot's Operating Handbook.
NOTE: If you are intercepted by a U.S. Military or law enforcement aircraft, immediately: 1. Follow the instructions given by the intercepting aircraft. (See chart below.) Attempt to communicate with the intercepting aircraft and/or ATC on the emergency frequency 121.5 MHz, giving the identity and position of your aircraft and the nature of the flight. 2. If equipped with a transponder, squawk 7700, unless otherwise instructed by ATC. If any instructions received by radio from any sources conflict with those given by the intercepting aircraft by visual or radio signals, request clarification while continuing to comply with the instructions given by the intercepting aircraft.

Engine Failure During Takeoff  [EMERGENCY]
[ ]  Throttle [MEMORY] .... IDLE
[ ]  Brakes [MEMORY] .... APPLY
[ ]  Mixture [MEMORY] .... IDLE CUT-OFF
[ ]  Ignition Switch [MEMORY] .... OFF
[ ]  Master [MEMORY] .... OFF

Engine Failure Immediately After Takeoff  [EMERGENCY]
[ ]  Airspeed .... 72 KTS
[ ]  Fuel Selector Valve .... SWITCH TANKS
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON

Engine Failure During Flight  [EMERGENCY]
[ ]  Airspeed .... 72 KTS
[ ]  Carburetor Heat .... ON
[ ]  Fuel Selector Valve .... SWITCH TANKS
[ ]  Mixture .... RICH
[ ]  Master Switch .... ON
[ ]  Auxiliary Fuel Pump .... ON
[ ]  Ignition Switch .... BOTH
[ ]  Primer .... IN & LOCKED
NOTE: If engine failure was caused by fuel exhaustion, power will not be regained after tanks are switched until empty fuel lines are filled, which may require up to ten seconds.

Landing W/O Power  [EMERGENCY]
[ ]  Max Glide Airspeed .... 72 KTS
[ ]  Transponder .... Squawk 7700
[ ]  Radio .... MAYDAY on 121.5 MHz
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF
[ ]  Door .... OPEN
[ ]  Flaps .... FULL
[ ]  Touchdown Speed .... NEAR STALL

Spins  [EMERGENCY]
[ ]  Throttle .... IDLE
[ ]  Rudder .... FULL OPPOSITE TO ROTATION
[ ]  Control Wheel .... FULL FORWARD
[ ]  Rudder .... NEUTRAL (WHEN ROTATION STOPS)
[ ]  Control Wheel .... REGAIN LEVEL FLIGHT

Engine Roughness  [ABNORMAL]
[ ]  Magnetos .... CHECK L & R
[ ]  Mixture .... LEAN AS NECESSARY

Transponder Codes
[ ]  Hijack .... 7500
[ ]  No Radio .... 7600
[ ]  Emergency .... 7700

Electrical Fire / Cabin Fire  [EMERGENCY]
[ ]  Master Switch .... OFF
[ ]  Cabin Heat and Air .... OFF
[ ]  Window Vent .... OPEN
[ ]  Land .... AS SOON AS POSSIBLE

Wing Fire  [EMERGENCY]
[ ]  Wing Strobes .... OFF
[ ]  Nav Lights .... OFF
[ ]  SIDE SLIP TO KEEP FLAMES AWAY FROM FUEL TANKS

Engine Fire During Flight  [EMERGENCY]
[ ]  Fuel Selector Valve .... OFF
[ ]  Throttle .... CLOSED
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Cabin Heat and Air .... OFF
[ ]  Defroster .... OFF
[ ]  Airspeed .... 100 KTS
[ ]  ATTEMPT TO BLOW OUT FLAMES BY DIVING, ALTITUDE PERMITTING
[ ]  Forced Landing .... EXECUTE

Engine Fire During Start on Ground  [EMERGENCY]
[ ]  Cranking .... CONTINUE
IF ENGINE STARTS
[ ]  Power .... 1800 RPM – 2 MIN
[ ]  Engine .... SHUTDOWN & INSPECT
[ ]  Fuel Selector .... OFF
[ ]  Master Switch .... OFF
[ ]  Ignition Switch .... OFF
IF ENGINE FAILS TO START
[ ]  Passengers .... EVACUATE
[ ]  Engine .... SECURE
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Master Switch .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Fire .... EXTINGUISH

Night Flight — Cockpit
[ ]  Required Documents .... AVAILABLE
[ ]  Gust Lock .... REMOVE AND STOW
[ ]  Master and Radio Switch .... ON
[ ]  Fuel Quantity Gauges .... CHECK
[ ]  Master Switch .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Flaps .... DOWN
[ ]  Ignition Switch .... ON
[ ]  Nav Lights .... ON
[ ]  Wing and Tail Strobes .... ON

Right Wing
[ ]  Flap .... SECURE & UNDAMAGED
[ ]  Aileron .... FREE & CORRECT
[ ]  Wing Tip & Light .... UNDAMAGED
[ ]  Nav & Strobe Light .... OPERATIONAL
[ ]  Aileron Counterweight .... FREE
[ ]  Tiedown .... REMOVED
[ ]  Fuel Tank .... FULL, CAP SECURE
[ ]  Fuel Color .... BLUE (100 LL)
[ ]  Tank Drain .... DRAIN, SECURE
[ ]  Landing Gear, Fairing .... UNDAMAGED
[ ]  Tire .... PROPERLY INFLATED
[ ]  Chocks .... REMOVED

Nose
[ ]  Windshield .... CLEAN & UNDAMAGED
[ ]  Engine Oil Level .... 6 TO 8 QTS
[ ]  Engine Oil Dipstick .... SECURED
[ ]  Propeller .... SECURE & UNDAMAGED
[ ]  Spinner .... SECURE & UNDAMAGED
[ ]  Cowling .... SECURE & UNDAMAGED
[ ]  Landing Light .... SECURE & UNDAMAGED
[ ]  Nose Gear, Fairing .... UNDAMAGED

Nose (cont.)
[ ]  Do Not Tow Streamer .... REMOVED
[ ]  Tire .... PROPERLY INFLATED
[ ]  Tow Bar .... REMOVED & STOWED
[ ]  Chocks .... REMOVED
[ ]  Alternator Belt .... TENSION
[ ]  Fuel Sump Drain .... DRAIN, SECURE

Left Wing
[ ]  Fuel Tank .... FULL, CAP SECURE
[ ]  Tank Drain .... DRAIN, SECURE
[ ]  Fuel Color .... BLUE (100LL)
[ ]  Landing Gear, Fairing .... UNDAMAGED
[ ]  Tire .... PROPERLY INFLATED
[ ]  Chocks .... REMOVED
[ ]  Wing Tip & Light .... UNDAMAGED
[ ]  Nav & Strobe Light .... OPERATIONAL
[ ]  Aileron Counterweight .... FREE
[ ]  Tiedown .... REMOVED
[ ]  Pitot Cover .... REMOVED
[ ]  Pitot Mast .... UNDAMAGED
[ ]  Aileron .... FREE
[ ]  Flap .... SECURE & UNDAMAGED

Empennage
[ ]  Elevators .... FREE
[ ]  Rudder .... FREE
[ ]  Trim Tabs .... SECURE & UNDAMAGED
[ ]  Tail Cone & Light .... SECURE & UNDAMAGED
[ ]  Nav & Strobe Light .... OPERATIONAL
[ ]  Tie Down .... REMOVED

Cockpit — Before Starting Engine
[ ]  Ignition Switch .... OFF
[ ]  Preflight Inspection .... COMPLETE
[ ]  Flaps .... UP
[ ]  Seats, Belts .... ADJUSTED, LOCKED
[ ]  Door .... LATCHED
[ ]  Radio Master .... OFF
[ ]  Parking Brake .... SET
[ ]  Fuel Selector .... FULLEST TANK
[ ]  Controls .... CHECK
[ ]  Circuit Breakers .... CHECK

Engine Start (Cold)
[ ]  Master Switch .... ON
[ ]  Mixture .... FULL RICH
[ ]  Fuel Pump .... ON
[ ]  Fuel Pressure .... CHECK
[ ]  Carburetor Heat .... OFF
[ ]  Prime .... PUMP THROTTLE ONCE
[ ]  Throttle .... OPEN ¼ INCH
[ ]  Propeller .... CLEAR
[ ]  Ignition Switch .... BOTH
[ ]  Start Button .... ENGAGE
[ ]  Oil Pressure .... CHECK
[ ]  Engine .... WARM UP 1000 RPM
[ ]  Radios .... ON
[ ]  Transponder .... STANDBY

Instrument Check
[ ]  Compass .... FULL
[ ]  Altimeter .... SET, NOTE ERROR
[ ]  VSI .... INDICATES ZERO
[ ]  AI .... SET
[ ]  DG .... SET TO COMPASS
[ ]  ASI .... ON ZERO
[ ]  TC .... LEVEL, BALL CENTER

Before Taxi
[ ]  Parking Brake .... SET
[ ]  Brakes .... TEST
[ ]  Strobes (Wing & Tail) .... ON
[ ]  Nav Lights .... AS REQUIRED
[ ]  Radios .... ON, CHECKED
[ ]  ATIS Information .... RECORDED
[ ]  Taxi Clearance .... OBTAINED
[ ]  Transponder .... SET CODE, SQUAWK 1200 FOR VFR
[ ]  Flight Plan .... OPENED
[ ]  Flight Following .... REQUESTED

During Taxi
[ ]  Compass .... FULL AND FREE
[ ]  TC .... SHOWS TURN, BALL FREE

Before Takeoff
[ ]  Parking Brake .... SET
[ ]  Lights .... AS REQUIRED
[ ]  Flight Instruments .... SET
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Throttle .... 2000 RPM
[ ]  Magnetos .... CHECK (175 RPM Max drop, 50 RPM diff.)
[ ]  Carburetor Heat .... ON, CHECK RPM
[ ]  Carburetor Heat .... OFF
[ ]  Engine Instruments .... IN GREEN
[ ]  Vacuum Gauge .... IN GREEN
[ ]  Throttle .... 1000 RPM
[ ]  Trim Tab .... SET TO NEUTRAL -1
[ ]  Mixture .... FULL RICH
[ ]  Throttle Friction Lock .... ADJUSTED
[ ]  Fuel Pump .... OFF, CHECK, ON
[ ]  Parking Brake .... OFF
[ ]  Strobe/Nav Lights .... ON/AS REQ'D
[ ]  Transponder .... ON-ALT
[ ]  Tower Clearance .... OBTAINED

Normal Takeoff
[ ]  Flaps .... UP
[ ]  Carburetor Heat .... OFF
[ ]  Auxiliary Fuel Pump .... ON
[ ]  Throttle .... FULL OPEN
[ ]  Rotate .... 50 KTS
[ ]  Climb Speed .... 74 KTS

Soft Field Takeoff / Short Field Takeoff — Obstacle Clearance
[ ]  Flaps .... 25° (Second Notch)
[ ]  Carburetor Heat .... OFF
[ ]  Fuel Pump .... ON
[ ]  Position .... END OF RUNWAY
[ ]  Brakes .... FULL
[ ]  Throttle .... FULL OPEN
[ ]  Brakes .... RELEASE
[ ]  Rotate .... 50 KTS
[ ]  Initial Climb Speed .... 64 KTS

Climb Out
[ ]  Normal Climb .... 75 – 90 KTS
[ ]  VY – Best Rate Climb .... 74 KTS
[ ]  VX – Best Angle Climb .... 64 KTS

Cruise
[ ]  Fuel Pump .... OFF
[ ]  Power .... 2200-2600 RPM
NOTE: AVOID 2000-2200 RPM
[ ]  Trim Tab .... SET
[ ]  Mixture .... ADJUST
[ ]  Fuel Selector .... SWITCH AS NEEDED

Before Landing
[ ]  Seats, Belts .... ADJUST, LOCK
[ ]  Fuel Selector .... ON, FULLEST TANK
[ ]  Mixture .... FULL RICH
[ ]  Fuel Pump .... ON
[ ]  Parking Brake .... OFF
[ ]  Flaps .... AS REQUIRED, BELOW 100 KTS
[ ]  Airspeed .... 74 KTS
[ ]  Landing Light .... ON AS REQUIRED

After Landing
[ ]  Flaps .... UP
[ ]  Auxiliary Fuel Pump .... OFF
[ ]  Landing Light .... OFF(DAY)/ON (NIGHT)
[ ]  Carburetor Heat .... OFF
[ ]  Transponder .... STANDBY
[ ]  Taxi Clearance .... OBTAINED
[ ]  Flight Plan .... CLOSED

Shut-Down & Securing Plane
[ ]  Electrical Equipment, Radios .... OFF
[ ]  Lights .... OFF
[ ]  Throttle .... 1200 RPM
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Ignition .... OFF
[ ]  Keys .... REMOVED
[ ]  Master Switch .... OFF
[ ]  Gust Lock .... INSTALLED
[ ]  Chocks/Tiedowns .... INSTALLED
[ ]  Pitot Tube Cover .... INSTALLED
[ ]  Do Not Tow Streamer .... INSTALLED

Transponder Codes
[ ]  Hijack .... 7500
[ ]  No Radio .... 7600
[ ]  Emergency .... 7700

Light Gun Signals
ON GROUND
[ ]  Steady GREEN .... TAKE OFF
[ ]  Flashing GREEN .... TAXI
[ ]  Steady RED .... STOP
[ ]  Flashing RED .... CLEAR RUNWAY
[ ]  Flashing White .... RETURN TO RAMP
[ ]  RED/GREEN FLASH .... USE CAUTION
IN FLIGHT
[ ]  Steady GREEN .... LAND
[ ]  Flashing GREEN .... RETURN TO LAND
[ ]  Steady RED .... GIVE WAY TO TRAFFIC
[ ]  Flashing RED .... DO NOT LAND
[ ]  RED/GREEN FLASH .... USE CAUTION
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