Piper PA-28-151 Warrior — John_PipperWarriorPA28-151 checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Engine Fire - Start" item count differs between passes (40 vs 6); verify nothing was dropped.

Preflight Inspection
IN CABIN
[ ]  Seat Belt control
[ ]  Master Switch
[ ]  Fuel Quantitiy Gauges
[ ]  All ext Lights
[ ]  Stall warning
[ ]  Master Switch
[ ]  Control Surfaces
[ ]  External Damage
[ ]  Operational interface
[ ]  Surface and Hinges
[ ]  Free of Snow, Ice, Frost
WINGS
[ ]  Fuel Supply Cap
[ ]  2 Fuel Sumps
[ ]  Fuel Vents
[ ]  Pito Head Lft Wing
MAIN LANDING GEAR
[ ]  Strut Inflation
[ ]  Tires Inflation, Wear
[ ]  Brake Disc
[ ]  Brake line
NOSE
[ ]  Wind Sheild
[ ]  Prop.
[ ]  spinner
[ ]  Air Inlets
[ ]  Fuel - Oil leaks
[ ]  Oil
[ ]  Fuel Strainer Sump
[ ]  Tire Inflation, Wear
[ ]  Strut Inflation
BAGGAGE COMPARTMENT
[ ]  Tow Bar
[ ]  Baggage
[ ]  Door Closed
IN CABIN
[ ]  Flight Controls
[ ]  Cabin Door
[ ]  A.R.R.O.W. papers
[ ]  Belts. Inertia Reel

Before Start
[ ]  Chocks
[ ]  P-Break
[ ]  Circuit brks
[ ]  Carb Heat
[ ]  Avionics
START ENGINE-COLD
[ ]  Throttle
[ ]  Master switch
[ ]  Elec. Fuel Pump
[ ]  Mixture
[ ]  Primer
[ ]  Starter
[ ]  Throttle
[ ]  Oil Press.
START ENGINE-HOT
[ ]  Throttle
[ ]  Master switch
[ ]  Elec. Fuel Pump
[ ]  Mixture
[ ]  Starter
[ ]  Throttle
[ ]  Oil Press.
START ENIGINE-FLD
[ ]  Throttle
[ ]  Master switch
[ ]  Elec. Fuel Pump
[ ]  Mixture
[ ]  Starter
[ ]  Throttle
[ ]  Oil Press.
[ ]  Throttle
BEFORE TAXI
[ ]  Elec. Fuel Pump
[ ]  P-Break
[ ]  Avionics
[ ]  Transponder
[ ]  Taxi Area
[ ]  Throttle
[ ]  Brakes
[ ]  Steering

Ground Run-Up
[ ]  P-Brake
[ ]  Elec. Fuel Pump
[ ]  RPM
[ ]  Mag
[ ]  Carb Heat
[ ]  Vacuum
[ ]  Oil Temp
[ ]  Oil Press
[ ]  Annunciator
[ ]  Elec. Fuel Pump
[ ]  Fuel Press.
[ ]  Throttle
[ ]  Flight Controls
NOTE: Engine is warm when throttle can be open without engine faltering.
BEFORE TAKE OFF
[ ]  Instruments
[ ]  Mixture
[ ]  Transponder
[ ]  Lights
[ ]  Electric Fuel Pump
[ ]  T/O Trim
[ ]  Flaps
NORMAL TAKE OFF
[ ]  Trim Tab
[ ]  Accelerate
SHORT FIELD TAKE OFF
[ ]  Flaps
[ ]  Accelerate
[ ]  Yoke - maintain back pressure at VR to climb
NOTE: Mantian 50 kts until obstacle clearance….. after clear……
[ ]  Accelerate
[ ]  Flaps
NOTE: L/D - 73 Vs - 50
NOTE: Vy - 75 Vso - 44
NOTE: Vx - 63 Vno - 126
NOTE: Vne - 160 Vfe - 103
NOTE: Va - 111

Soft Field, No Obsctacle
[ ]  Flaps
[ ]  Starter
[ ]  Lift Nose Gear ASAP
[ ]  Accel in Grnd Effect
[ ]  Climb
AFTER TAKE-OFF
[ ]  Flaps
[ ]  Elec. Fuel Pump
[ ]  Fuel Press
[ ]  Lights
[ ]  Mixture
APPROACH AND LAND
[ ]  Lights
[ ]  Fuel Selector
[ ]  Seat Belts
[ ]  Elec. Fuel Pump
[ ]  Mixture
[ ]  Flaps
[ ]  VREF 40 deg
AFTER LANDING
[ ]  Flaps
[ ]  Elec. Fuel Pump
[ ]  Radios
[ ]  Throttle rpm
[ ]  Mixture
[ ]  Lights
STOP ENGINE
[ ]  Avionics
[ ]  Mixture
[ ]  Magnetos
[ ]  Master Switch
PARKING
[ ]  P Break
[ ]  Yoke
[ ]  Chocks
[ ]  Tie Downs
[ ]  Cover

Engine Fire - Start
[ ]  Starter        crank engine
[ ]  Mixture
[ ]  Throttle
[ ]  Elec. Fuel Pump
[ ]  Fuel selector
[ ]  Abandon if Continues
ENGINE FAILURE DURING T/O
[ ]  if insufficient runway
[ ]  Maintain Safe Air Speed
[ ]  Make only shallow turns
[ ]  Flaps as situation req.
IF SUFFICIENT ALT. FOR RESTART
[ ]  Air Speed
[ ]  Fuel Selector
[ ]  Elec. Fuel Pump
[ ]  Mixture
[ ]  Carb Heat
ENGINE LOSS IN FLIGHT
[ ]  Fuel selector
[ ]  Elec. Fuel Pump
[ ]  Mixture
[ ]  Carb Heat
[ ]  Gauges
[ ]  Primer
WHEN POWER IS RESTORED
[ ]  Carb Heat
[ ]  Elec. Fuel Pump
POWER OFF LANDING
[ ]  Squak
[ ]  Glide
[ ]  Landing Site
[ ]  Establish spiral patern
[ ]  Position for normal approach
NOTE: When field can easily be reached slow to 63 kts.
WHEN COMMITED
[ ]  Ignition
[ ]  Master Switch
[ ]  Fuel selector
[ ]  Mixture
[ ]  Belts

Fire In Flight
[ ]  Source of Fire
ELEC FIRE SMOKE IN CABIN
[ ]  Master Switch
[ ]  Vents
[ ]  Cabin Heat
[ ]  Land as soon as posible
ENGINE FIRE
[ ]  Fuel Selector
[ ]  Throttle
[ ]  Mixture
[ ]  Elec Fuel Pump
[ ]  Heater
[ ]  Defroster
[ ]  Make power off landing
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