Piper PA-28-161 Warrior II — David_Kohl_PiperWarriorIIChecklists5x8
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Danbury Radio Frequencies" item count differs between passes (12 vs 13); verify nothing was dropped.
content_gap: Section "Pre-flight Inspection – Exterior" item count differs between passes (11 vs 54); verify nothing was dropped.
content_gap: Section "Takeoff Reference Speeds" item count differs between passes (6 vs 9); verify nothing was dropped.

Pre-flight Planning
[ ]  Weather .... Checked
[ ]  Performance data .... Checked
[ ]  Weight & balance
[ ]  Aircraft documents .... Verified
NOTE: Airworthiness certificate, Registration, Operations manual (ARrOw)

Pre-flight Inspection – Interior
[ ]  Parking brake .... Set as desired
[ ]  Controls .... Free and clear
[ ]  Ignition .... Off
[ ]  Avionics .... Off
[ ]  Master switch .... On
[ ]  Lights .... On and verified
[ ]  Fuel pump .... On
[ ]  Fuel pressure / quantity .... Checked
[ ]  Fuel pump .... Off
[ ]  Master switch .... Off
[ ]  Flaps .... Extended

Pre-flight Inspection – Exterior
RIGHT WING
[ ]  Flap condition .... Checked
[ ]  Aileron .... Checked
[ ]  Wing tip .... Checked
[ ]  Wing surface condition .... Checked
[ ]  Fuel level .... Checked
[ ]  Fuel vent .... Checked
[ ]  Fuel sump .... Drained
[ ]  Main gear strut .... Checked
[ ]  Tire, brakes and fluid .... Checked
[ ]  Tie down .... Removed

Engine Cowling
[ ]  Windshield .... Checked
[ ]  Surface condition .... Checked
[ ]  Right cowling fasteners .... Open
[ ]  Interior wiring, pipes, etc. .... Checked
[ ]  Oil level .... Between 6 and 8 quarts
[ ]  Right cowling fasteners .... Closed
[ ]  Propeller .... Checked
[ ]  Spinner .... Checked
[ ]  Alternator belt .... Checked
[ ]  Air inlets .... Free and clear
[ ]  Exhaust system .... Tight
[ ]  Nose gear strut .... Checked
[ ]  Tire .... Checked
[ ]  Left cowling fasteners .... Open
[ ]  Interior wiring, pipes, etc. .... Checked
[ ]  Brake fluid .... Checked
[ ]  Left Cowling fasteners .... Closed
[ ]  Fuel sump .... Checked
[ ]  Surface condition .... Checked
[ ]  Windshield .... Checked

Left Wing
[ ]  Main gear strut .... Checked
[ ]  Tire, brakes and fluid .... Checked
[ ]  Fuel sump .... Checked
[ ]  Fuel vent .... Checked
[ ]  Tie down .... Removed
[ ]  Pitot and static port .... Checked
[ ]  Fuel level .... Checked
[ ]  Stall warning .... Checked
[ ]  Surface condition .... Checked
[ ]  Wing tip .... Checked
[ ]  Aileron .... Checked
[ ]  Flap condition .... Checked

Aft Fuselage and Empennage
[ ]  Left surface condition .... Checked
[ ]  Antennas .... Checked
[ ]  Stabilator, trim tab .... Checked
[ ]  Rudder .... Checked
[ ]  Tie down .... Removed
[ ]  Tail cone, skid .... Checked
[ ]  Right surface condition .... Checked
[ ]  Baggage door .... Checked

Pre-flight Inspection (continued)
INTERIOR
[ ]  Flaps .... Retracted
[ ]  Seats .... Adjusted and locked
[ ]  Seatbelts .... On
[ ]  Shoulder harness .... On
[ ]  Passenger briefing .... Complete

Before Engine Start
[ ]  Trim (elevator & rudder) .... Set
[ ]  Fuel selector .... Lowest tank
[ ]  Heat / fresh air controls .... Set
[ ]  Circuit breakers .... Checked
[ ]  Carb heat .... Cold
[ ]  Friction lock .... Set
[ ]  Mixture .... Full rich
[ ]  Throttle .... Set
[ ]  Primer .... As required, then locked
[ ]  Mags .... Off
[ ]  Flight instruments .... Checked
[ ]  Avionics .... Off
[ ]  Lights .... Beacon on
[ ]  Fuel pump .... On
[ ]  Master switch .... On
[ ]  Fuel pressure .... Checked
[ ]  Propeller area .... Cleared
[ ]  Toe brakes .... Feet on pedals
[ ]  Parking brake .... Released
[ ]  Ignition switch .... Start engine

After Engine Start
[ ]  Throttle .... 1,000 RPM
[ ]  Oil pressure .... Checked
[ ]  Fuel pump .... Off
[ ]  Fuel pressure .... Checked
[ ]  Alternator .... Checked
[ ]  Vacuum .... Checked
[ ]  Avionics .... On
[ ]  Radios .... Set
[ ]  ATIS .... Obtain
[ ]  Altimeter .... Set
[ ]  Directional gyro .... Magnetic Compass

Taxi
[ ]  Ground control for taxi .... Call
[ ]  Parking brake .... Released
[ ]  Toe brakes .... Checked
[ ]  Flight controls .... As required for wind
[ ]  Taxi .... Monitor traffic
[ ]  Flight instruments .... Checked
[ ]  Hold in run-up area .... Hold

Before Takeoff
[ ]  Parking brake or toe brakes .... Set
[ ]  Throttle .... 1000 RPM
[ ]  Trim .... Set
[ ]  Fuel pump .... On
[ ]  Fuel pressure .... Checked
[ ]  Fuel selector .... Fullest tank
[ ]  Fuel pump .... Off
[ ]  Fuel pressure .... Checked

Engine Run-up
[ ]  Throttle .... 2000 RPM
[ ]  Magnetos .... Checked
NOTE: Max drop 175 RPM, Max difference 50 RPM
[ ]  Engine Instruments .... Green band
[ ]  Enunciator lights .... V A O Checked
[ ]  Vacuum .... 4.8 to 5.2 PSI
[ ]  Ammeter .... Charging
[ ]  Carb heat .... Some decrease, no rise
[ ]  Mixture .... Full rich
NOTE: Lean mixture above 3000 feet
[ ]  Throttle .... Idle, then 1000 RPM
[ ]  Parking brake .... Verify off

Pre-flight Completion
[ ]  Altimeter .... Indicated alt = Ground alt
[ ]  Directional gyro .... Magnetic compass
[ ]  Flight instruments .... Checked
[ ]  Radios .... COM / NAV set
[ ]  Flight controls .... Free and clear
[ ]  Flaps .... Set as needed
[ ]  Safety briefing .... Complete
[ ]  Doors and windows .... Locked
[ ]  Tower .... Call

Position and Hold
[ ]  Strobe lights .... On
[ ]  Nav lights .... On for night flight
[ ]  Auto-pilot .... Verify Off
[ ]  Flight controls .... Free and clear
[ ]  Transponder .... On ALT

Cleared for Takeoff
[ ]  Fuel pump .... On
[ ]  Fuel pressure .... Checked
[ ]  Landing lights .... On
[ ]  Time .... Check

After Takeoff
[ ]  Flaps .... Up
[ ]  Landing lights .... Off
[ ]  Fuel pump .... Off
[ ]  Fuel pressure .... Checked

Cruise
[ ]  Cruise power .... Set
[ ]  Mixture .... Set
[ ]  Engine instruments .... Checked
[ ]  Directional Gyro .... Magnetic Compass
[ ]  Fuel selector .... As required
NOTE: Switch tanks after first ½ hour and then every hour

Descent
[ ]  ATIS .... Obtain
[ ]  Tower .... Call
[ ]  Safety briefing .... Complete
[ ]  Seat belts and harness .... On
[ ]  Landing lights .... On
[ ]  Fuel pump .... On
[ ]  Fuel pressure .... Checked
[ ]  Fuel selector .... Fullest tank
[ ]  Mags .... Checked on both
[ ]  Engine instruments .... Checked
[ ]  Directional Gyro .... Magnetic Compass
[ ]  Primer .... Locked
[ ]  Mixture .... Full rich
[ ]  Carb heat .... Checked

Approach for Landing
[ ]  VFE Clean to 10˚ .... 103 KIAS
[ ]  VMin Approach .... 70 KIAS
[ ]  VLanding with flaps at 40˚ .... 63 KIAS

After Landing
[ ]  Flaps .... Retract
[ ]  Trim .... Reset
[ ]  Fuel pump .... Off
[ ]  Fuel pressure .... Checked
[ ]  Landing and strobe lights .... Off
[ ]  Transponder .... Standby
[ ]  Ground control .... Call

Engine Shutdown
[ ]  Parking brake .... As required
[ ]  Throttle .... 1000 RPM
[ ]  Avionics .... Off
[ ]  Mixture .... Idle cutoff
[ ]  Magnetos .... Off after prop stops
[ ]  Lights .... Off
[ ]  Master switch .... Off

Secure Aircraft
[ ]  Controls .... Seat belt secured
[ ]  All switches .... Verify off
[ ]  Hobbs / Tach times .... Record
[ ]  Doors and windows .... Closed
[ ]  Aircraft .... Tie down

Engine Fire During Start  [EMERGENCY]
Engine Fire During Start
[ ]  Starter .... Continue cranking
[ ]  Mixture .... Idle cutoff
[ ]  Throttle .... Wide open
[ ]  Fuel pump .... Off
[ ]  Fuel selector .... Off
[ ]  If fire persists .... Evacuate

Engine Fire During Flight  [EMERGENCY]
Engine Fire During Flight
[ ]  Airspeed .... Increase
[ ]  Fuel pump .... Off
[ ]  Fuel selector .... Off
[ ]  Throttle .... Closed
[ ]  Mixture .... Idle cutoff
[ ]  Magnetos .... Off
[ ]  Cabin heat / defrost / air .... Off
[ ]  Emergency landing check .... Perform

Electrical Fire (Smoke)  [EMERGENCY]
Electrical Fire (Smoke)
[ ]  Master switch .... Off
[ ]  Electrical equipment .... Off
[ ]  Floor air vents .... Open
[ ]  Cabin heat / air .... Off
[ ]  If smoke stops .... Troubleshoot
[ ]  Land .... ASAP

Loss of Oil Pressure  [EMERGENCY]
Loss of Oil Pressure
[ ]  Land .... ASAP
[ ]  Prepare for Engine failure

Loss of Fuel Pressure  [EMERGENCY]
Loss of Fuel Pressure
[ ]  Fuel pump .... On
[ ]  Fuel selector .... Switch tanks
[ ]  Fuel pressure .... Checked
[ ]  Prepare for Engine failure

High Oil Temperature  [EMERGENCY]
High Oil Temperature
[ ]  Mixture .... Full rich
[ ]  Land .... ASAP
[ ]  Prepare for Engine failure

Alternator / Generator Failure  [EMERGENCY]
Alternator / Generator Failure
[ ]  Ammeter .... Check
[ ]  Alternator switch .... Off
[ ]  Circuit breakers .... Check
[ ]  Alternator switch .... On
NOTE: If power cannot be restored, reduce electrical load
[ ]  Land .... ASAP

Engine Failure  [EMERGENCY]
Engine Failure
[ ]  Safe airspeed .... 73 KIAS
[ ]  Best place to land .... Choose
[ ]  Carb heat .... On
[ ]  Begin maneuvering toward safe landing area
[ ]  Fuel pump .... On
[ ]  Mixture .... Different setting
[ ]  Throttle .... Different setting
[ ]  Primer .... Verify locked
[ ]  Fuel pressure .... Checked
[ ]  Magnetos .... Checked
[ ]  Fuel selector .... Switch tanks

Emergency Landing  [EMERGENCY]
Emergency Landing
[ ]  Best glide speed .... 73 KIAS
[ ]  Seat belt / harness .... On
[ ]  Fuel selector .... Off
[ ]  Magnetos .... Off
[ ]  Mixture .... Idle cutoff
[ ]  Fuel pump .... Off
[ ]  Door .... Consider opening
[ ]  Master switch .... Off

Transponder Codes
[ ]  7500 .... Hijacking
[ ]  7600 .... Lost radio communications
[ ]  7700 .... General emergency
[ ]  7777 .... Military interceptor

Pilot-Controlled Lighting
[ ]  Seven clicks .... Turns on, high intensity
[ ]  Five clicks .... Medium intensity
[ ]  Three clicks .... Low intensity

ATC Light Signals
ON THE GROUND
[ ]  Flashing Green .... Cleared to taxi
[ ]  Steady Green .... Cleared for takeoff
[ ]  Flashing Red .... Taxi clear of runway
[ ]  Steady Red .... Stop
[ ]  Flashing White .... Return to FBO
[ ]  Alt Red and Green .... Use caution
IN THE AIR
[ ]  Flashing Green .... Return for landing
[ ]  Steady Green .... Cleared to land
[ ]  Flashing Red .... Airport unsafe
[ ]  Steady Red .... Give way, circle
[ ]  Alt Red and Green .... Use caution

Takeoff Reference Speeds
[ ]  VRotate (clean) .... 55 KIAS
[ ]  VRotate (25˚ flaps) .... 52 KIAS
[ ]  VY .... 79 KIAS
NOTE: Best Rate: Greatest alt gain in shortest time
[ ]  VX .... 63 KIAS
NOTE: Best Angle: Greatest alt gain in shortest distance

Danbury Runways
[ ]  Rwy 08-26 .... 4422X150
[ ]  Rwy 17-35 .... 3135X100

Danbury Radio Frequencies
[ ]  ATIS .... 127.75
[ ]  Ground Control .... 121.60
[ ]  Tower / CTAF .... 119.40
[ ]  UNICOM .... 122.95
[ ]  NY Dep / Appr .... 126.40
[ ]  Clearance Delivery .... 128.60
NOTE: when DXR tower closed
[ ]  Carmel VOR/DME .... 116.60
[ ]  ILS/DME 08 .... 111.55

Danbury Radio Frequencies
[ ]  ATIS .... 127.75
[ ]  Ground Control .... 121.60
[ ]  Tower / CTAF .... 119.40
[ ]  UNICOM .... 122.95
[ ]  NY Dep / Appr .... 126.40
[ ]  Bridgeport FSS .... 122.20
[ ]  Carmel VOR/DME .... 116.60
[ ]  ILS/DME 08 .... 111.55
NOTE: Mayday: Call 121.5 and Squawk 7700
[ ]  VA at 2325 Lbs .... 111 KIAS
[ ]  VA at 1531 Lbs .... 88 KIAS
[ ]  VEn-Route Climb .... 87 KIAS
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