Piper PA-28-161 Warrior II — p28a_checklist_moorabbin
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "POWER OFF LANDING" item count differs between passes (1 vs 3); verify nothing was dropped.

PRE START
[ ]  Loose items stowed
[ ]  Seat adjusted
[ ]  Hatches and harnesses secure
[ ]  Trims through range set to take off
[ ]  Flaps checked, set zero
[ ]  Park Brake on
[ ]  Fuel on left tank
[ ]  Carburetor Heat off
[ ]  Mixture idle cut off
[ ]  Throttle closed
[ ]  Instruments checked and set
[ ]  Avionics off
[ ]  Switches off
[ ]  Master on
[ ]  Circuit breakers in
[ ]  Controls full and free, correct sense

START CHECKS
[ ]  Mixture rich
[ ]  Throttle 1 cm open
[ ]  Fuel pump on, check press & off
[ ]  Prime Cold – 5 times, Hot – 0 times
[ ]  Check “Clear Prop”
[ ]  Magnetos start

AFTER START
[ ]  Throttle set 1000 rpm
[ ]  Oil pressure green within 30 secs
[ ]  Alternator on
[ ]  Ammeter positive charge
[ ]  Suction within limits
[ ]  Gyro instruments erection and sync
[ ]  Annunciators test & out
[ ]  Avionics on
[ ]  Beacon on
[ ]  Transponder STBY

TAXI CHECKS
[ ]  Brakes checked
[ ]  Instruments turning checks

RUN-UP CHECKS
[ ]  Park brake on
[ ]  Fuel selector check tank
[ ]  Oil temp & pressure green arc
[ ]  Lookout all clear
[ ]  Throttle set 2000 rpm
[ ]  Oil temp & pressure green arc
[ ]  Magnetos left, both, right, both
[ ]  Carb Heat on, check, drop then off
[ ]  Ammeter positive charge
[ ]  Suction 4.8” – 5.1” Hg
[ ]  Slow idle smooth running
[ ]  Throttle set 1000 rpm

PRE T/O VITAL ACTIONS
[ ]  T trims set, throttle friction adjusted
[ ]  M mixture rich
[ ]  P primer – locked
[ ]  F fuel on, contents checked
[ ]  F 3 stages flap checked
[ ]  I instruments checked and set
[ ]  auto pilot checked
[ ]  S switches, as required
[ ]  C controls full & free
[ ]  H hatches & harnesses secure

PRE LINE UP CHECKS
[ ]  F fuel pump on, flaps set
[ ]  I instruments, DG to runway heading
[ ]  S switches, lights as required
[ ]  T transponder to ALT

AFTER T/O CHECKS
[ ]  Flaps retracted
[ ]  Power set as required
[ ]  Oil temp & pressure green arc
[ ]  Fuel pump off, pressure checked

Pre manoeuvre checks
[ ]  H Height
[ ]  A Airframe
[ ]  S Security
[ ]  E Engine
[ ]  L Location
[ ]  L Lookout

PRE LANDING CHECKS
[ ]  B Brakes, check pressure and off
[ ]  U Undercarriage down
[ ]  M Mixture rich
[ ]  F Fuel pump on, press & contents
[ ]  O Oil Temp & Pressure
[ ]  C Carb Heat on
[ ]  H Hatches & Harnesses secure

AFTER LANDING CHECKS
[ ]  Flaps retract
[ ]  Fuel Pump off
[ ]  Strobes off
[ ]  Transponder STBY
[ ]  Radio to SMC

SHUTDOWN
[ ]  Park brake on
[ ]  Throttle set 1000 rpm
[ ]  Avionics off
[ ]  Beacon off
[ ]  Magnetos check for RPM drop
[ ]  Temp and pressure green arc
[ ]  Alternator off
[ ]  Mixture idle cut off
[ ]  Master off
[ ]  Magnetos off, key out
[ ]  Park brake release if tieing down

POST FLIGHT
[ ]  Controls secure
[ ]  Hatches secure
[ ]  Tie downs secured

RADIO FREQUENCIES
[ ]  MB GROUND 119.9 MHz
[ ]  MB TOWER (EAST) 118.1 MHz
[ ]  MB TOWER (WEST) 123.0 MHz
[ ]  MB ATIS 398 or 120.9 MHz
[ ]  EN GROUND 121.9 MHz
[ ]  EN TOWER 125.1 MHz
[ ]  EN ATIS 356 or 119.8 MHz
[ ]  ML RAS 135.7 MHz
[ ]  ML APP 124.7 MHz
[ ]  ML DEP 118.9 or 129.4 MHz
[ ]  ML TWR 120.5 MHz
[ ]  ML SMC 121.7 MHz
[ ]  ML ACD 127.2 MHz
[ ]  ML ATIS 114.1 or 132.7 MHz

ENGINE FIRE DURING START  [EMERGENCY]
[ ]  Starter crank engine
[ ]  Mixture idle cut off
[ ]  Throttle open
[ ]  Electric fuel pump off
[ ]  Fuel selector off
[ ]  Abandon if fire continues

ENGINE FIRE IN FLIGHT  [EMERGENCY]
[ ]  Mixture idle cut-off
[ ]  Throttle closed
[ ]  Fuel Pump off
[ ]  Fuel Selector off
[ ]  Heater off
[ ]  Defroster off
[ ]  Proceed with POWER OFF LANDING

ENGINE FAILURE IN FLIGHT  [EMERGENCY]
INITIAL ACTIONS:
[ ]  CHECK FOR FIRE
[ ]  Throttle set 1/3 position
[ ]  Carburetor Heat on
[ ]  Mixture rich
[ ]  Fuel pump on
[ ]  Fuel selector change tanks
[ ]  ASSESS WIND
[ ]  SELECT FIELD
[ ]  MAKE PLAN
TROUBLE CHECKS:
[ ]  Fuel on contents checked
[ ]  Mixture through range, set rich
[ ]  Oil temps and pressure
[ ]  Switches check magnetos
[ ]  Throttle through range set 1/3 position
[ ]  MAYDAY CALL
SHUTDOWN CHECKS:
[ ]  Brakes check pressure and off
[ ]  Undercarriage down
[ ]  Switches all off, fuel off
[ ]  Hatches and harnesses secure

LOSS OF OIL PRESSURE / HIGH OIL TEMPERATURE  [EMERGENCY]
[ ]  Land as soon as possible and investigate cause.
[ ]  Prepare for power off landing

POWER OFF LANDING  [EMERGENCY]
NOTE: For other emergency procedures refer to section 3 of the Pilots Operating Handbook.

AIRSPEEDS
[ ]  Basic Stall Speed (VS1) 50 KIAS
[ ]  Stall with Flap (VS0) 44 KIAS
[ ]  Best Climb Angle (VX) 63 KIAS
[ ]  Best Climb Rate (VY) 79 KIAS
[ ]  Cruise Climb (Normal) 87 KIAS
[ ]  Flap Limit Speed (VFE) 103 KIAS
[ ]  Threshold 65 KIAS
[ ]  Manoeuvre Speed (VA) 88 - 111 KIAS
[ ]  Flight Planning TAS 105 KTAS
[ ]  Maximum Cruising (VNO) 126 KIAS
[ ]  Never Exceed (VNE) 160 KIAS
[ ]  Best Glide 73 KIAS
[ ]  TOSS 64 KIAS
[ ]  Base 70 KIAS
[ ]  Maximum Crosswind 17 KIAS

WEIGHT LIMITATIONS
[ ]  Max Takeoff Weight 1055 Kg Lb
[ ]  Empty Weight: Refer flight manual
[ ]  Max Baggage Weight

FUEL
[ ]  Type: 100 Octane Avgas (green) or 100 LL (blue)
[ ]  Quantity: Total 189 lt, Useable 181 lt (fuel flow at 75%)
[ ]  Typical Consumption: 36 lt per hour
[ ]  Endurance with 45 min reserve intact: 5 hrs

POWER SETTINGS
[ ]  Max RPM 2700 RPM
[ ]  Static RPM

ENGINE
[ ]  Avco Lycoming IO-320 D2A or D3G
[ ]  4 cylinder, horizontally opposed, direct drive, air cooled, fuel injected
[ ]  Output: 160 Hp @ 2700 rpm

OIL
[ ]  Type: Aviation grade D100
[ ]  Quantity: Max 8 US quarts, Min 6 US quarts (Company reqts)
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