Piper PA-28-180 Cherokee Archer — pa28180_abbreviated_checklist_millstone_valley
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Piper Cherokee Airspeeds (MCAS)" item count differs between passes (11 vs 1); verify nothing was dropped.

BEFORE STARTING ENGINE
NOTE: Refer to Aircraft Flight Manual for N3471R or N4677R as Appropriate.
[ ]  Exterior Preflight .... COMPLETE
[ ]  Tach/Hobbs Meter .... RECORD
[ ]  Seats, Belts, Harnesses .... ADJUST & LOCKED
[ ]  Radios & Electrical Equipment .... OFF
[ ]  Brakes .... TEST & SET

STARTING ENGINE
[ ]  Parking Brake .... SET
[ ]  Carburetor Heat .... COLD
[ ]  Fuel Selector .... SET TO DESIRED TANK
COLD START
[ ]  Throttle .... OPEN ¼ INCH
[ ]  Master Switch .... ON
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture .... RICH
[ ]  Magnetos .... ROTATE SWITCH CLOCKWISE WHILE PRESSING IN
N4677R: With Magnetos on Both, Press the Starter Push-button.
[ ]  Throttle .... ADVANCE WHEN ENGINE FIRES
HOT START
[ ]  Throttle .... OPEN ½ INCH
[ ]  Master Switch .... ON
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture .... IDLE CUTOFF
[ ]  Starter .... ROTATE SWITCH CLOCKWISE WHILE PRESSING IN
N4677R: With Magnetos on Both, Press the Starter Push-button.
[ ]  Mixture .... ADVANCE WHEN ENGINE FIRES
[ ]  Throttle .... ADJUST
FLOODED START
[ ]  Throttle .... OPEN FULLY
[ ]  Master Switch .... ON
[ ]  Electric Fuel Pump .... OFF
[ ]  Mixture .... IDLE CUT OFF
[ ]  Magnetos .... ROTATE SWITCH CLOCKWISE WHILE PRESSING IN
N4677R: With Magnetos on Both, Press the Starter Push-button.
[ ]  Mixture .... ADVANCE WHEN ENGINE FIRES
[ ]  Throttle .... ADJUST

GROUND CHECK
[ ]  Brakes .... SET
[ ]  Throttle .... 1800 RPM
[ ]  Magnetos .... CHECK
125 MAX DROP/50 DIFF.
[ ]  Carburetor Heat .... CHECK FOR RPM DROP
[ ]  Engine Gauges .... CHECK
[ ]  Fuel Pump .... CHECK OPERATION

TAKEOFF
[ ]  Fuel .... ON PROPER TANK
[ ]  Electric Fuel Pump .... ON
[ ]  Engine Gauges .... CHECKED
[ ]  Carburetor Heat .... OFF
[ ]  Mixture .... SET
[ ]  Quadrant Friction Lock .... SET
[ ]  Trim Tabs .... SET
[ ]  Flaps .... SET
[ ]  Controls .... FREE & CORRECT
[ ]  Door .... LATCHED

ENROUTE CLIMB
[ ]  Airspeed .... 85 - 100 MPH
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... RICH
Unless engine is rough.

CRUISE
[ ]  Power .... 2300 to 2700
No more than 75%.
[ ]  Fuel Selector .... ON PROPER TANK
[ ]  Mixture .... FULL RICH BELOW 5000 FT

APPROACH & LANDING
[ ]  Fuel Selector .... ON PROPER TANK
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture .... SET
[ ]  Flaps .... SET
[ ]  Airspeed .... 85 MPH (NO FLAPS) OR 80 MPH (FLAPS)

BALKED LANDING
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... COLD
[ ]  Wing Flaps .... RETRACT TO 2nd NOTCH
[ ]  Airspeed .... 85 MPH
[ ]  Wing Flaps .... RETRACT (slowly)

NORMAL LANDING
[ ]  Touchdown .... MAIN WHEELS FIRST
[ ]  Landing Roll .... LOWER NOSE WHEEL GENTLY
[ ]  Braking .... MINIMUM REQUIRED

AFTER LANDING
[ ]  Wing Flaps .... UP
[ ]  Fuel Pump/Unnecessary Equipment .... OFF

SECURING AIRCRAFT
[ ]  Parking Brake .... SET
[ ]  Radios, Electrical Equipment .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
[ ]  Tach/Hobbs Meter .... RECORD

Piper Cherokee Airspeeds (MCAS)
NOTE: Vr 65
NOTE: Vx 74
NOTE: Vy 85
NOTE: Va 129
NOTE: Vs1 63
NOTE: Vso 54
NOTE: Vfe 115
NOTE: Vno 140
NOTE: Vne 171
NOTE: Glide 85
NOTE: XW demo 15
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