Piper PA-28-200R Arrow II — jimquinn_arrow2_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Preflight / Engine Start / Taxi / Ground Run-Up / Take Off / Cruise / Landing / Emergency
[ ]  Master .... ON
[ ]  Advance mixture when eng starts.
[ ]  Oil Pressure .... GREEN
[ ]  Throttle .... 1400 – 1500 RPM
[ ]  Mixture .... Lean for taxi
[ ]  Oil Press, Oil Temp .... GREEN
[ ]  Rotate .... 60-70 MPH
[ ]  Climb .... 95 mph then 100 MPH Vy
[ ]  Gear / Flaps .... UP
[ ]  Max Crosswind .... 20 MPH (17kts)
[ ]  Alternator .... OFF, pull CB
[ ]  Non essential .... OFF, terminate flight ASAP
[ ]  Avionics master .... OFF
[ ]  Alternator CB .... IN
[ ]  Master .... OFF, then ON + check
[ ]  If still discharge, BATT .... ON
[ ]  If fire out: Master on if critical .... One essential equipment at a time
[ ]  Reset circuit breakers .... if critical
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