Piper PA-28-200R Arrow II — MikeOMalley_PA28R-200_CHECKLIST-EMERGENCY
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

ENGINE POWER LOSS INFLIGHT  [EMERGENCY]
[ ]  PITCH FOR 105
[ ]  FIND SUITABLE FIELD
[ ]  ATTEMPT RESTART
[ ]  Fuel selector .... Full tank
[ ]  Fuel Pump .... ON
[ ]  Mixture .... ADJUST (RICH)
[ ]  Alternate Air .... ON
[ ]  Engine Gauges .... CHECK
[ ]  Fuel Selector .... CHECK POSITION
WHEN POWER RESTORED
[ ]  Alternate air .... OFF
[ ]  Fuel pump .... OFF
IF POWER NOT RESTORED
[ ]  Ignition switch .... “R” then “L” then “Both”
[ ]  Throttle and Mixture .... Adjust
GO TO: IF POWER STILL NOT RESTORED PROCEDE TO POWER OFF LANDING CHECKLIST

POWER OFF LANDING  [EMERGENCY]
[ ]  GEAR DOWN
[ ]  SECURE ENGINE
[ ]  Mixture [MEMORY] .... IDLE CUTOFF
[ ]  Throttle [MEMORY] .... CLOSE
[ ]  Gear [MEMORY] .... DOWN
[ ]  Master .... OFF
[ ]  Ignition .... OFF
[ ]  Fuel selector .... OFF
[ ]  BRIEF PASSENGERS
[ ]  SEATS .... ADJUST FULL AFT
[ ]  SEATBELTS .... TIGHTEN
[ ]  DOOR .... PROP OPEN
[ ]  FLAPS .... AS REQUIRED
[ ]  TOUCHDOWN AT SLOWEST POSSIBLE SPEED

PROPELLER OVERSPEED  [EMERGENCY]
[ ]  THROTTLE .... RETARD
[ ]  OIL PRESSURE .... CHECK
[ ]  PROPELLER- FULL DECREASE RPM, THEN SET IF ANY CONTROL
[ ]  AIRSPEED- REDUCE
[ ]  THROTTLE- AS REQUIRED TO REMAIN BELOW 2700 RPM

EMERGENCY GEAR EXTENTION  [EMERGENCY]
[ ]  Master .... ON
[ ]  Breakers .... CHECK
[ ]  Panel lights .... OFF (IN DAYTIME)
[ ]  Gear indicator bulbs .... CHECK
[ ]  Airspeed- REDUCE BELOW 100
[ ]  Landing gear selector .... DOWN
[ ]  Engage Emergency Gear Leaver
IF GEAR STILL NOT DOWN
[ ]  Yaw aircraft sharply back and forth with rudder, and pitch aircraft up sharply

SPINS  [EMERGENCY]
[ ]  THROTTLE [MEMORY] .... IDLE
[ ]  RUDDER [MEMORY] .... FULL OPPOSITE DIRECTION OF ROTATION
[ ]  CONTROL WHEEL [MEMORY] .... FULL FORWARD
[ ]  RUDDER .... NEUTRAL (WHEN ROTATION STOPS)
[ ]  CONTROL WHEEL .... AS REQUIRED

FIRE  [EMERGENCY]
ON GROUND
DURING ENGINE START
[ ]  MIXTURE [MEMORY] .... IDLE CUTOFF
[ ]  THROTTLE .... OPEN
[ ]  STARTER .... CONTINUE CRANKING
AFTER ENGINE START
[ ]  CONTINUE OPERATING
[ ]  FUEL SELECTOR .... OFF
BEFORE EXTERNAL EXTINGUISHER APPLICATION
[ ]  MIXTURE .... IDLE CUTOFF
IN-FLIGHT
[ ]  SOURCE OF FIRE .... CHECK
ELECTRICAL FIRE
[ ]  Master Switch .... OFF
[ ]  Vents .... OPEN
[ ]  Cabin Heat .... OFF
[ ]  LAND AS SOON AS PRACTICABLE
ENGINE FIRE
[ ]  Fuel Selector .... OFF
[ ]  Throttle .... CLOSED
[ ]  Mixture .... IDLE CUTOFF
[ ]  Heater .... OFF
[ ]  Defroster .... OFF
[ ]  LAND IMMEDIATELY

LOSS OF OIL PRESSURE  [EMERGENCY]
[ ]  Oil Temp .... CHECK
[ ]  Power- reduce if possible
[ ]  LAND AS SOON AS PRACTICAL
[ ]  PREPARE FOR ENGINE FAILURE

LOSS OF FUEL PRESSURE  [EMERGENCY]
[ ]  Fuel Pump .... ON
[ ]  Mixture .... FULL RICH
[ ]  Fuel Selector .... CHECK
[ ]  LAND AS SOON AS PRACTICABLE

ENGINE ROUGHNESS  [EMERGENCY]
[ ]  Alternate Air .... ON
[ ]  Mixture .... ADJUST
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector .... SWITCH
[ ]  Engine Gauges .... CHECK
[ ]  Mags .... CHECK
[ ]  LAND AT NEAREST AIRPORT
[ ]  PREPARE FOR POWER OFF LANDING

ALTERNATOR FAILURE  [EMERGENCY]
[ ]  Electrical Load .... REDUCE
[ ]  Breakers .... CHECK
[ ]  “ALT” Switch .... CYCLE
NOTE: If alternator does not reset, reduce electrical load and land as soon as practicable. If battery is completely discharged, landing gear will not function normally, nor will position indicators, stall warning horn, or landing gear warning horn.
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