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Passenger Briefing
[ ]  Seat belts, Shoulder Harnesses
[ ]  Door Operation
[ ]  Emergency Exits
[ ]  Emergency Brace Position
[ ]  Fire Extinguisher
[ ]  Eating, drinking, smoking
[ ]  Control interference
[ ]  Collision avoidance
[ ]  Physiological considerations
[ ]  Conversation
[ ]  Supplemental information

Before Engine Start
[ ]  Door .... Closed and latched
[ ]  Seats .... Adjusted
[ ]  Seat belts and harnesses .... Fasten
[ ]  Fire extinguisher .... Secure
[ ]  Pitch trim .... Takeoff
[ ]  Flaps .... Retracted
[ ]  Rudder trim .... Neutral
[ ]  Prop .... Full forward
[ ]  Mixture .... Idle Cut-Off
[ ]  Alternate Air .... Off
[ ]  Alternate Static .... Off
[ ]  Fuel Selector .... Desired Tank
[ ]  Breakers .... Check
[ ]  Vent fan .... Off
[ ]  Pitot heat .... Off
[ ]  Avionics Master .... Off

Engine Start- Cold
[ ]  Beacon .... On
[ ]  Throttle .... Open ½ Inch
[ ]  Master .... On
[ ]  Fuel Pump .... On
[ ]  Mixture .... Full Rich until positive fuel flow indicated
[ ]  Mixture .... Idle cut-off
[ ]  Ignition .... Start
[ ]  Mixture .... FULL RICH when engine fires
[ ]  Throttle .... 800 RPM
[ ]  Oil Pressure and Temp .... Check
[ ]  Fuel pump .... Off

Engine Start- Hot
[ ]  Beacon .... On
[ ]  Throttle .... Open ½ Inch
[ ]  Master .... On
[ ]  Fuel Pump .... On
[ ]  Mixture .... Idle cut-off
[ ]  Ignition .... Start
[ ]  Mixture .... FULL RICH when engine fires
[ ]  Throttle .... 800 RPM
[ ]  Oil Pressure and Temp .... Check
[ ]  Fuel pump .... Off

Engine Start- Flooded
[ ]  Beacon .... On
[ ]  Throttle .... Full open
[ ]  Master .... On
[ ]  Fuel Pump .... On
[ ]  Mixture .... Idle cut-off
[ ]  Ignition .... Start
[ ]  Mixture .... FULL RICH when engine fires
[ ]  Throttle .... 800 RPM
[ ]  Oil Pressure and Temp .... Check
[ ]  Fuel pump .... Off

Warm Up
[ ]  Throttle .... 800-1200 RPM
[ ]  Annunciator Panel .... Test
[ ]  Flight Instruments .... Set and Check
[ ]  Avionics .... On and Set
[ ]  COMM .... Freq, Vol, Opr
[ ]  NAV .... Freq, Ident, Indicator, Accuracy, Course
[ ]  DME .... Freq, Ident
[ ]  ADF .... Freq, Ident
[ ]  MB .... Test, Sensitivity, Audio
[ ]  Transponder .... Test, Code
[ ]  LORAN .... Set

Taxi
[ ]  Taxi Area .... Clear
[ ]  Brakes and Steering .... Check
[ ]  Instruments .... Taxi Inst. Check
[ ]  Airspeed .... “Zero”
[ ]  Attitude .... Erect, Stable
[ ]  Altimeter .... Set, 75’ max
[ ]  VSI .... “Zero” noted
[ ]  DG .... Turning freely
[ ]  TC .... Proper Yaw, ball opposite
[ ]  Compass .... Fluid, turning freely
[ ]  ADF .... Tracking

Run-up
[ ]  Brakes .... Set
[ ]  Throttle .... 2000
[ ]  Engine Gauges .... Green
[ ]  Mags .... Check 175 max, 50 diff
[ ]  Vacuum .... 5 InHg ±0.1”
[ ]  Ammeter .... Check, load
[ ]  Alternate air .... Check
[ ]  Prop .... Cycle, then full forward

Take-off
[ ]  Fuel .... proper tank
[ ]  Fuel Pump .... On
[ ]  Engine Gauges .... Check
[ ]  Flight instruments .... Check and Set
[ ]  Master .... On
[ ]  Alternate Air .... Closed
[ ]  Mixture .... Set
[ ]  Prop .... Full forward
[ ]  Lights .... As required
[ ]  Transponder .... Alt
[ ]  Controls .... Free and Correct
[ ]  Seat backs .... Erect
[ ]  Seat belts, Harnesses .... Set
[ ]  Empty seats .... Secured
[ ]  Flaps .... Exercised and Set
[ ]  Trim .... Set
[ ]  Controls .... Free and Correct
[ ]  Door .... Latched
[ ]  Briefing
[ ]  Runway
[ ]  Crosswind
[ ]  Heading, altitude
[ ]  Emergency procedures
[ ]  Time .... Noted

Short Field
[ ]  Flaps .... 25°
[ ]  Rotate .... 60-65
[ ]  Vx .... 85
[ ]  Gear .... Up
[ ]  Vy .... 100
[ ]  Flaps .... Retract slowly

Climb
[ ]  Fuel Pump .... Off at 1000’ AGL
[ ]  Airspeed .... As required (110 MPH)

Cruise
[ ]  Lights .... As required
[ ]  Power .... As desired
[ ]  Mixture .... Lean

Descent
[ ]  Mixture .... Enrichen as required
[ ]  Airspeed .... As required
[ ]  Lights .... As required
[ ]  Weather
[ ]  Approach Briefing

Landing
[ ]  Seat backs .... erect
[ ]  Belts, harness .... fastened
[ ]  Fuel .... Proper tank
[ ]  Fuel pump .... On
[ ]  Mixture .... Set
[ ]  Propeller .... Set
[ ]  Gear .... DOWN (150 MPH)
[ ]  Flaps .... Set (125 MPH)

After Landing
[ ]  Transponder .... “STBY”
[ ]  Pitot Heat .... Off
[ ]  Alternate Air .... Off
[ ]  Flaps .... Retract
[ ]  Fuel Pump .... Off
[ ]  Lights .... As required

Shutdown
[ ]  Throttle .... Idle
[ ]  Avionics .... Off
[ ]  Mixture .... Idle Cut Off
[ ]  Electrical Switches .... Off
[ ]  Mags .... Off
[ ]  Master .... Off
[ ]  Trim .... Neutral
[ ]  Control Wheel .... Secure
[ ]  Tie-Downs .... Secure

NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
Source: Piper/PA-28-200R Arrow II/MikeOMalley_PA28R-200_CHECKLIST-NORMAL.txt
Rights: licensed
Checklist hash: 5da985ed7dc981efe12dcdd68d20c64d0d4b193af973af22e39ae4e035f3bdbd
Verify against the aircraft's own approved documentation before use.
