Piper PA-28-200R Arrow — John_Peck_N98JG_Piper_PA-28R_Emergency_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Emergency Landing Gear Extension" item count differs between passes (10 vs 11); verify nothing was dropped.

Emergency Landing Gear Extension  [EMERGENCY]
[ ]  Master Switch .... CHECK ON
[ ]  Landing Gear Actuator/Indicator Circuit Breakers .... CHECK IN
[ ]  Panel Lights (To prevent dimming gear indicators) .... OFF
[ ]  Gear Indicator Lights .... EXCHANGE BULBS
[ ]  Airspeed .... REDUCE BELOW 100 MPH
[ ]  Landing Gear Switch .... DOWN
IF GEAR FAILS TO LOCK DOWN, TRY THE FOLLOWING UNTIL GEAR LOCKS DOWN:
[ ]  Emergency Gear Lever .... OVERRIDE UP
[ ]  Emergency Gear Lever .... DOWN, FISHTAIL AIRPLANE
[ ]  Emergency Gear Lever .... HOLD UP, FISHTAIL AIRPLANE

Engine Failures  [EMERGENCY]
ENGINE FAILURE DURING FLIGHT
[ ]  Airspeed .... 105 MPH
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture .... RICH
[ ]  Fuel Tanks .... SWITCH
[ ]  Ignition Switch .... BOTH (OR START if propeller is stopped)

Fires — Engine Fire In Flight  [EMERGENCY]
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Master Switch .... OFF
[ ]  Cabin Heat and Air (except vents) .... OFF
[ ]  Airspeed (If fire is not extinguished, increase glide speed to find an airspeed which will provide an incombustible mixture) .... 105 MPH
[ ]  Forced Landing .... EXECUTE

Fires — Electrical Fire In Flight  [EMERGENCY]
[ ]  Master Switch .... OFF
[ ]  All Other Switches (except ignition switch) .... OFF
[ ]  Vents/Cabin Air/Heat .... CLOSED
[ ]  Fire Extinguisher .... ACTIVATE
WARNING: After discharging an extinguisher within a closed cabin, ventilate the cabin.

Fires — Cabin Fire  [EMERGENCY]
[ ]  Master Switch .... OFF
[ ]  Vents/Cabin Air/Heat (to avoid drafts) .... CLOSED
[ ]  Fire Extinguisher (if available) .... ACTIVATE
[ ]  Land the airplane as soon as possible to inspect for damage .... EXECUTE

Fires — Wing Fire  [EMERGENCY]
[ ]  Navigation Light Switch .... OFF
[ ]  Pitot Heat Switch .... OFF
[ ]  Wing Strobe Light Switch .... OFF
NOTE: Perform a side slip to keep flames away from the fuel tank and cabin, and land as soon as possible, using flaps only as required for final approach and touchdown.

Forced Landings — Emergency Landing Without Engine Power  [EMERGENCY]
[ ]  Airspeed .... 105 MPH
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Wing Flaps .... AS REQUIRED (40° recommended)
[ ]  Master Switch .... OFF
[ ]  Door .... UNLATCH PRIOR TO TOUCHDOWN
[ ]  Touchdown .... SLIGHTLY TAIL LOW
[ ]  Brakes .... APPLY HEAVILY
NOTE: For GEAR UP landing on soft ground or water, hold emergency gear lever in override up position and leave flaps retracted.
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