Piper PA-28-201R Arrow III — pa28r-201_chklist_landrum
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Cruise" item count differs between passes (15 vs 3); verify nothing was dropped.
content_gap: Section "Pre Start" item count differs between passes (24 vs 25); verify nothing was dropped.

Pre Start
[ ]  Seats and Belts .... ADJUST
[ ]  Passengers .... INSTRUCT
[ ]  Flaps .... UP
[ ]  Circuit Breakers .... CHECK
[ ]  Alternate Air .... OFF
[ ]  Parking Brake .... SET
[ ]  Prop .... HIGH RPM
[ ]  Gear .... DOWN
[ ]  Avionics .... OFF
[ ]  Master .... ON
[ ]  Gear Lights .... THREE GREEN
[ ]  Fuel Selector .... DESIRED TANK
[ ]  DAY Anti-collision Lts .... ON
[ ]  NIGHT Nav Lts .... ON
[ ]  Throttle .... ½ in OPEN
[ ]  Fuel Pump .... ON
[ ]  Mixture .... RICH THEN ICO
[ ]  Prop .... “CLEAR”
[ ]  Starter .... ENGAGE
[ ]  Mixture .... RICH
[ ]  Warmup .... 800-1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Radios .... ON
[ ]  Transponder .... STANDBY

Taxi
[ ]  Parking Brake .... OFF
[ ]  Strobes .... OFF FOR TAXI
[ ]  Taxi .... CHECK BRAKES
[ ]  Fuel Pumps .... OFF

Before Takeoff
[ ]  Parking Brake .... SET
[ ]  Propeller .... HIGH RPM
[ ]  Mixture .... RICH
[ ]  Throttle .... 2000
[ ]  Mags .... CHK (175 MAX, 50 Diff)
[ ]  Vacuum .... 4.8 – 5.1
[ ]  Oil Temp / Press .... CHECK
[ ]  Ammeter .... CHECK
[ ]  Annunciator Panel .... TEST
[ ]  Alternate Air .... CHECK
[ ]  Propeller .... EXERCISE
[ ]  Fuel Pump .... ON
[ ]  Fuel Pressure .... CHECK
[ ]  Throttle .... 1000
[ ]  Trim .... NEUTRAL

Takeoff
[ ]  Fuel Selector .... SET
[ ]  Fuel Pump .... ON
[ ]  Engine Guages .... CHECK
[ ]  Alt Air .... CLOSED
[ ]  Seat Backs .... ERECT
[ ]  Seatbelts .... FASTENED
[ ]  Mixture .... SET
[ ]  Propeller .... HIGH RPM
[ ]  Flaps .... SET
[ ]  Trim .... SET
[ ]  Controls .... FREE
[ ]  Instruments .... CHECK/SET
[ ]  Door .... LATCHED

Normal
[ ]  Flaps .... SET
[ ]  Trim .... SET
[ ]  Rotate .... 65 - 75
[ ]  Gear .... UP

After Takeoff
[ ]  Gear .... CHECK UP
[ ]  Flaps .... UP
[ ]  Climb .... 90
[ ]  Man. Pressure .... 25in
[ ]  Props .... 2500
[ ]  Fuel Pump .... OFF
[ ]  Engine Temp. .... CHECK

Cruise
[ ]  Man Pressure .... 23in
[ ]  Props .... 2300
[ ]  Mixture .... LEAN (10 gph)
V-SPEEDS
NOTE: Vso 55 KIAS
NOTE: Vs1 60 KIAS
NOTE: Vx 78 KIAS
NOTE: Vldmax 79 KIAS
NOTE: Vy 90 KIAS
NOTE: Vfe 103 KIAS
NOTE: Vlo 107 KIAS
NOTE: Vle 129 KIAS
NOTE: Va 118-96 KIAS
NOTE: Vno 146 KIAS
NOTE: Vne 183 KIAS

Descent
[ ]  Fuel Selector .... SET
[ ]  Seats/Belts .... ADJUST
[ ]  Fuel Pumps .... ON
[ ]  Mixture .... RICH
[ ]  Prop .... HIGH RPM
[ ]  Gear .... DOWN – 3GR
[ ]  Flaps .... SET
[ ]  Man Press .... 17-18 in
[ ]  Landing Light .... ON
NOTE: BCGUMPS

After Landing
[ ]  Flaps .... UP
[ ]  Trim .... NEUTRAL
[ ]  Landing Light .... OFF
[ ]  Taxi Light .... AS REQ
[ ]  Transponder .... OFF
[ ]  Mixture .... LEAN for TAXI
[ ]  Fuel Pump .... OFF

Shutdown
[ ]  Electrical Equip .... OFF
[ ]  Avionics .... OFF
[ ]  Prop .... HIGH RPM
[ ]  Throttle .... 1000 RPM
[ ]  Fuel Pump .... OFF
[ ]  Mixture .... IDLE CUTOFF
[ ]  Magneto .... OFF
[ ]  Master .... OFF
[ ]  Controls .... LOCKED

Initial
[ ]  Control Lock .... REMOVE
[ ]  Gear .... DOWN
[ ]  Master .... ON
[ ]  Gear Ind Lights .... CHECK
[ ]  Fuel Gauges .... CHECK
[ ]  Nav Lights .... CHECK
[ ]  Pitot Heat .... CHECK
[ ]  ELT .... CHECK
[ ]  Alternator Lt .... CHECK
[ ]  Cabin/Inst Lts .... CHECK
[ ]  Master .... OFF
[ ]  Static Drain .... DRAINED
[ ]  Trim .... NEUTRAL
[ ]  Storm Window .... OPEN
[ ]  Flaps .... FULL
[ ]  Windows .... CLEAN
[ ]  Papers .... ONBOARD
[ ]  Preflight .... PERFORM

HOT Start  [ABNORMAL]
[ ]  Seats and Belts .... ADJUST
[ ]  Passengers .... INSTRUCT
[ ]  Flaps .... UP
[ ]  Circuit Breakers .... CHECK
[ ]  Alternate Air .... OFF
[ ]  Parking Brake .... SET
[ ]  Prop .... HIGH RPM
[ ]  Gear .... DOWN
[ ]  Avionics .... OFF
[ ]  Master .... ON
[ ]  Gear Lights .... THREE GREEN
[ ]  Fuel Selector .... DESIRED TANK
[ ]  DAY Anti-collision Lts .... ON
[ ]  NIGHT Nav Lts .... ON
[ ]  Throttle .... ½ in
[ ]  Fuel Pump .... ON
[ ]  Mixture .... ICO
[ ]  Prop .... “CLEAR”
[ ]  Starter .... ENGAGE
[ ]  Mixture .... RICH
[ ]  Warmup .... 800-1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Radios .... ON
[ ]  Transponder .... STANDBY

Flooded Start  [ABNORMAL]
[ ]  Seats and Belts .... ADJUST
[ ]  Passengers .... INSTRUCT
[ ]  Flaps .... UP
[ ]  Circuit Breakers .... CHECK
[ ]  Alternate Air .... OFF
[ ]  Parking Brake .... SET
[ ]  Prop .... HIGH RPM
[ ]  Gear .... DOWN
[ ]  Avionics .... OFF
[ ]  Master .... ON
[ ]  Gear Lights .... THREE GREEN
[ ]  Fuel Selector .... DESIRED TANK
[ ]  DAY Anti-collision Lts .... ON
[ ]  NIGHT Nav Lts .... ON
[ ]  Throttle .... FULL OPEN
[ ]  Fuel Pump .... OFF
[ ]  Mixture .... ICO
[ ]  Prop .... “CLEAR”
[ ]  Starter .... ENGAGE
[ ]  Mixture .... RICH
[ ]  Warmup .... 800-1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Radios .... ON
[ ]  Transponder .... STANDBY

Engine Out Procedure  [EMERGENCY]
[ ]  Trim [MEMORY] .... 79 KIAS
[ ]  Locate Field (size, shape, surface, slope, surroundings) .... CHECK
[ ]  Turn .... TO FIELD
[ ]  Radio call .... MAKE
[ ]  Execute Power Off Landing .... EXECUTE

Engine Troubleshoot  [EMERGENCY]
[ ]  Fuel Flow .... CHECK
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector .... SET
[ ]  Alternate Air .... ON
[ ]  Engine Gauges .... CHECK
NOTE: If Engine Still Dead Continue

Securing Engine  [EMERGENCY]
[ ]  Fuel Pump .... OFF
[ ]  Selector .... OFF
[ ]  Mixture .... ICO
[ ]  Magnetos .... OFF
[ ]  Master .... OFF
[ ]  Door .... CRACK OPEN
[ ]  Belts .... TIGHT
[ ]  Min possible airspeed .... MAINTAIN

Landing Gear Emergency Extension  [EMERGENCY]
[ ]  Gear Selector .... DOWN
[ ]  Master .... ON
[ ]  Circuit Breaker .... CHECK IN
[ ]  Nav Lights .... CHECK OFF
[ ]  Gear Bulbs .... CHECK
[ ]  Airspeed .... < 87 KIAS
[ ]  Manual Extn .... ARM & PULL
[ ]  Yaw Aircraft to Drop Gear .... YAW
[ ]  Gear Indicators .... 3 GREEN

Gear Up Landing  [EMERGENCY]
[ ]  Flaps .... AS DESIRED
[ ]  Proceed with Securing Engine .... PROCEED

Electrical Fire  [EMERGENCY]
[ ]  Master Switch [MEMORY] .... OFF
[ ]  Air Vents .... OPEN
[ ]  Cabin Heat .... OFF
NOTE: Land As Soon As Practical

Loss of Oil Pressure  [EMERGENCY]
[ ]  Prepare for Engine Out Procedure .... PREPARE

Engine Fire (Ground)  [EMERGENCY]
[ ]  Starter .... CRANK
[ ]  Mixtures .... ICO
[ ]  Throttles .... FULL OPEN
[ ]  Fuel Selectors .... OFF
[ ]  Fuel Pumps .... OFF

Engine Fire (Flight)  [EMERGENCY]
[ ]  Fuel Selector [MEMORY] .... OFF
[ ]  Mixture [MEMORY] .... ICO
[ ]  Prop .... FULL FWD
[ ]  Fuel Pump .... OFF
[ ]  Magnetos .... OFF
[ ]  Alternator .... OFF
[ ]  Cabin Heat .... OFF
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