Piper PA-28-235 Cherokee — Eric_Duensing_pa28_235_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

BEFORE STARTING ENGINE
[ ]  Preflight inspection .... COMPLETE
[ ]  Seats, Seat Belts .... ADJUST AND LOCK
[ ]  Avionics Master .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Autopilot .... OFF
[ ]  Circuit Breakers .... CHECK IN
[ ]  Brakes .... TEST
[ ]  Fuel Selector Valve .... FULLEST TANK

STARTING ENGINE
[ ]  Carburetor heat .... OFF
[ ]  Throttle .... OPEN 1/4"
[ ]  Master Switch .... ON
[ ]  Electric Fuel Pump .... ON
[ ]  Primer .... AS REQUIRED
[ ]  Primer .... LOCKED
[ ]  Mixture .... FULL RICH
[ ]  Propeller Area .... CLEAR
[ ]  Depress Starter (release when engine starts)
[ ]  Throttle .... 800 RPM
[ ]  Oil pressure .... CHECK
[ ]  Electric Fuel Pump .... OFF
[ ]  Mixture .... LEAN FOR TAXI
[ ]  Avionics Master .... ON
[ ]  Fan, heater and defroster .... ON as required
[ ]  Navigation, Cockpit, and Taxi Lights .... ON as required
[ ]  Anti-collision lights .... ON
[ ]  Transponder .... TEST, then SDBY
[ ]  Altimeter .... SET to setting given by ATC
[ ]  Heading Indicator .... Set with magnetic compass
[ ]  Taxiing .... CHECK brakes immediately after airplane begins moving

DURING TURNS WHILE TAXIING
[ ]  Turn Coordinator .... Indicates skidding turn in proper direction
[ ]  Heading Indicator .... Turns in proper direction

BEFORE TAKEOFF
[ ]  Cabin Door .... CLOSED AND LATCHED
[ ]  Flight controls .... FREE AND CORRECT
[ ]  Fuel Selector Valve .... FULLEST TANK
[ ]  Flaps .... CHECK
[ ]  Flaps .... UP
[ ]  Elevator and Rudder Trim .... SET FOR TAKEOFF
[ ]  Mixture .... FULL RICH
[ ]  Parking Brake .... SET
[ ]  Throttle .... 1800 RPM
[ ]  Magnetos .... Check (max drop 175 RPM, max diff. 50 RPM)
[ ]  Carburetor Heat .... ON (check for RPM to drop about 100 RPM and stay down)
[ ]  Carburetor Heat .... OFF (check for RPM to return to 1700)
[ ]  Electric Fuel Pump .... ON (check fuel pressure)
[ ]  Ammeter .... CHECK
[ ]  Oil Pressure and Temperature .... Normal operating
[ ]  Suction Gauge .... 4.5" Hg
[ ]  Throttle .... 800 RPM
[ ]  Flight instruments .... SET
[ ]  Attitude Indicator .... Check, Set for level flight
[ ]  Heading Indicator .... Recheck heading
[ ]  Vertical Speed Indicator .... Note indication of 0 fpm climb
[ ]  Airspeed Indicator .... indicates 0
[ ]  Clock .... CHECK and SET
[ ]  Pitot Heat .... CHECK
[ ]  Communication Radio .... Tower or CTAF
[ ]  Navigation Radio .... SET if flying cross-country
[ ]  Autopilot .... OFF
[ ]  Transponder .... ALT
[ ]  Window .... CLOSED
[ ]  Parking Brake .... OFF

NORMAL TAKEOFF
[ ]  Flaps .... 0°
[ ]  Throttle .... FULL OPEN
[ ]  Airspeed Indicator .... Indicates increasing speed
[ ]  Elevator Control .... Rotate at 65 MPH
CLIMB SPEEDS
[ ]  Best angle (Vx) .... 90 MPH
[ ]  Best rate (Vy) .... 100 MPH
[ ]  Normal .... 115 MPH

SHORT FIELD TAKEOFF
[ ]  Flaps .... 25° (2nd notch)
[ ]  Brakes .... HOLD
[ ]  Throttle .... FULL OPEN
[ ]  Brakes .... RELEASE
[ ]  Elevator Control .... Rotate at 60 MPH
[ ]  Climb Speed .... 90 MPH until obstacles cleared, then as appropriate
[ ]  Flaps .... RETRACT after obstacles cleared

CRUISE
[ ]  Electric Fuel Pump .... OFF
[ ]  Elevator and Rudder Trim .... ADJUST
[ ]  Power .... Adjust to 75% per Power Setting Table
[ ]  Mixture .... lean to peak EGT minus 125 degrees

BEFORE LANDING
[ ]  Seats, Seat Belts, .... ADJUST AND LOCK
[ ]  Electric Fuel Pump .... ON
[ ]  Fuel Selector Valve .... FULLEST TANK
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON (IF ICING IS INDICATED)

NORMAL LANDING
[ ]  Wing Flaps .... BELOW 115 MPH
[ ]  Approach Speed .... 90 MPH

BALKED LANDING
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF
[ ]  Flaps .... RETRACT TO 25° IMMEDIATELY
[ ]  Airspeed .... 90 MPH
[ ]  Flaps .... RETRACT (after establishing a climb)

AFTER LEAVING RUNWAY
[ ]  Flaps .... RETRACT
[ ]  Carburetor Heat .... OFF
[ ]  Transponder .... SDBY
[ ]  Electric Fuel Pump .... OFF

SHUTDOWN
[ ]  Avionics Master .... OFF
[ ]  Electrical Equipment .... OFF (except anti-collision light)
[ ]  Throttle .... IDLE
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magneto Switch .... OFF (after propeller stops turning)
[ ]  Anti-collision lights .... OFF
[ ]  Master Switch .... OFF
[ ]  Vents .... CLOSED
[ ]  Control Wheel .... SECURED WITH SEAT BELT
[ ]  Tiedowns .... SECURED
[ ]  Flight Plan .... CLOSED

VUJ
[ ]  AWOS .... 128.175
[ ]  GROUND .... 121.75
[ ]  TOWER .... 126.275

FLAPS
[ ]  1ST .... 10 DEGREES
[ ]  2ND .... 25 DEGREES
[ ]  3RD .... 40 DEGREES
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