Piper PA-32RT-300T Lance — Jason_Helmka_PA32_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Preflight Inspection
CABIN
[ ]  Hobbs/Tach .... Check
[ ]  AROW .... Check
[ ]  Master Switch .... On
[ ]  Fuel .... Check Quantity
[ ]  Lights .... Check
[ ]  Flaps .... 10°
[ ]  Pitot Heat .... Test if IFR
[ ]  Master Switch .... Off
[ ]  Fuel Sump Lever .... Short push
RIGHT WING
[ ]  Flap, Aileron, Wing Tip .... Check
[ ]  Leading Edge .... Check
[ ]  Fuel Sump .... 1 Sample
[ ]  Fuel Level .... Check
[ ]  Tie Down .... Remove
[ ]  Landing Gear .... Check
[ ]  Fuel Sump .... 2 Sample
NOSE
[ ]  Windshield .... Clean
[ ]  Alternator Belt .... Check
[ ]  Prop & Spinner .... Check
[ ]  Nose Wheel & Gear .... Check
[ ]  Oil .... Check
[ ]  Air intake scoop .... Check
LEFT WING
[ ]  Leading Edge .... Check
[ ]  Landing Gear .... Check
[ ]  Fuel Sump .... 3 Sample
[ ]  Tie Down .... Remove
[ ]  Fuel Level .... Check
[ ]  Fuel Sump .... 4 Sample
[ ]  Pitot Tube .... Check
[ ]  Flap, Aileron, Wing Tip .... Check
EMPENNAGE
[ ]  Rear Door .... Secure
[ ]  Tie Down .... Remove
[ ]  Surfaces .... Check
[ ]  Controls .... Check
[ ]  Antennas .... Checks
[ ]  Lights .... Check

Starting Engine
[ ]  Seat Track/Back .... Lock
[ ]  Avionics .... Off
[ ]  Beacon .... On
[ ]  Brakes .... Set
[ ]  Throttle .... Crack open
[ ]  Prop .... Foward
[ ]  Master/ALT .... On
[ ]  Fuel Pump .... On
[ ]  Mixture .... Rich until 10 GPH flow then close
[ ]  Starter .... Engage
[ ]  Mixture .... Full rich when engine starts
[ ]  Throttle .... 700 RPM
[ ]  Oil Pressure .... Check
[ ]  Fuel Pump .... Off
[ ]  Fuel Pressure .... Check

Taxi
[ ]  Seat Belts/Harness .... On
[ ]  Flaps .... Up
[ ]  Avionics .... On
[ ]  Transponder .... 1200 or assigned
[ ]  ATIS .... Receive
[ ]  Altimeter .... Set

Engine Run-Up
[ ]  Brakes .... Set
[ ]  Fuel .... Fullest Tank
[ ]  Trim .... Neutral
[ ]  Flight Controls .... Free & Correct
[ ]  Annunciator Lights .... Check
[ ]  Instruments .... Set
[ ]  Mixture .... Full Rich
[ ]  Throttle .... 2000 RPM
[ ]  Mags .... Check L & R
[ ]  Prop .... Cycle
[ ]  Alternate air .... Check
[ ]  Vacuum .... Check
[ ]  Fuel Pressure .... Check
[ ]  Amps .... Check
[ ]  Oil Pressure .... Check
[ ]  Oil Temperature .... Check
[ ]  Throttle .... Idle

Pre-Takeoff
[ ]  Flaps .... 25°
[ ]  Mixture .... Best Power
[ ]  Fuel Pump .... On
[ ]  Pitot Heat .... As Req
[ ]  Doors/Windows .... Closed
[ ]  Door Seals .... Presurise
[ ]  Airconditioner .... Off
[ ]  Landing Light .... On
[ ]  Brakes .... Release

Takeoff
[ ]  Throttle .... Full
[ ]  Oil Pressure .... Check
[ ]  Rotate .... 70 KIAS
[ ]  Vy .... 87 KIAS
[ ]  Gear .... UP befor 106

Climb
[ ]  Airspeed .... 87 KIAS
[ ]  Flaps Up .... Reduce to 25
[ ]  Mixture .... 75% power
[ ]  Throttle .... 25"
[ ]  Prop .... 2500 RPM
[ ]  Fuel Pump .... Off
[ ]  Landing Lights .... Off
[ ]  CHT .... Below 350

Cruise
[ ]  Power .... 22" to 25"
[ ]  Prop .... 2400 to 2500 RPM
[ ]  Mixture .... 65% power
[ ]  Instruments .... Check
[ ]  Fuel .... Switch 30 mins

Descent
[ ]  Mixture .... Increase
[ ]  Fuel .... Fullest Tank
[ ]  ATIS .... Receive
[ ]  Instruments .... Set

Before Landing
[ ]  Landing Light .... On
[ ]  Seat Belts/Harness .... On
[ ]  Mixture .... Rich
[ ]  Prop .... Foward
[ ]  Fuel Pump .... On
[ ]  Fuel .... Fullest Tank
[ ]  Landing Gear .... Down

Normal Landing
[ ]  Flaps .... 25 to 40
[ ]  Airspeed .... 80 KIAS
[ ]  GUMP check .... On final
[ ]  Touch down .... 70 KIAS

Go Around
[ ]  Power .... Full
[ ]  Landing gear .... Positive rate UP
[ ]  Flaps .... 10 then positive rate UP

After Landing
[ ]  Flaps .... Up
[ ]  Fuel Pump .... Off
[ ]  Landing Light .... Off
[ ]  Pitot Heat .... Off
[ ]  Trim .... Neutral
[ ]  Door Seals .... Release

Shutdown
[ ]  Avionics .... Off
[ ]  Mixture .... Idle Cut-Off
[ ]  Mags .... Off
[ ]  Master/ALT .... Off
[ ]  Lights .... Off
[ ]  Hobbs/Tach .... Record
[ ]  Yoke .... Secure
[ ]  Tie Downs .... Secure

Emergency Procedures  [EMERGENCY]
ENGINE FAILURE DURING TAKEOFF
[ ]  Aircraft Control .... Maintain
[ ]  Airspeed .... 92 KIAS
[ ]  Fuel Selector .... Off
[ ]  Mixture .... Idle Cut-Off
[ ]  Fuel Pump .... Off
[ ]  Flaps .... Down
[ ]  Landing Gear .... Down
[ ]  Master .... Off
[ ]  Mags .... Off
[ ]  Door .... Unlatch
ENGINE FAILURE IN FLIGHT
[ ]  Airspeed .... 92 KIAS
[ ]  Landing Site .... Pick
[ ]  Fuel Selector .... Switch Tanks
[ ]  Fuel Pump .... On
[ ]  Mixture .... Rich
[ ]  Alternate Air .... Open
[ ]  Mags .... Check All
[ ]  Master .... On
NO TIME FOR RESTART
[ ]  Airspeed .... Maintain 92 KIAS
[ ]  Landing Site .... Pick
[ ]  Transponder .... 7700
[ ]  Radio .... 121.50 Declare Emergency
[ ]  ELT .... On
[ ]  Seatbelts/Harness .... On
[ ]  Flaps .... As Req
[ ]  Landing gear .... If terrain allows
[ ]  Mixture .... Idle Cut-Off
[ ]  Master .... Off
[ ]  Mags .... Off
[ ]  Door .... Unlatch
[ ]  Short Final .... 75 KIAS
[ ]  Body .... Protect

Electrical Fire In Flight  [EMERGENCY]
[ ]  All Elec Devices .... Off
[ ]  Master .... Off
[ ]  Vents, Cabin Heat & Air .... Off
[ ]  If Fire Out Master .... On Only If Critical
[ ]  Turn On One Ess Elec Device at a Time .... Check
[ ]  Reset Circuit Breakers .... Only If Critical

Landing Gear Failure  [EMERGENCY]
[ ]  Gear Selector .... Down
[ ]  Master Switch .... On
[ ]  Circuit Breakers .... Check
[ ]  Radio Lights .... Off
[ ]  Gear Indicator Bulbs .... Check
IF NOT DOWN
[ ]  Airspeed .... Below 87 KIAS
[ ]  Gear Selector .... Down
[ ]  Override Lever .... Engaged (While Fish tailing)
[ ]  Emergency Gear Lever .... Hold Down
NOTE: Hold lever down for at least 10 sec.

All Other Emergencies  [EMERGENCY]
NOTE: ALL OTHER EMERGENCIES REFER TO POH

V-Speeds
[ ]  Vr (Rotation Speed) .... 65 KIAS
[ ]  Vx (Best Angle) .... 87 KIAS
[ ]  Vy (Best Rate) .... 92 KIAS
[ ]  Va (Maneuvering Speed) .... 106-132 KIAS
[ ]  Vs (Stall Speed) .... 66 KIAS
[ ]  Vso (Stall- Full Flaps) .... 61 KIAS
[ ]  Vfe (Max Flaps Extended) .... 106 KIAS
[ ]  Vle (Max landing gear ext) .... 129 KIAS
[ ]  Vno (Max Normal Operating) .... 148 KIAS
[ ]  Vne (Never Exceed) .... 191 KIAS
[ ]  Vglide (Best Glide) .... 92 KIAS
[ ]  Max Crosswind .... 17 KIAS
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