Piper PA-34-200 Seneca — jochman-clseneca
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Engine Failure  [EMERGENCY]
[ ]  Minimum Control Speed .... 80 MPH
[ ]  Blue Line Speed .... 105 MPH
[ ]  Mixture, Prop, Throttle .... FORWARD
[ ]  Flaps & Gear .... RETRACT
[ ]  Electric Fuel Pumps .... ON
[ ]  Identify .... DEAD FOOT = DEAD ENGINE
[ ]  Verify .... RETARD THROTTLE
[ ]  Propeller of Dead Engine .... FEATHER
[ ]  Mixture of Dead Engine .... IDLE CUT OFF
[ ]  Trim .... AS REQUIRED
[ ]  Bank .... 5º TO GOOD ENGINE
[ ]  Fuel Pump of Dead Engine .... OFF
[ ]  Magnetos of Dead Engine .... OFF
[ ]  Cowl Flaps of Dead Engine .... CLOSE
[ ]  Cowl Flaps of Good Engine .... AS NEEDED
[ ]  Alternator of Dead Engine .... OFF
[ ]  Electrical Load .... REDUCE
[ ]  Fuel to Dead Engine .... OFF
[ ]  Fuel to Good Engine .... ON or CROSSFEED
[ ]  Fuel Pump of Good Engine .... OFF

Restart Engine  [EMERGENCY]
[ ]  Mixture .... AS REQUIRED
[ ]  Fuel Boost Pump .... ON
[ ]  Fuel Selector .... CROSSFEED
[ ]  Magnetos .... SELECT L or R ONLY
[ ]  Alternate Air .... ON

Unfeathering Procedure  [EMERGENCY]
[ ]  Fuel Selector Dead Engine .... ON
[ ]  Fuel Pump on Dead Engine .... OFF
[ ]  Throttle .... OPEN ¼ INCH
[ ]  Prop .... FORWARD
[ ]  Mixture .... RICH
[ ]  Magneto Switches .... ON
[ ]  Starter .... ENGAGE, PROP WINDMILLS
[ ]  Throttle .... RETARD, ENGINE WARM
IF ENGINE DOES NOT START
[ ]  Prime w/Fuel Pump .... 3 SECONDS
[ ]  Repeat Steps .... STEPS 6, 7, 8
[ ]  Alternator .... ON

Before Engine Start
[ ]  Seats .... ADJUSTED
[ ]  Seat Belts, Harness .... FASTENED
[ ]  Parking Brake .... SET
[ ]  Circuit Breakers .... IN
[ ]  Radios .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Alternate Air .... OFF
[ ]  Alternators .... ON

Starting Engines
[ ]  Mixture Controls .... IDLE CUT-OFF
[ ]  Throttle Controls .... OPEN ½ INCH
[ ]  Propeller Controls .... FORWARD
[ ]  Master Switch .... ON
[ ]  Magneto Switchs .... ON
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture Control .... RICH FOR 3 SEC.
[ ]  Propeller Area .... CLEAR
[ ]  Starter .... ENGAGE
[ ]  Mixture Control .... ADVANCE
[ ]  Oil Pressure .... CHECK
[ ]  Repeat Steps 8-11 for Other Engine .... AS REQUIRED
[ ]  Electric Fuel Pumps .... OFF

Hot Engine Start
[ ]  Mixture Controls .... IDLE CUT-OFF
[ ]  Throttle Controls .... OPEN ½ INCH
[ ]  Propeller Controls .... FORWARD
[ ]  Master Switch .... ON
[ ]  Magneto Switch .... ON
[ ]  Electric Fuel Pump .... OFF
[ ]  Propeller Area .... CLEAR
[ ]  Starter .... ENGAGE
[ ]  Mixture Control .... ADVANCE
[ ]  Oil Pressure .... CHECK
[ ]  Repeat Steps 7-10 for Other Engine .... AS REQUIRED

Flooded Engine Start
[ ]  Mixture Controls .... IDLE CUT-OFF
[ ]  Throttle Controls .... FULL FORWARD
[ ]  Propeller Controls .... FORWARD
[ ]  Master Switch .... ON
[ ]  Magneto Switch .... ON
[ ]  Electric Fuel Pump .... OFF
[ ]  Propeller Area .... CLEAR
[ ]  Starter .... ENGAGE
NOTE: When engine fires, retard throttle and advance mixture slowly.

Pre-Takeoff Check
[ ]  Parking Brake .... ON
ENGINE RUN-UP
[ ]  Mixture Controls .... FORWARD
[ ]  Propeller Controls .... FORWARD
[ ]  Throttle Controls .... 1500 RPM
[ ]  Propeller Controls .... CHECK FEATHER
[ ]  Throttle Controls .... 2000 RPM
[ ]  Propeller Governor .... CHECK
[ ]  Propeller Controls .... EXERCISE
[ ]  Propeller Controls .... FULL FORWARD
[ ]  Alternate Air Controls .... CHECK OFF/ON
[ ]  Engine Gauges .... GREEN
[ ]  Vacuum Gauge .... 4.5 to 5.2
[ ]  Magnetos .... CHECK
[ ]  Alternators .... CHECK
[ ]  Throttles .... 800-1000 RPM
[ ]  Fuel .... ON
[ ]  Alternators .... ON
[ ]  Altimeter .... SET
[ ]  Attitude Indicator .... SET
[ ]  Directional Gyro .... SET
[ ]  Clock .... WOUND & SET
[ ]  Mixtures .... SET

Pre-Takeoff Check - Continued
[ ]  Propellers .... FORWARD
[ ]  Friction Lock .... ADJUST
[ ]  Alternate Air .... OFF
[ ]  Cowl Flaps .... SET
[ ]  Seat Backs .... ERECT
[ ]  Wing Flaps .... SET
[ ]  Trim (Stabilator & Rudder) .... SET
[ ]  Seat Belts, Harnesses .... FASTENED
[ ]  Empty Seat Belts .... FASTENED
[ ]  Controls .... FREE & CORRECT
[ ]  Doors .... LATCHED
[ ]  Electric Fuel Pumps .... ON
[ ]  Pitot Heat .... AS REQUIRED
[ ]  Transponder .... ON
[ ]  Lights .... AS REQUIRED

Pre-Landing Check
[ ]  Seat Backs .... ERECT
[ ]  Seat Belts, Harnesses .... FASTENED
[ ]  Fuel Selectors .... ON
[ ]  Cowl Flaps .... AS REQUIRED
[ ]  Electric Fuel Pumps .... ON
[ ]  Mixture Controls .... RICH
[ ]  Propellers .... 2500 RPM
[ ]  Landing Gear .... DOWN
[ ]  Flaps .... AS REQUIRED

Post Landing Check
[ ]  Wing Flaps .... RETRACT
[ ]  Cowl Flaps .... OPEN
[ ]  Electric Fuel Pumps .... OFF

Shut Down
[ ]  Radios and Electric Equipment .... OFF
[ ]  Mixture Controls .... IDLE CUT-OFF
[ ]  Magneto Switches .... OFF
[ ]  Master Switch .... OFF
[ ]  Alternators .... OFF
[ ]  Parking Brake .... AS REQUIRED

Aircraft Performance Speeds
[ ]  VS0 – Landing configuration stall at gross weight, power off .... 69 MPH
[ ]  VS1 – Cruise configuration stall at gross weight, power off .... 76 MPH
[ ]  1.3 VS0 – Fence Speed .... 95 MPH
[ ]  1.5 VS0 – Approach Speed .... 105 MPH
[ ]  VX – Best Angle of Climb Speed .... 90 MPH
[ ]  VY – Best Rate of Climb Speed .... 105 MPH
[ ]  Normal Cruise .... 24 Hg 2400 RPM
[ ]  Slow Cruise .... 23 Hg 2300 RPM
[ ]  VFE – Max. Flap Extension .... 125 MPH
[ ]  VLE – Max. Gear Extension .... 150 MPH
[ ]  VLR – Max. Gear Retraction .... 125 MPH
[ ]  VA – Maneuvering Speed .... 133-146 MPH
[ ]  VNO – Top of Green Arc .... 190 MPH
[ ]  VNE – Red Line – Never Exceed .... 217 MPH
[ ]  VMC – Minimum Control Speed with Critical Engine Inoperative (Red Radial) .... 80 MPH
[ ]  VXSE – Best Angle of Climb Speed, One Engine Inoperative .... 90 MPH
[ ]  VYSE – Best Rate of Climb Speed, One Engine Inoperative .... 105 MPH
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