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Preflight Inspection
COCKPIT
[ ]  1. Control Lock .... REMOVE
[ ]  2. Ignition .... OFF
[ ]  3. Master Switch .... ON
[ ]  4. Fuel Gauges .... CHECK
[ ]  5. Alternator Warning Light .... CHECK
[ ]  6. Master Switch .... OFF
[ ]  7. Primary Flight Controls .... CHECK
[ ]  8. Flaps .... CHECK
[ ]  9. Static Drain .... DRAINED
[ ]  10. Windows .... CLEAN
[ ]  11. Baggage .... STOWED
[ ]  12. Required Papers .... ON BOARD
[ ]  13. Parking Brake .... ON
LEFT WING
[ ]  1. Surface Condition .... CHECK
[ ]  2. Flap and Hinges .... CHECK
[ ]  3. Aileron and hinges .... CHECK
[ ]  4. Wing Tip .... CHECK
[ ]  5. Lights .... CHECK
[ ]  6. Fuel Cap .... OPEN
[ ]  7. Fuel Quantity and Color .... CHECK
[ ]  8. Fuel Cap .... CLOSE and SECURE
[ ]  9. Fuel Vent .... CHECK
[ ]  10. Fuel Tank Sump .... DRAIN
[ ]  11. Pitot Head .... UNOBSTRUCTED
[ ]  12. Stall Warning .... CHECK
[ ]  13. Landing Gear and Tire .... CHECK
[ ]  14. Brake Block and Disk .... CHECK
[ ]  15. Chock and Tie Down .... REMOVED
NOSE SECTION
[ ]  1. Fuel Strainer .... DRAIN
[ ]  2. General Condition .... CHECK
[ ]  3. Prop and Spinner .... CHECK
[ ]  4. Air Inlets .... CLEAR
[ ]  5. Engine Compartment .... CHECK
[ ]  6. Oil .... CHECK QUANTITY
[ ]  7. Dipstick .... PROPERLY SEATED
[ ]  8. Alternator Belt .... CHECK TENSION
[ ]  9. Cowling .... CLOSED and SECURE
[ ]  10. Nose Gear Tire .... CHECK
[ ]  11. Nose Wheel Strut .... Proper Inflation (3")
[ ]  12. Windshield .... CLEAN
RIGHT WING
[ ]  1. Check as Left Wing .... CHECK
FUSELAGE (RIGHT SIDE)
[ ]  1. General Condition .... CHECK
[ ]  2. Antennas .... CHECK
[ ]  3. Side and Rear Window .... CHECK
[ ]  4. Static Vents .... UNOBSTRUCTED
EMPENNAGE
[ ]  1. General Condition .... CHECK
[ ]  2. Hinges and Attachments .... CHECK
[ ]  3. Tie Down .... REMOVED
FUSELAGE (RIGHT SIDE)
[ ]  1. Check as Left Side .... CHECK

Before Starting Engine
[ ]  1. Cabin Doors .... CLOSED AND LATCHED
[ ]  2. Overhead Latch .... ENGAGED
[ ]  3. Seats .... ADJUSTED AND LOCKED
[ ]  4. Seat Belts & Harnesses .... FASTENED
[ ]  5. Circuit Breakers .... IN
[ ]  6. Parking Brake .... SET
[ ]  7. Carburetor Heat .... FULL OFF
[ ]  8. Fuel Selector .... DESIRED TANK

Engine Start (COLD)
[ ]  1. Prime .... AS REQUIRED (LEAVE OUT)
[ ]  2. Throttle .... OPEN ½ INCH
[ ]  3. Master Switch .... ON
[ ]  4. Electric Fuel Pump .... ON
[ ]  5. Mixture .... FULL RICH
[ ]  6. Starter .... ENGAGE
[ ]  7. Primer .... PUSH IN SLOWLY
[ ]  8. Throttle .... ADVANCE SLIGHTLY
[ ]  9. Oil Pressure .... CHECK
[ ]  10. Electric Fuel Pump .... OFF
[ ]  11. Fuel Pressure .... CHECK
[ ]  12. Primer .... LOCKED

Engine Start (Hot)
[ ]  1. Throttle .... CRACKED
[ ]  2. Master Switch .... ON
[ ]  3. Electric Fuel Pump .... ON
[ ]  4. Mixture .... FULL RICH
[ ]  5. Starter .... ENGAGE
[ ]  6. Throttle .... ADJUST
[ ]  7. Oil Pressure .... CHECK
[ ]  8. Electric Fuel Pump .... OFF
[ ]  9. Fuel Pressure .... CHECK

Engine Start (Flooded)
[ ]  1. Throttle .... OPEN FULL
[ ]  2. Master Switch .... ON
[ ]  3. Electric Fuel Pump .... ON
[ ]  4. Mixture .... IDLE CUT-OFF
[ ]  5. Starter .... ENGAGE
[ ]  6. Mixture .... ADVANCE
[ ]  7. Throttle .... RETARD
[ ]  8. Oil Pressure .... CHECK
[ ]  9. Fuel Pressure .... CHECK

Starting Engine (External Power)
[ ]  1. Master Switch .... OFF
[ ]  2. All Electrical Equipment .... OFF
[ ]  3. Terminals .... CONNECT
[ ]  4. External Power Plug .... INSERT
[ ]  5. Proceed with Normal Start .... START
[ ]  6. Throttle .... LOWEST RPM
[ ]  7. External Power Plug .... DISCONNECT
[ ]  8. Master Switch .... ON – CHECK AMMETER
[ ]  9. Oil Pressure .... CHECK

Warm Up
[ ]  1. Throttle .... 800 to 1200 RPM

Taxiing
[ ]  1. Intercom .... ON
[ ]  2. Radios .... ON
[ ]  3. Taxi Area .... CLEAR
[ ]  4. Brakes .... CHECK
[ ]  5. Steering .... CHECK

Ground Check
[ ]  1. Brakes .... SET
[ ]  2. Throttle .... 1800 RPM
[ ]  3. Magnetos .... 175 Max/ 50 Diff.
[ ]  4. Vacuum .... 5.0" Hg ± .1
[ ]  5. Oil Temp .... CHECK
[ ]  6. Oil Pressure .... CHECK
[ ]  7. Carburetor Heat .... CHECK
[ ]  8. Throttle .... RETARD

Before Takeoff
[ ]  1. Master Switch .... CHECK ON
[ ]  2. Flight Instruments .... CHECK
[ ]  3. Fuel Selector .... PROPER TANK
[ ]  4. Mixture .... SET
[ ]  5. Electric Fuel Pump .... ON
[ ]  6. Carburetor Heat .... OFF
[ ]  7. Engine Gauges .... CHECK
[ ]  8. Static Source .... NORMAL
[ ]  9. Seats .... LATCHED IN TRACK
[ ]  10. Seat Backs .... ERECT
[ ]  11. Belts/Harness .... FASTENED
[ ]  12. Empty Seat Belt .... FASTENED
[ ]  13. Flaps .... SET
[ ]  14. Trim Tab .... SET
[ ]  15. Controls .... FREE
[ ]  16. Doors .... CLOSED and LATCHED
[ ]  17. Overhead Latch .... ENGAGED
[ ]  18. Transponder .... ON ALT

Normal Takeoff
[ ]  1. Flaps .... SET
[ ]  2. Trim Tab .... SET
[ ]  3. Accelerate .... 53 KIAS
[ ]  4. Control Wheel .... Back Pressure to Rotate to Climb Attitude

Short Field Takeoff, Obstacle Clearance
[ ]  1. Flaps .... 21° (first notch)
[ ]  2. Accelerate .... 53 KIAS
[ ]  3. Control Wheel .... Back Pressure to Rotate to Climb Attitude
[ ]  4. Accelerate (until over obstacle) .... 61 KIAS
[ ]  5. Accelerate (after over obstacle) .... 70 KIAS
[ ]  6. Flaps .... RETRACT SLOWLY

Short Field Takeoff, No Obstacle
[ ]  1. Flaps .... 21° (first notch)
[ ]  2. Accelerate .... 53 KIAS
[ ]  3. Control Wheel .... Back Pressure to Rotate to Climb Attitude
[ ]  4. Accelerate (after breaking ground) .... 70 KIAS
[ ]  5. Flaps .... RETRACT SLOWLY

Soft Field Takeoff, Obstacle Clearance
[ ]  1. Flaps .... 21° (first notch)
[ ]  2. Accelerate and lift off nose as soon as possible.
[ ]  3. Lift off at slowest possible airspeed.
[ ]  4. Accelerate just above ground .... 61 KIAS to climb past obstacle height
[ ]  5. Accelerate (after over obstacle) .... 70 KIAS
[ ]  6. Flaps .... RETRACT SLOWLY

Soft Field Takeoff, No Obstacle
[ ]  1. Flaps .... 21° (first notch)
[ ]  2. Accelerate and lift off nose as soon as possible.
[ ]  3. Lift off at slowest possible airspeed.
[ ]  4. Accelerate just above ground best rate of climb speed .... 70 KIAS
[ ]  5. Flaps .... RETRACT SLOWLY

Climb
[ ]  1. VX – Best Angle of Climb Speed .... 61 KIAS
[ ]  2. VY – Best Rate of Climb Speed .... 70 KIAS
[ ]  3. Electric Fuel Pump .... OFF

Cruising
[ ]  1. Normal Max. Power .... 75%
[ ]  2. Power .... SET PER TABLE
[ ]  3. Mixture .... ADJUST
[ ]  4. Fuel Selector .... SWITCH AS NEEDED

Approach and Landing
[ ]  1. Fuel Selector .... PROPER TANK
[ ]  2. Seat Backs .... ERECT
[ ]  3. Belts/Harness .... FASTEN
[ ]  4. Electric Fuel Pump .... ON
[ ]  5. Mixture .... SET
[ ]  6. Flaps .... SET (89 KIAS MAX)
[ ]  7. Trim .... 70 KIAS
[ ]  8. Final Approach Speed .... 67 KIAS

Stopping Engine
[ ]  1. Flaps .... RETRACT
[ ]  2. Electric Fuel Pump .... OFF
[ ]  3. Radios .... OFF
[ ]  4. Magnetos .... CHECK GROUND
[ ]  5. Throttle .... FULL AFT
[ ]  6. Mixture .... IDLE CUT-OFF
[ ]  7. Magnetos .... OFF
[ ]  8. Master Switch .... OFF
[ ]  9. Intercom .... OFF

Parking
[ ]  1. Parking Brake .... SET
[ ]  2. Control Wheel .... SECURED WITH BELTS
[ ]  3. Flaps .... FULL Up
[ ]  4. Wheel Chocks .... IN PLACE
[ ]  5. Tie Downs .... SECURE
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