Piper PA-44-180 Seminole — Ahmed_Nimer_Piper_44-180_simulator_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Taxi In And Engine Shut Down Checks" item count differs between passes (14 vs 16); verify nothing was dropped.

Warning
WARNING: THIS CHECK LIST IS FOR SIMULATION USE ONLY AND YOU CANT USE IT FOR REAL FLYING

Pre Start Checks
[ ]  Passneger Brief .... COMPLETED
[ ]  External Checks .... COMPLETED
[ ]  Door .... LATCH
[ ]  Belts, Shoulder Starps .... SECURE, CHECK
[ ]  Alternators .... ON
[ ]  Parking Brake .... ON
[ ]  Landing Gears .... DOWN
[ ]  Throttles .... CHECK/IDEL
[ ]  Propeller Controls .... CHECK/FULL FWD
[ ]  Mixtures .... CHECK/ICO
[ ]  Throttles Friction .... SET
[ ]  Carb Heat .... CHECK/OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Trimmers .... NEUTRAL
[ ]  Fuel Selector .... ON
[ ]  Electrics .... OFF
[ ]  Circuit Breakers .... ALL IN
NOTE: YOU CAN NOT START THE ENGINES IF YOU DID NOT COMPLETE ALL OF THE PRE START PROCEDURES.
PRE START CHECK LIST COMPLETED


Starting Engines Checks
[ ]  Battery Master Switch .... ON
[ ]  Anti Collision Lights .... FIN
[ ]  3 Greens .... CHECK
[ ]  Throttles .... 1/4 IN OPEN
[ ]  Propellers .... FULL
[ ]  Mixtures .... RICH
[ ]  Fuel Pumps .... ON
[ ]  Primer .... OPERATE
[ ]  Propeller Area .... CLEAR
[ ]  Magnetos .... ON
[ ]  Starter .... ENGAGE
[ ]  Throttles .... 1000 RPM
[ ]  OIL PRESSURE .... CHCHK
[ ]  Alternators .... CHECK
[ ]  Suction .... CHECK
[ ]  Fuel Pumps .... OFF
[ ]  Fuel Pressure .... CHECK
NOTE: Repeat items From 7-17 For Each Engine In Turn.
NOTE: YOU CAN NOT TAXI IF YOU DID NOT COMPLETE ALL OF THE ENGINE START PROCEDURES.
ENGINE START CHECK LIST COMPLETED

Before Taxi Checks
[ ]  Radio Master & Radio Nav .... ON
[ ]  Heater & Fan .... SET
[ ]  Radio /Nav Eq .... SET/CHECK
[ ]  Transponder .... TEST/STBY
[ ]  Gryo Compass .... CHECK
[ ]  Flight Instruments .... CHECK
[ ]  Lights .... AS REQUIRED
[ ]  Taxi Clearance .... OBTAIN
[ ]  Altimeter .... SET QNH
NOTE: YOU CAN NOT TAXI IF YOU DID NOT COMPLETE ALL OF THE BEFORE TAXI PROCEDURES.
BEFORE TAXI CHECK LIST COMPLETED

Taxi Checks
[ ]  Area .... CLEAR
[ ]  Parking Brakes .... OFF
[ ]  Brakes .... CHECK
[ ]  Instruments .... CHECK
[ ]  Fuel Selectors .... X-FEED/ON
NOTE: TAXI TO THE RUNWAY MAX SPEED 20KT
NOTE: YOU CAN NOT TAXI IF YOU DID NOT COMPLETE ALL OF THE TAXI CHECKS PROCEDURES.
TAXI CHECK LIST COMPLETED

Ground Run Up Checks
[ ]  Parking Brakes .... ON
[ ]  Mixtures .... RICH
[ ]  Propellers .... FULL FWD
[ ]  Engine Instruments .... CHECK
[ ]  Throttles .... 1500 RPM
[ ]  Propellers .... FEATHER CHECK (max drop 500)
[ ]  Throttles .... 2000 RPM
[ ]  Magnetos .... CHECK (max drop 175, max dif 50)
[ ]  Propellers .... EXERCISE (max drop 300)
[ ]  Carb Heat .... CHECK/OFF
[ ]  Engine Instruments .... CHECK
[ ]  Warning Lights .... OUT
[ ]  Alternators .... CHECK
[ ]  Suction .... CHECK (4.8to5.2 In Hg)
[ ]  Throttles .... IDEL/Check(500to600RPM)
[ ]  Throttles .... 1000 RPM
[ ]  Throttles Friction .... SET
NOTE: YOU CAN NOT TAKE OFF IF YOU DID NOT COMPLETE ALL OF THE GROUND RUN UP PROCEDURES.
GROUND RUN UP CHECKS COMPLETED.

Before T/OFF Checks
[ ]  Fuel Contents .... CHECK
[ ]  Fuel Pumps .... ON
[ ]  Fuel Selectors .... ON
[ ]  Mixtures .... RICH
[ ]  Engine Instruments .... CHECK
[ ]  Warning Lights .... CHECK/TEST
[ ]  Flight Instruments .... CHECK
[ ]  Flight Controls .... CHECK/FREE MOVMENT
[ ]  Trimmers .... SET FOR T/OFF
[ ]  Carb Heat .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Flaps .... CHECK/SET 1 NUTCH FOR T/OFF
[ ]  Landing Lights .... ON
[ ]  Navigation Lights .... ON
[ ]  Recognition Lights .... ON
[ ]  Transponder .... SET/ON
[ ]  Departure Clearance .... OBTAINED
[ ]  Rad Nav Eq .... SET FOR DEPARTURE
[ ]  Emergency Brief .... COMPLTETED
NOTE: When you Cleared Into runway
[ ]  Pitot heater .... AS REQUIRED
[ ]  Ventilation FAN .... OFF
NOTE: YOU CAN NOT TAKE OFF IF YOU DID NOT COMPLETE ALL OF THE BEFOR TAKE OFF PROCEDURES.
BEFORE TAKE OFF CHECKS COMPLETED.

Take Off Procedures Checks
[ ]  Throttles .... FULL
[ ]  Air Speed Indicator .... INCREASE
[ ]  Engine Instruments .... ALL IN GREEN
[ ]  Flight Instruments .... NORMAL INDECATION
[ ]  Air Speed 90KT .... ROTATE
[ ]  Brakes .... ON/OF
[ ]  Positive Rate Of Climb .... GEARS UP
NOTE: DO NOT TAKE OFF IF YOU DID NOT COMPLETE ALL OF THE TAKE OFF PROCEDURES.
TAKE OFF PROCEDURES COMPLETED.

After T/OFF And Climb Out Checks
[ ]  AT 500 AGL .... FLAPS UP
[ ]  AT 700 AGL .... POWER SET 45"MAP&24RPM
[ ]  Engine Instruments .... CHECK
[ ]  Landing Lights .... OFF
[ ]  Fuel Pumps .... OFF (at 1000AGL Or At TOC)
[ ]  Radio Nav Eq .... SET
[ ]  After 5000 FEET .... APPLY FULL POWER
NOTE: YOU MUST COMPLETE ALL OF THE CLIMB OUT CHECK BEFORE YOU REACH THE TOP OF CLIMB.
AFTER TAKE OFF AND CLIMB OUT CHECKS COMPLETED.

Cruise Checks
[ ]  Power .... SET
[ ]  Mixtures .... SET
[ ]  Fuel Pumps .... OFF
[ ]  Cowl Flaps .... CLOSED
[ ]  Engine Instruments .... CHECK/ALL IN GREEN
[ ]  Alternators .... CHECK
[ ]  Suction .... CHECK
[ ]  Flight Instruments .... CHECK
NOTE: YOU CANNT CONTINUE YOUR FLIGHT IF YOU DID NOT COMPLETE ALL OF THE CRUISE PROCEDURES.
CRUISE CHECKS COMPLETED

Descent Checks
[ ]  Fuel Contents .... CHECK
[ ]  Fuel Pumps .... ON
[ ]  Fuel Selectors .... ON
[ ]  Mixtures .... SET/RICH
[ ]  Engine Instruments .... NORMAL INDICATION
[ ]  Alternators .... CHECK
[ ]  Suction .... CHECK
[ ]  Flight Instruments .... CHECK/NORMAL
[ ]  Rad Nave Eq .... SET/CHECK
[ ]  Altimeter .... SET/CHECK
[ ]  Briefing .... COMPLETED
NOTE: If the OAT Above 10 C Open the Cowl Flaps
NOTE: YOU CAN NOT LAND IF YOU DID NOT COMPLETE ALL OF THE DESCENT PROCEDURES.
DESCENT CHECKS COMPLETED

Approach Checks
[ ]  Mixtures .... RICH
[ ]  Propeller .... SET
[ ]  Altimeter .... QNH/SET
[ ]  Transponder .... SET
[ ]  Landing Lights .... ON
[ ]  Cowl Flaps .... OPEN
NOTE: DO NOT LAND IF YOU DID NOT COMPLETE ALL OF THE APPROACH PROCEDURES.
APPROACH CHECKS COMPLETED.

Landing Checks
[ ]  Landing Gears .... Air speed WHITE ARC/DOWN
[ ]  3 Greens .... CHECK
[ ]  Flaps .... WHITE ARC/SET 2 NUTCH
[ ]  Mixtures .... RICH
[ ]  Propellers .... FULL
FINAL CHECKS
[ ]  Mixture .... RICH
[ ]  Propeller .... FULL
[ ]  3 Greens .... CHECK
[ ]  Landing Speed .... 75-80KT
[ ]  Touch Down .... MAINTAIN R/W CENTER LINE
[ ]  Breakes .... APPLY SLOWLY
APPROACH AND LANDING CHECKS COMPLETED

After Landing Checks
[ ]  Flaps .... UP
[ ]  Fuel Pumps .... OFF
[ ]  Carb Heart .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Lights .... AS REQUIRED
[ ]  Pitot Hearter .... OFF
[ ]  Radio NAV Eq .... OFF (except the one in use)
AFTER LANDING CHECKS COMPLETED.

Taxi In And Engine Shut Down Checks
[ ]  Taxi In Clearance .... OBTAINED
[ ]  Lights .... AS REQUIRE
ENGINE SHUTDOWN CHECKS
[ ]  Parking Breaks .... ON
[ ]  Lights .... AS REQUIRED
[ ]  Throttles .... IDEL
[ ]  Mixtures .... SET/IDEL
[ ]  RADIO&NAV Eq&GPS .... OFF
[ ]  Alternators .... OFF
[ ]  Magnetos .... OFF
[ ]  Battery Master Switch .... OFF
[ ]  Lights .... OFF
[ ]  All Switches .... OFF
ENGINE SHUT DOWN CHECKS COMPLETED.

Closing Warning
WARNING: DO NOT USE THIS CHECK LIST FOR REAL FLYING BECAUSE ITS FOR SIMULATOR ONLY.
NOTE: Made By: Ahmed Nimer Jordan.
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