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Takeoff
NORMAL TAKEOFF – FLAPS 0°
[ ]  Power 2000 RPM – Check Engine Gauges .... CHECK
[ ]  Rotate VR 75K – Takeoff VLOF 80K .... ROTATE
[ ]  Climb BLUELINE – 88K .... CLIMB
[ ]  No Runway – Positive Rate – GEAR UP .... GEAR UP
[ ]  500' AGL – 100K .... 100K
[ ]  1000' AGL – 24" / 2500 RPM – Takeoff Checklist .... TAKEOFF CHECKLIST
SHORT FIELD TAKEOFF – FLAPS 0°
[ ]  Hold Brakes .... HOLD
[ ]  Power 2000 RPM – Check Engine Gauges .... CHECK
[ ]  Release Brakes .... RELEASE
[ ]  Rotate VR 70K .... ROTATE
[ ]  Climb 75K to 50' .... CLIMB
[ ]  Climb BLUELINE – 88K .... CLIMB
[ ]  No Runway – Positive Rate – GEAR UP .... GEAR UP
[ ]  500' AGL – 100K .... 100K
[ ]  1000' AGL – 24" / 2500 RPM – Takeoff Checklist .... TAKEOFF CHECKLIST

Approach
NORMAL APPROACH (1 OR 2 ENGINE)
[ ]  Approach Checklist .... COMPLETE
[ ]  Downwind 100K (17") .... 100K
[ ]  GEAR DOWN / FLAPS 25° .... GEAR DOWN / FLAPS 25°
[ ]  Descend BLUELINE – 88K (15") .... DESCEND
[ ]  “GEAR DOWN – CHECKLIST” .... GEAR DOWN – CHECKLIST
[ ]  Base – “BLUELINE GUMP” .... BLUELINE GUMP
[ ]  400' AGL – “GEAR DOWN STABILIZED” .... GEAR DOWN STABILIZED
[ ]  Power Slow RETARD over RUNWAY END .... RETARD
[ ]  Touchdown 75K .... TOUCHDOWN
SHORT FIELD APPROACH
[ ]  Approach Checklist .... COMPLETE
[ ]  Downwind 100K (17") .... 100K
[ ]  GEAR DOWN / FLAPS 25° .... GEAR DOWN / FLAPS 25°
[ ]  Descend BLUELINE – 88K (15") .... DESCEND
[ ]  “GEAR DOWN – CHECKLIST” .... GEAR DOWN – CHECKLIST
[ ]  Base – “BLUELINE GUMP” .... BLUELINE GUMP
[ ]  600' AGL / FLAPS 40 / SPEED 75K .... FLAPS 40 / 75K
[ ]  400' AGL – “GEAR DOWN STABILIZED” .... GEAR DOWN STABILIZED
[ ]  Power Slow RETARD in FLARE .... RETARD
[ ]  Touchdown – FLAPS UP / MAXIMUM BRAKING .... TOUCHDOWN

Instrument Approaches
ILS APPROACH (1 OR 2 ENGINE)
[ ]  Approach Checklist .... COMPLETE
[ ]  100K to Intercept (17") .... 100K
[ ]  G/S Int. – GEAR DOWN / FLAPS 25° .... GEAR DOWN / FLAPS 25°
[ ]  G/S Intercept – “NO FLAGS” .... NO FLAGS
[ ]  G/S Descent – BLUELINE - 88K (2E - 15" / 1E - 20") .... BLUELINE 88K
[ ]  “GEAR DOWN – CHECKLIST” .... GEAR DOWN – CHECKLIST
[ ]  1000' AGL “BLUELINE GUMP” .... BLUELINE GUMP
[ ]  400' AGL “GEAR DOWN – STABILIZED” .... GEAR DOWN – STABILIZED
[ ]  100' ABOVE MINS “100 TO GO” .... 100 TO GO
[ ]  Power Slow RETARD over RUNWAY END .... RETARD
[ ]  Touchdown 75K .... TOUCHDOWN
NON-PRECISION APPROACH (1 OR 2 ENGINE)
[ ]  Approach Checklist .... COMPLETE
[ ]  100K Procedure Turn (17") .... 100K
[ ]  2E – 2Miles FAF GEAR DOWN / FLAPS 25° .... GEAR DOWN / FLAPS 25°
[ ]  1E – FAF GEAR DOWN / FLAPS 0° .... GEAR DOWN / FLAPS 0°
[ ]  FAF – “NO FLAGS” .... NO FLAGS
[ ]  FAF Descent – 88K (2E - 13" / 1E - 15") .... 88K
[ ]  “GEAR DOWN – CHECKLIST” .... GEAR DOWN – CHECKLIST
[ ]  1000' AGL “BLUELINE GUMP” .... BLUELINE GUMP
[ ]  100' ABOVE MINS “100 TO GO” .... 100 TO GO
[ ]  MDA – Level (2E - 20" / 1E – FULL) .... LEVEL
[ ]  1E - Leaving MDA – FLAPS 25° .... FLAPS 25°
[ ]  400' AGL “GEAR DOWN – STABILIZED” .... GEAR DOWN – STABILIZED
[ ]  Power Slow RETARD over RUNWAY END .... RETARD
[ ]  Touchdown 75K .... TOUCHDOWN
CIRCLE TO LAND (2 ENGINE ONLY)
[ ]  FAF – FLAPS 0° .... FLAPS 0°
[ ]  Turning Final, Leaving MDA – FLAPS 25° .... FLAPS 25°

Missed Approach
[ ]  Full Power – PITCH 88K .... FULL POWER / PITCH 88K
[ ]  Slow FLAPS 0° .... FLAPS 0°
[ ]  Positive Rate – GEAR UP .... GEAR UP
[ ]  500' AGL – 100K .... 100K
[ ]  1000' AGL - 24" / 2500 RPM – Takeoff Checklist .... TAKEOFF CHECKLIST
[ ]  HOLDING SPEED 100K .... 100K

Steep Turns
[ ]  SPEED 120K - 20" / 2300 RPM .... 120K
[ ]  50° BANK – POWER 23" - TRIM .... 23" / TRIM

VMC Demo
[ ]  Clearing Turns – 100K (17") .... 100K
[ ]  LEFT Throttle – IDLE .... IDLE
[ ]  RIGHT Throttle – FULL POWER .... FULL POWER
[ ]  5° BANK .... 5° BANK
[ ]  PITCH 1° / SEC – LIMIT RUDDER @ 77K .... PITCH 1°/SEC / LIMIT RUDDER
[ ]  LOSS OF DIRECTIONAL CONTROL or STALL WARNING .... RECOGNIZE
[ ]  PITCH DOWN – POWER TO IDLE .... PITCH DOWN / IDLE
[ ]  Slow POWER to FULL – 82K and then 88K .... FULL POWER / 82K / 88K

Stalls and Slow Flight
SLOW FLIGHT
[ ]  Clearing Turns – 100K (17") .... 100K
[ ]  GEAR DOWN / FLAPS 40° .... GEAR DOWN / FLAPS 40°
[ ]  GEAR DOWN Checklist .... COMPLETE
[ ]  LEVEL FLIGHT – 70K .... 70K
[ ]  CRUISE POWER .... SET
[ ]  FLAPS 0° / SPEED 82K .... FLAPS 0° / 82K
[ ]  Positive Rate – GEAR UP .... GEAR UP
[ ]  SPEED 88K .... 88K
STALL – POWER OFF
[ ]  Clearing Turns – 100K (17") .... 100K
[ ]  GEAR DOWN / FLAPS 40° .... GEAR DOWN / FLAPS 40°
[ ]  GEAR DOWN Checklist .... COMPLETE
[ ]  DESCENT – 80K .... 80K
[ ]  POWER to IDLE – Pitch to BUFFET .... IDLE / PITCH TO BUFFET
[ ]  PITCH DOWN – FULL POWER .... PITCH DOWN / FULL POWER
[ ]  FLAPS 0° / SPEED 82K .... FLAPS 0° / 82K
[ ]  Positive Rate – GEAR UP .... GEAR UP
[ ]  SPEED 88K .... 88K
STALL – POWER ON
[ ]  Clearing Turns – 100K (17") .... 100K
[ ]  POWER 13" / SPEED 80K .... 13" / 80K
[ ]  POWER 18" / Pitch to BUFFET .... 18" / PITCH TO BUFFET
[ ]  PITCH DOWN – FULL POWER .... PITCH DOWN / FULL POWER
[ ]  SPEED 82K .... 82K
[ ]  SPEED 88K .... 88K

Configuration Checklist
[ ]  Fuel Selectors – ON .... ON
[ ]  Cowl Flaps – OPEN .... OPEN
[ ]  Mixtures – RICH .... RICH
[ ]  Prop – HIGH .... HIGH
[ ]  Fuel Pumps - ON .... ON
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