Piper PA-46-350P Malibu Mirage — Pete_Sandhu_Piper_PA46-350P_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

1 BEFORE STARTING ENGINE
[ ]  Preflight .... COMPLETE
[ ]  Paper & Documents .... ABOARD
[ ]  Chocks & Tow bar .... REMOVED
[ ]  Seat & Seats Belts .... SECURE
[ ]  Window Shades .... OPEN
[ ]  Circuit Breakers .... CHECK IN
[ ]  Induction Air .... CHECK then PRIMARY
[ ]  Cabin Altitude Selector .... SET
[ ]  Altitude Rate Control .... 9 O'clock Position
[ ]  Landing Gear Selector .... DOWN
[ ]  Cabin Pressurization Control .... CAGED
[ ]  Cabin Pressure Dump Switch .... NORMAL
[ ]  Avionics Radio Master .... OFF
[ ]  Ice Protection Equipment .... OFF
[ ]  Propeller .... FULL INCREASE
[ ]  Fuel Selector .... Desired Tank for Takeoff
[ ]  Mixture .... IDLE CUTOFF
[ ]  Hobbs .... RECORD

2 STARTING ENGINE
[ ]  Brakes .... SET
[ ]  Emergency Fuel Pump .... OFF
[ ]  Check Area .... CLEAR
[ ]  Battery Master (ExternalPower = off) .... ON
[ ]  Alternators (ExternalPower = off) .... ON
[ ]  Magnetos .... ON
[ ]  wait for Engine Instruments
[ ]  Fuel Computer .... SET
[ ]  Throttle .... HALF
[ ]  Mixture .... RICH (4 secs) then IDLE CUTOFF
NOTE: (if engine is hot, no prime required)
[ ]  Starter .... ENGAGE
[ ]  Mixture
[ ]  Oil Pressure (within 30 sec) .... GREEN

3 BEFORE TAXIING
[ ]  Alternators .... CHECK
[ ]  Throttle .... 1000-1200
[ ]  Mixture .... Lean for Taxi
[ ]  Fuel Boost Pump .... on for High Elevations
[ ]  External Lights .... as REQUIRED
[ ]  Aux. Fuel Pump .... ON
[ ]  Avionics Radio Master .... ON
[ ]  EFIS .... ON
[ ]  Wing Flaps .... CHECK
[ ]  Spoiler .... CHECK
[ ]  Annunciator Panel .... TEST
[ ]  ATIS .... OBTAIN
[ ]  Altimeters (3) .... SET
[ ]  Heading Bug .... Set to Departure Runway
[ ]  Environmental System .... As Desired

4 TAXIING
[ ]  Brakes .... CHECK
[ ]  Turning Instruments .... CHECK

5 BEFORE TAKEOFF & RUN–UP
[ ]  Flight Plan .... ENTER
[ ]  Flight Instruments .... SET
[ ]  Doors .... CLOSED (4 GREEN)
[ ]  Seats .... ADJUSTED AND LOCKED
[ ]  Armrests &Table .... STOWED
[ ]  Pressurization .... SET
[ ]  Flight Controls .... CHECK
[ ]  Electric Trim .... TEST & SET
[ ]  Rudder Trim .... SET
[ ]  Flaps .... 10 degrees (Normal Takeoff)
[ ]  Minimum Oil Temp for Run–Up .... 100°F
ENGINE RUN–UP
[ ]  Mixture .... RICH
[ ]  Throttle .... 1700 RPM
[ ]  Magentos (ea.max 150, diff.max 50) .... CHECK
[ ]  Propeller .... CHECK
[ ]  Engine Instruments .... GREEN
[ ]  Vacuum System (4.5“ to 5.2“) .... GREEN
[ ]  Throttle .... 1200 RPM
[ ]  Alternators (2) .... CHECK
[ ]  De–Ice / Anti–Ice .... CHECK
[ ]  Throttle .... 1000 RPM
[ ]  Autopilot .... TEST & OFF
[ ]  Annunciator Panel .... CHECK
[ ]  Stall Warning Horn .... TEST
[ ]  Manifold & Static Line .... DRAIN

6 CLEARED FOR TAKEOFF
[ ]  Emergency Fuel Pump .... ON
[ ]  Lights .... SET
[ ]  Ice Protection .... SET
[ ]  Air Conditioning .... OFF

7 TAKEOFF
[ ]  Heading Bug
[ ]  Throttle .... Slowly Apply Full Power (3 secs)
[ ]  Rotate .... 80 KIAS
[ ]  Best Angle –Vx .... 90 KIAS
[ ]  Best Rate –Vy .... 110 KIAS
[ ]  Positive Rate of Climb .... GEAR UP
NOTE: (Check Annunciator for Warnings)
AT SAFE ALTITUDE
[ ]  Flaps .... RETRACT
[ ]  Fuel Pump .... OFF

8 CRUISE CLIMB
[ ]  Manifold Pressure .... 35“
[ ]  Propeller Control .... 2400 RPM
[ ]  Mixture Control .... 32 GPH
[ ]  Airspeed .... 125 KIAS
[ ]  Pressurization / Altimeter .... SET

9 CRUISE
[ ]  Mixture .... Lean to 1550 TIT
[ ]  High Speed .... 30”/2400 RPM
[ ]  Economy .... 25”/2000 RPM
[ ]  Fuel Imbalance .... Max 10 Gallons

10 DESCENT
[ ]  Power slowly reduce 15 min before arrival
[ ]  Mixture .... CRUISE SETTING
[ ]  Propeller Control .... CRUISE SETTING
[ ]  Pressurization / Altimeter .... SET

11 APPROACH & BEFORE LANDING
[ ]  Seat & Seats Belts .... SET
[ ]  Fuel Selector .... PROPER TANK
[ ]  Landing Gear down locked .... 3 GREEN
[ ]  Mixture .... RICH
[ ]  Propeller .... FULL
[ ]  Aux. Fuel Pump .... ON
[ ]  Pressurization .... CHECK
[ ]  Ice Protection .... CHECK
[ ]  Toe Brake .... PUMP & TEST then lower feet
[ ]  Induction Air .... PRIMARY
[ ]  Airspeed .... 85 KIAS

12 AFTER LANDING & PARKING
[ ]  Ice Protection .... OFF
[ ]  Flaps / Spoiler .... RETRACT
[ ]  EFIS & Avionics Radio Master .... OFF
[ ]  Engine cool down .... TIT STABLE
[ ]  Mixture .... IDLE CUTOFF
[ ]  Magentos / Alternators .... OFF
[ ]  Battery Master .... OFF
[ ]  HOBBS .... RECORD

1 LIMITATIONS & SPEEDS KIAS
[ ]  V1 (decision speed at half TODA) .... 55
[ ]  Vde-ice .... 183
[ ]  VA (light - heavy) .... 103 - 135
[ ]  Vglide .... 90
NOTE: Angle of Bank ⌠ Vs (Vso): 10°⌠70 (60)   30°⌠76 (66)   45°⌠82 (75)   60°⌠98 (86)
[ ]  Basic Empty Weight .... 2997lbs
[ ]  Max Takeoff Weight .... 4300lbs
[ ]  Zero Fuel Weight .... 4100lbs
[ ]  Max Landing Weight .... 4100lbs
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