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Before Starting Engine
[ ]  Preflight .... COMPLETE
[ ]  Paper & Documents .... ABOARD
[ ]  Control Locks & Tow bar .... REMOVED
[ ]  Seat & Seats Belts .... SET
[ ]  Circiut Breakers .... CHECK
[ ]  Induction / Alternate Air .... CHECK
[ ]  Landing Gear Selector .... DOWN
[ ]  Avionics Radio Master .... OFF
[ ]  Mixture, Prop, Throttle .... SET

Starting Engine
[ ]  Brakes .... SET
[ ]  Battery Master (ExternalPower = off) .... ON
[ ]  Alternators (ExternalPower = off) .... ON
[ ]  Magnetos .... ON
[ ]  Prime, Fuel Pump LH/RH check .... 6 SEC
[ ]  Starter .... ENGAGE
[ ]  Oil Pressure within 30 sec .... GREEN

Before Taxiing & Taxi Check
[ ]  Mixture .... SET
[ ]  Propeller .... SET
[ ]  Induction / Alternate Air .... PRIMARY
[ ]  Avionics Radio Master .... ON & SET
[ ]  Wing Flaps .... CHECK
[ ]  Spoiler .... CHECK
[ ]  Brakes .... CHECK
[ ]  Turning Instruments .... CHECK
[ ]  Annunciator Panel .... TEST

Before Takeoff & Run–Up
[ ]  Flight Instruments, Clocks .... SET
[ ]  Autopilot .... TEST & OFF
[ ]  Doors & Windows .... CLOSED
[ ]  Pressurization .... SET
[ ]  Flight Contorls .... CHECK
[ ]  Trim Tabs .... CHECK & SET
[ ]  Minimum Oil Temp for Run–Up .... 100°F
ENGINE RUN–UP
[ ]  Throttle .... 1700 RPM
[ ]  Magetos (ea.max 150, diff.max 50) .... CHECK
[ ]  Propeller .... CHECK
[ ]  Engine Instruments .... GREEN
[ ]  Vacuum System (4.5" to 5.2") .... GREEN
[ ]  Throttle .... 1200 RPM
[ ]  Alternators .... CHECK
[ ]  De–Ice / Anti–Ice .... CHECK
[ ]  Throttle .... 1000 RPM
[ ]  Manifold & Static Line .... DRAIN
[ ]  Aux. Fuel Pump .... AS REQUIRED
[ ]  Lights .... SET

Takeoff
[ ]  Fuel Selector .... PROPER TANK
[ ]  Flaps .... SET
[ ]  Ice Protection .... SET
[ ]  Gyro / Txpdr / Altimeter .... CHECK & SET
[ ]  Throttle .... FULL POWER
[ ]  Rotate .... 77 KIAS
[ ]  Best Angle – Vx .... 90 KIAS
[ ]  Best Rate – Vy .... 110 KIAS

Cruise Climb
[ ]  Manifold Pressure .... 34" – 35"
[ ]  Propeller Control .... 2400 RPM
[ ]  Mixture Control (35 UsGal/h) .... FULL RICH
[ ]  Airspeed .... 125 KIAS
[ ]  Aux. Fuel Pump .... LOW (IF REQ'D)
[ ]  Induction / Alternate Air .... SET
[ ]  Pressurization / Altimeter .... SET

Descent
[ ]  Mixture .... MIN. 1500°F TIT
[ ]  Propeller Control .... CRUISE SETTING
[ ]  Pressurization / Altimeter .... SET
[ ]  ATIS & Appr. Briefing .... CHECK
[ ]  Power .... AS REQ'D

Approach & Before Landing
[ ]  Fuel Selector .... PROPER TANK
[ ]  Seat & Seats Belts .... SET
[ ]  Aux. Fuel Pump .... AS REQUIRED
[ ]  Landing Gear down locked .... 3 GREEN
[ ]  Flaps / Spoiler .... AS REQUIRED
[ ]  Toe Brakes .... PUMP & TEST
[ ]  Induction / Alternate Air .... PRIMARY
[ ]  Airspeed .... 85 KIAS

After Landing & Parking
[ ]  Ice Protection & Txpdr .... OFF
[ ]  Flaps / Spoiler .... RETRACT
[ ]  Avionics Radio Master .... OFF
[ ]  Engine cool down .... 800°F TIT, CHT GREEN
[ ]  Engine (after 3-4min) .... SHUT DOWN
[ ]  Magentos / Alternators .... OFF
[ ]  Battery Master .... OFF
[ ]  Brake & Flight Control Lock .... SET

Limitations & Speeds (KIAS)
[ ]  Oil Temperatur min. for Take-Off .... 100°F
[ ]  Oil Temperatur max. allowable .... 240°F
[ ]  Oil Temperatur Cruise .... 170-200°F
[ ]  Cylinder Heat Temp in Flight .... MAX. 420°F
[ ]  Cylinder Heat Temp max. allowable .... 460°F
[ ]  T.I.T. in Flight .... MIN. 1500°F, MAX. 1750°F
[ ]  T.I.T. max. allowable for 30 sec. .... 1800°F
SPEEDS KIAS
[ ]  V1 (decision speed at half TODA) .... 55
[ ]  Vrot .... 77
[ ]  Vx .... 90
[ ]  Vy .... 110
[ ]  Vlgear up .... 130
[ ]  Vlgear down .... 170
[ ]  Vle .... 200
[ ]  Vflap down 10° .... 170
[ ]  Vde-ice .... 183
[ ]  VA max (4100lbs/1860kg) .... 135
[ ]  VA min (2450lbs/1110kg) .... 103
[ ]  Vglide .... 90
[ ]  norm.cruise TAS x 70% = if gear down cruise
[ ]  Vs (clean) .... 69
[ ]  Vso (landing) .... 58
ANGLE OF BANK (VS (VSO))
[ ]  10° .... 70 (60)
[ ]  30° .... 76 (66)
[ ]  45° .... 82 (75)
[ ]  60° .... 98 (86)
[ ]  BEW .... 1324kg (2918lbs)
[ ]  MTOW .... 1860kg (4100lbs)
[ ]  ZFW .... 1772kg (3900lbs)
[ ]  MLW .... 1772kg (3900lbs)
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