PZL 150A Koliber — Ariel_Batista_PZL_Koliber_150a_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Light Signals" item count differs between passes (10 vs 6); verify nothing was dropped.

Preflight Inspection
COCKPIT
[ ]  Canopy
[ ]  Aircraft docs (AROW)
[ ]  Weight & Balance
[ ]  Control wheel lock .... Remove
[ ]  Hobbs/Tach
[ ]  Magneto SW/Ignition .... Off
[ ]  Avionics Power Switch .... Off
[ ]  Master Switch .... On
[ ]  Fuel quantity indicators
[ ]  Flaps .... Extend
[ ]  Trimming tab .... “T-O” Position
[ ]  Fuel valve .... On fullest tank
[ ]  Stall warning
[ ]  Master Switch .... Off
LEFT WING
[ ]  Wing tie-down .... Disconnect
[ ]  Flaps
[ ]  Aileron
[ ]  Pitot tube
[ ]  Fuel tank vent open
[ ]  Slats
[ ]  Fuel Quantity
[ ]  Fuel Filler Plug
[ ]  Fuel tank sump .... Sample
[ ]  Main wheel tire
[ ]  Brakes
[ ]  Landing/Taxi Light(s)
NOSE
[ ]  Engine oil level
[ ]  Fuel strainer .... Sample
[ ]  Propeller and spinner
[ ]  Alternator belt
[ ]  Air intake
[ ]  Carburetor air filter
[ ]  Nose wheel strut & tire
RIGHT WING
[ ]  Wing tie-down .... Disconnect
[ ]  Aileron
[ ]  Flaps
[ ]  Fuel Quantity
[ ]  Fuel Filler Plug
[ ]  Fuel tank sump .... Sample
[ ]  Slats
[ ]  Main wheel tire
[ ]  Brakes
FUSELAGE AND EMPENAGE
[ ]  Rivets
[ ]  Rudder Cables Both sides
[ ]  Tail Tie-Down .... Disconnect
[ ]  Control surfaces
[ ]  Trim Tab
[ ]  Antennas

Before starting engine
[ ]  Preflight inspection
[ ]  Passenger Briefing
[ ]  Seats, belts .... Adjust & Lock
[ ]  Brakes
[ ]  Fuel Selector Valve .... Fullest Tank
[ ]  Avionics Power Switch .... Off
[ ]  Electrical Equip
[ ]  Circuit breakers

Starting Engine
[ ]  Mixture .... Rich (IN)
[ ]  Carburetor heat .... Cold (IN)
[ ]  Battery & Alternator SW .... On
[ ]  Fuel Pump .... On
[ ]  Anti-Collision light .... On
[ ]  Prime
[ ]  Throttle .... Open 1/4 inch
[ ]  Propeller area
[ ]  Starter .... Engage
[ ]  Engine .... 800-1000 rpm
[ ]  Oil Pressure

Before Taxi
[ ]  Avionics Master Switch .... On
[ ]  Fuel Pump .... Off
[ ]  Turn and Bank .... On
[ ]  Lights
[ ]  Radios .... Frequencies Set
[ ]  Brake
[ ]  Primer

Taxi
[ ]  Elevator .... Neutral or Aft.
[ ]  Flaps .... Up
[ ]  Flight & Engine Inst.

Engine Run-Up
[ ]  Parking brake .... Set
[ ]  Mixture .... Rich
[ ]  Throttle .... 1700 RPM
[ ]  Magnetos
[ ]  Carburetor Heat
[ ]  Engine Inst & Ammeter
[ ]  Fuel Pump
[ ]  Suction Gauge
[ ]  Throttle .... 800-1000

Before Takeoff
[ ]  Flight Controls
[ ]  Canopy .... Closed
[ ]  Emergency Trim S/W
[ ]  Electric Trim
[ ]  Flaps
[ ]  Encoder Switch .... On
[ ]  Transponder
[ ]  Avionics
[ ]  Lights

Takeoff Normal
[ ]  Flaps .... Up
[ ]  Throttle .... Full Open
[ ]  Rotate .... 45 – 50 Kts.
[ ]  Initial Climb .... 62 Kts.
[ ]  Passing 500 FT .... Fuel Pump Off

T/O Short & Soft
[ ]  Flaps .... Full
[ ]  Control Stick .... Full Back
[ ]  Throttle .... Full Open
[ ]  Control Stick .... Ease Forward
[ ]  Initial Climb .... 50-55 Kts.
[ ]  Passing 100 FT .... 61 Kts.
[ ]  Flaps .... Retract Slowly
[ ]  Passing 500 FT .... Fuel Pump Off

Climb
[ ]  Power .... Full Open
[ ]  Engine Temp
[ ]  Best Angle of Climb Vx
[ ]  Best Rate of Climb Vy
[ ]  Lights

Cruise
[ ]  Power
[ ]  Mixture .... Adjust
[ ]  Trim
[ ]  Fuel Tanks
NOTE: Switch tanks with Pumps on

Descent
[ ]  Power
[ ]  Mixture .... Rich
[ ]  Carb Heat

Before Landing
[ ]  Belts & Harnesses
[ ]  Flight instruments
[ ]  Radios
[ ]  ATIS
[ ]  Fuel Pump .... On
[ ]  Fuel Tanks
NOTE: Switch tanks with Pumps on
[ ]  Carb Heat .... On (Out)
[ ]  Mixture .... Rich
[ ]  Landing light .... On
[ ]  Airspeed .... 65-75 KIAS (Flaps Up)
NOTE: 60-70 KIAS (Flaps Dn)

After landing
[ ]  Flaps .... Up
[ ]  Carb Heat .... Cold (In)
[ ]  Transponder .... Standby
[ ]  Landing light .... Off

Parking
[ ]  Avionics .... Off
[ ]  Electrical .... Off
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... Cut-off
[ ]  Ignition switch .... Off
[ ]  Master switch .... Off

Securing the aircraft
[ ]  Control Lock .... Install
[ ]  Hobbs/Tach
[ ]  Canopy
[ ]  Tie-downs

Go-around
[ ]  Throttle .... Full
[ ]  Carb Heat .... Cold (In)
[ ]  Flaps .... 20(
[ ]  Climb .... 55 KIAS
[ ]  Flaps .... 10(
[ ]  Climb .... 60 KIAS
[ ]  Flaps .... Up
[ ]  Climb .... 79 KIAS

Engine failure
TAKEOFF
[ ]  Throttle .... Idle
[ ]  Brakes .... Apply
[ ]  Flaps .... Retract
[ ]  Mixture .... IDLE cut-off
[ ]  Ignition .... Off
[ ]  Master switch .... Off

Engine failure
AFTER TAKEOFF
[ ]  Airspeed .... 65 KIAS (flaps UP)
NOTE: 60 KIAS (flaps DN)
[ ]  Mixture .... Idle Cut-off
[ ]  Fuel shutoff valve .... Off (Out)
[ ]  Ignition .... Off
[ ]  Flaps
[ ]  Master switch .... Off
[ ]  Cabin Doors .... Unlatch
[ ]  Land .... Straight Ahead

Engine failure
DURING FLIGHT
[ ]  Airspeed .... 65 KIAS
LOOK FOR A FIELD
[ ]  Fuel shutoff valve .... On (In)
[ ]  Fuel selector valve .... Both
[ ]  Aux Fuel Pump Switch .... On
[ ]  Primer .... In & Locked
[ ]  Mixture .... Rich
[ ]  Ignition .... BOTH (or START)
[ ]  Airspeed .... 65 KIAS (flaps UP)
NOTE: 60 KIAS (flaps DN)
[ ]  Mixture .... Idle Cut-off
[ ]  Fuel shutoff valve .... Off (Out)
[ ]  Ignition .... Off
[ ]  Flaps
[ ]  Mayday .... Transmit 121.5
[ ]  Mayday .... Squawk 7700
[ ]  Master switch .... Off
[ ]  Touchdown .... Tail Low

Carburetor Icing  [ABNORMAL]
[ ]  Throttle .... Full
[ ]  Carb Heat .... On (Out)
[ ]  Mixture .... Adjust

Engine Roughness  [ABNORMAL]
[ ]  Magnetos
[ ]  Mixture .... Lean as necessary

Engine Fire during start  [EMERGENCY]
[ ]  Crank
[ ]  Power .... 1700 RPM (2 min)
[ ]  Engine

Engine Fire during flight  [EMERGENCY]
[ ]  Mixture .... Idle Cut-off
[ ]  Fuel shutoff valve .... Off (Out)
[ ]  Master Switch .... Off
[ ]  Boost Pump .... Off
[ ]  Cabin Heat/Air .... Off
[ ]  Airspeed .... 100 KIAS

Electrical failure  [ABNORMAL]
[ ]  Load meter
[ ]  Alternator .... Off
REDUCE LOAD TO MINIMUM
[ ]  Breaker/alt
[ ]  Alternator .... On
IF STILL NO POWER:
[ ]  Alternator .... Off
REDUCE LOAD AND LAND

Electrical overload  [ABNORMAL]
[ ]  Master Switch .... Off
[ ]  Master Switch .... On
[ ]  Over-voltage light .... Off
WARNING: or TERMINATE flight ASAP

Spin Recovery  [EMERGENCY]
[ ]  Ailerons .... NEUTRAL
[ ]  Throttle .... IDLE
[ ]  Rudder .... Full opposite
[ ]  Control wheel .... Full forward
[ ]  Rudder control/wheel .... Neutral
[ ]  Pitch .... Level

Light Signals
[ ]  Steady Green — On Ground
[ ]  Steady Green — In Flight
[ ]  Flashing Green — On Ground
[ ]  Flashing Green — In Flight
[ ]  Steady Red — On Ground
[ ]  Steady Red — In Flight
[ ]  Flashing Red — On Ground
[ ]  Flashing Red — In Flight
[ ]  Flashing white — On Ground
[ ]  Red/Green alternating

Comm Freq
[ ]  ATIS
[ ]  Ground
[ ]  Tower
[ ]  Club
[ ]  Fuel

V-Speeds (KIAS)
[ ]  Rotate Vr
[ ]  Normal Climb Vclm
[ ]  Max angle Vx (Sea Level)
[ ]  Max angle Vx (10,000 ft)
[ ]  Climb rate Vy (Sea Level)
[ ]  Climb rate Vy (10,000 ft)
[ ]  Maneuver Va
[ ]  Flaps Vfe
[ ]  Normal max Vno
[ ]  Never exceed Vne
[ ]  Stall (clean) Vs
[ ]  Stall (land) Vso
[ ]  Final Approach Flaps
[ ]  Final Approach No flaps
[ ]  Best Glide
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