Robinson R22 — michael_smith_r22_preflight_checklist_ds
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Cowl Door / Engine Right Side
[ ]  Check maintenance records, check general condition - leaks, discolorization dents, chafing, nicks, corrosion or cracks.
[ ]  Verify Telatemps show no unexplained temperature increases during prior flight.
COWL DOOR
[ ]  Master switch .... On
[ ]  Oil pressure, alternator, governor lights, low fuel .... On
[ ]  Warning light test switches .... Push to test
[ ]  Fuel quantity
[ ]  Rotor brake .... Actuation normal
[ ]  Master switch .... Off
[ ]  Aux fuel tank quantity
[ ]  Fuel filler cap .... Tight
[ ]  Aux fuel tank .... No leaks
[ ]  Aux fuel drain .... Sample
[ ]  Gearbox oil .... Full, no leaks
[ ]  Gearbox Telatemp .... Normal
[ ]  Flex coupling .... No cracks, nuts tight
[ ]  Yoke flanges .... No cracks
[ ]  Sprag clutch .... No leaks
[ ]  Static source .... Clear
[ ]  Control rod ends .... Free without looseness
[ ]  Steel tube frame .... No cracks
[ ]  All fasteners .... Tight
[ ]  Tail rotor control .... No interference
[ ]  Cowl door .... Latched
ENGINE RIGHT SIDE
[ ]  Carb air ducts .... Secure
[ ]  Carb heat scoop .... Secure
[ ]  Engine sheet metal .... No cracks
[ ]  Electrical terminals .... Tight
[ ]  Fuel line .... No leaks
[ ]  Oil cooler door
[ ]  Oil lines .... No leaks or chafing
[ ]  Exhaust system .... No cracks
[ ]  Engine general condition
[ ]  V-belt condition
[ ]  V-belt slack
[ ]  Sprag clutch .... No leaks
[ ]  Upper bearing .... No leaks
[ ]  Telatemp – upper bearing .... Normal
[ ]  Lower sheave groove wear .... Smooth & uniform
[ ]  Flex coupling .... No cracks, nuts tight
[ ]  Yoke flanges .... No cracks
[ ]  Steel tube frame .... No cracks
[ ]  Tail rotor control .... No interference

Engine - Rear / Empennage / Tail Rotor / Tailcone
ENGINE - REAR
[ ]  Cooling fan nut .... Pin in line w/ marks
[ ]  Cooling fan .... No cracks
[ ]  Fan scroll .... No cracks
[ ]  Telatemps – lower bearing .... Normal
[ ]  Lower bearing .... No leaks
EMPENNAGE
[ ]  Tail surfaces .... No cracks
[ ]  Fasteners .... Tight
[ ]  Position light
TAIL ROTOR
[ ]  Gearbox Telatemp .... Normal
[ ]  Gearbox .... Oil full, no leaks
[ ]  Blades .... Clean & no damage/cracks
[ ]  Rod ends .... Free without looseness
[ ]  Pitch link jam nuts .... Tight
[ ]  Teeter bearings
[ ]  Teeter bearing bolt .... Does not rotate
[ ]  Control bellcrank .... Free without looseness
TAILCONE
[ ]  Rivets .... Tight
[ ]  Skins .... No cracks or dents
[ ]  Strobe light condition
[ ]  Antenna
[ ]  Attachment bolts .... Tight

Engine - Left Side / Fuel Tank (Main) / Main Rotor
ENGINE - LEFT SIDE
[ ]  Engine sheet metal .... No cracks
[ ]  Exhaust system .... No cracks
[ ]  Engine oil .... 4-6 qts
[ ]  Fuel lines .... No leaks
[ ]  Gascolator drain .... Sample
[ ]  Throttle linkage .... Operable
[ ]  Battery & relay .... Secure
[ ]  Alternator belt tension
[ ]  Steel tube frame .... No cracks
[ ]  Engine general condition
FUEL TANK (MAIN)
[ ]  Leakage .... None
[ ]  Quantity
[ ]  Filler cap .... Tight
[ ]  Drain .... Sample
MAIN ROTOR
CAUTION: CAUTION – Do not pull rotor blades down as damage may occur. To lower one blade, push opposite blade up.
[ ]  Blades .... Clean & no damage/cracks
[ ]  Pitch change boots .... No leakage
[ ]  Main hinge bolts .... Cotter pins installed
[ ]  All rod ends .... Free without looseness
[ ]  Pitch link jam nuts .... Tight
[ ]  Pitch link safety wire .... Secure
[ ]  All fasteners .... Tight
[ ]  Swashplate scissors .... No excessive looseness
[ ]  Turn rotors 90° and level

Fuselage Left Side / Nose Section / Fuselage Right Side / Cabin Interior
FUSELAGE LEFT SIDE
[ ]  Baggage compartment
[ ]  Removable controls .... Secure if installed
[ ]  Collective control .... Clear
[ ]  Seat Belt .... Check condition & fastened
[ ]  Door .... Unlocked & latched
[ ]  Door hinge safety pin .... Installed
[ ]  Landing gear
[ ]  Ground handling wheel .... Removed
[ ]  Position light
NOSE SECTION
[ ]  Pitot tube .... Clear
[ ]  Windshield condition & cleanliness
[ ]  Fresh air vent .... Clear
[ ]  Landing lights
FUSELAGE RIGHT SIDE
[ ]  Landing gear
[ ]  Ground handling wheel .... Removed
[ ]  Position light
[ ]  Door hinge safety pin .... Installed
[ ]  Baggage compartment
CABIN INTERIOR
[ ]  Loose articles .... Removed or stowed
[ ]  Seat belts
[ ]  Instruments, switches, & controls
CAUTION: CAUTION – Removable controls should be removed if person in left seat is not a rated helicopter pilot.
CAUTION: CAUTION – When flying solo, fill left baggage compartment to capacity before using right baggage compartment. Avoid placing objects in compartments that might injure occupants if seat collapses during hard landing..
CAUTION: CAUTION – Shorter pilots may require cushion to obtain full travel of all controls. When using cushion, verify aft cyclic travel is not restricted.
NOTE: Notes: STAND BACK AND LOOK AT ENTIRE AREA!
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