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NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Approach Checklist" item count differs between passes (13 vs 15); verify nothing was dropped.
content_gap: Section "Landing Checklist" item count differs between passes (6 vs 16); verify nothing was dropped.

Pre-Start Checklist
[ ]  Parking Brakes .... SET
[ ]  Battery Switch .... OFF
[ ]  Alt Switch .... OFF
[ ]  Generator Switches .... OFF
[ ]  Throttle .... IDLE
[ ]  Landing Gear Lever .... CHECK DOWN
[ ]  Propeller .... HIGH RPM
[ ]  Fuel Cond. Lever .... FUEL CUTOFF (Ctrl-Shift-F1)
[ ]  Flaps .... UP
[ ]  Battery Switch .... ON
[ ]  Fuel Quantity .... CHECK
[ ]  Flight controls .... CHECK
[ ]  Check Weather .... (ATIS, Flight Services)
[ ]  De-Ice .... TEST/CHECK
[ ]  Request Clearance
[ ]  Transponder .... STANDBY
[ ]  Beacon .... ON

Startup Checklist
[ ]  Engine and Propeller Area .... CLEAR
[ ]  Throttle .... IDLE
[ ]  Fuel Flow .... ON (Ctrl-Shift-F4)
[ ]  Right Ignition and Engine Start Switch .... ON (hold until engine starts)
[ ]  Right ITT and Turbine PWR .... MONITOR
[ ]  Right Generator .... ON
[ ]  Left Ignition and Engine Start Switch .... ON (hold until engine starts)
[ ]  Left ITT and Turbine PWR .... MONITOR
[ ]  Left Generator .... ON
[ ]  Feather/Unfeather Props .... CHECK once
[ ]  Engine Instruments .... CHECK

Before Taxi Checklist
[ ]  Nav Lights .... ON
[ ]  Taxi Lights .... ON
[ ]  Heading Indicator/Altimeter .... SET
[ ]  Instruments .... NORMAL OPERATION
[ ]  Radios and Avionics .... CHECKED and SET
[ ]  Autopilot .... SET and OFF
[ ]  F/D .... ON
[ ]  Yaw Damper .... ON
[ ]  Request Taxi Clearance

Taxi Checklist
[ ]  Parking Brake .... RELEASE
[ ]  Brakes .... CHECK during taxi
[ ]  Directional Gyro .... PROPER IND. during turns
[ ]  Turn Coordinator .... PROPER IND. during turns
[ ]  Artificial Horizon .... ERECT during turns
[ ]  Taxi to assigned runway .... SPEED Max. 20 knots

Before Take-off Checklist
[ ]  Parking Brake .... SET
[ ]  Fuel Quantity .... CHECK
[ ]  Throttle .... IDLE
[ ]  Elevator Trim .... SET for takeoff
[ ]  Flaps .... Pos 1
[ ]  Flight Controls .... FREE AND CORRECT
[ ]  Engine/Flight Instruments .... CHECK
[ ]  Radios and Avionics .... SET
[ ]  Landing Lights .... ON
[ ]  Strobe Light .... ON
[ ]  Pitot Heat .... ON
[ ]  De-Ice .... AS REQUIRED
[ ]  Annunciator Lights .... CHECK
[ ]  Transponder .... ON
[ ]  Request Takeoff Clearance

Take-off Checklist
[ ]  Smoothly increase thrust to .... FULL
[ ]  Brakes .... RELEASE
[ ]  V1 = Vr = .... 110 KIAS
[ ]  Pitch .... 8-10 degrees
[ ]  V2 = .... 120 KIAS
[ ]  At Positive Climb Rate Touch Brakes
[ ]  Landing Gear .... RETRACT
[ ]  Flaps .... RETRACT
[ ]  Annunciator Lights/Eng. Instruments .... CHECK

Climb-out Checklist
[ ]  Autopilot .... CHECK and SET
[ ]  Taxi Lights .... OFF
[ ]  Landing Lights .... OFF
[ ]  Airspeed .... 205 KIAS / 1800 fpm 85%
[ ]  above 12,000 ft .... 200 KIAS / 1700 fpm 85%
[ ]  above 18,000 ft .... 180 KIAS / 1500 fpm 80%
[ ]  Engine Instruments .... MONITOR
[ ]  ATC .... AS REQUIRED
[ ]  At Transition Altitude (FL180) set Altimeter to .... 29,92" (1013mb)

Cruise Checklist
[ ]  Accelerate to cruise speed at 6,000 ft .... 240 KIAS 80%
[ ]  at 9,000 ft .... 240 KIAS 80%
[ ]  at 12,000 ft .... 230 KIAS 80%
[ ]  at 18,000 ft .... 220 KIAS 80%
[ ]  at 24,000 ft .... 220 KIAS 80%
[ ]  Service Ceiling .... FL310
[ ]  Engine+Instruments .... CHECK
[ ]  Fuel Quantity .... CHECK
[ ]  Radios .... TUNED and SET
[ ]  Autopilot .... CHECK and SET
[ ]  Lights .... AS REQUIRED

Descent Checklist
[ ]  Atis/Airport Information .... CHECK
[ ]  Altimeter .... CHECK
[ ]  Radios .... SET
[ ]  Descent Speed .... 240 KIAS 60%
[ ]  Descent Rate .... -1800 fpm
[ ]  Flaps / Landing Gear .... CHECK UP
[ ]  At Transition Altitude (FL180) reset Altimeter to local
[ ]  Check Weather .... (ATIS, Flight Services)

Approach Checklist
[ ]  Localizer Level Flight : Landing Lights .... ON
[ ]  Speed: Establish .... 180 KIAS 37%
[ ]  Flaps .... Pos 1
[ ]  Speed: Establish .... 160 KIAS 40%
[ ]  Flaps .... Pos 2
[ ]  Speed: Establish .... 140 KIAS 37%
[ ]  Landing Gear .... DOWN
[ ]  Turning toward runway: set flaps .... Pos 3 or FULL DOWN
[ ]  Final Glideslope Descent : Speed: Establish .... 130 KIAS 18%
[ ]  Descent Rate .... -xxx fpm
[ ]  Elevator Trim .... AS DESIRED
[ ]  Parking Brake .... VERIFY OFF
[ ]  De-Ice .... AS REQUIRED

Landing Checklist
[ ]  Landing Gear .... CHECK DOWN, 3 GREEN
[ ]  Autopilot .... OFF
[ ]  Landing Speed .... 120 KIAS
[ ]  Touchdown .... MAIN WHEELS FIRST
[ ]  Landing Roll .... LOWER NOSE WHEEL
[ ]  After touchdown Apply Reverse Thrust, at 60 kts: Cancel Reverse Thrust

Taxi To Ramp
[ ]  Strobe Light .... OFF
[ ]  Taxi Lights .... ON
[ ]  Landing Lights .... OFF
[ ]  Flaps .... RETRACT
[ ]  De-Ice .... OFF
[ ]  Transponder .... 1200
[ ]  Speed .... Max. 20 knots
[ ]  Elevator Trim .... TAKEOFF SETTING
[ ]  Avionics/Radios .... AS REQUIRED

Shutdown Checklist
[ ]  Parking Brake .... SET
[ ]  Throttle .... IDLE
[ ]  F/D .... OFF
[ ]  Taxi Lights .... OFF
[ ]  Pitot Heat .... OFF
[ ]  Nav Lights .... OFF
[ ]  Fuel Cond. Lever .... FUEL CUTOFF (Ctrl-Shift-F1)
[ ]  Beacon .... OFF
[ ]  Generators .... OFF
[ ]  Battery Switch .... OFF

Securing Aircraft
[ ]  Parking Brake .... Verify SET
[ ]  Throttle .... Verify IDLE
[ ]  All Switches .... Verify OFF
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