Saab 340 — MAX_Fs2ks340_Check
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

ENGINE STARTUP
[ ]  Park Brakes .... SET
[ ]  Battery switch .... ON
[ ]  Strobe and Beacon Lights .... ON
[ ]  Click on automatic startup engine button or CTRL+E .... PERFORM

AFTER ENGINE STARTUP
[ ]  Startup Engine Time .... LOGGED
[ ]  Engine power .... IDLE
[ ]  Low Idle .... CHECKED
[ ]  Fuel/Weight .... CHECKED AND LOGGED
[ ]  Avionic Master .... ON
[ ]  ATIS .... LOGGED
[ ]  Navaids .... SET
[ ]  AP Settings .... SET
[ ]  AP MAIN .... OFF
[ ]  Pitot Heat .... ON
[ ]  NAV Lights .... AS NEEDED

BEFORE TAKEOFF
[ ]  Flaps .... 7° (1ST POSITION)
[ ]  Prop RPM .... HIGH
[ ]  Trim position .... CHECKED
[ ]  AP MAIN and Flight Director .... ARMED
[ ]  Anti-Ice .... AS NEEDED
[ ]  Altimeters .... SET
[ ]  Landing Lights .... ON
[ ]  Transponder .... CODE SET

TAKEOFF AND CLIMB
[ ]  Thrust .... MAX POWER OR 95%
[ ]  Release Brakes
[ ]  Engine parameters .... CHECK
[ ]  Rotate at MTOW .... 115 KTS
[ ]  Pitch attitude after T/O .... 10°
[ ]  Retract landing gear with positive ROC
[ ]  At 500 ft and 130 kts IAS — Flaps .... UP
[ ]  Let accelerate to 160 kts IAS
[ ]  Reduce TORQUE .... 90-95%
[ ]  Engage AP with an initial ROC .... 2000 FPM
[ ]  Maintain until cruise altitude .... 160 KTS IAS AND 1500-2500 FPM ROC

CRUISE
[ ]  Reduce Prop RPM (ctrl-F2) .... 1650 RPM
[ ]  Reduce TORQUE .... 75-80%
NOTE: Usual cruise altitude is FL150-FL200
NOTE: Standard cruise speed is 280 kts TAS

DESCENT
[ ]  Establish a descent rate .... 1,500 FPM
[ ]  Maintain during descent .... 240 KTS IAS
[ ]  Landing Lights below 10,000 ft .... ON

APPROACH AND LANDING
[ ]  PROP RPM (ctrl-F4) .... HIGH
[ ]  Level approach flight (20-25 NM) clean configuration .... 210 KTS
[ ]  Glide slope alive — reduce speed and set Flaps 1 (7°) .... 170 KTS
[ ]  Passing the OM or 1500 ft — Gear Down, Flaps 3 (20°), Speed (Vref+5) .... 125 KTS
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