Schweizer SGS 2-33 — Eric_and_Ann_sgs_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

SGS 2-33 Flight Card
[ ]  Vne=98  Va=65
[ ]  W=51' L=30' H=10' ASP=18
[ ]  Slip=45-50
[ ]  G=20:1
[ ]  MPH
[ ]  Load limits -2.56<g<4.67
[ ]  Dual           0º
[ ]  Solo            0º
[ ]  45º      60º
[ ]  45º      60º
[ ]  L/D           50
[ ]  L/D            45       54
[ ]  60       70
[ ]  64
[ ]  M/Sink     42       50
[ ]  M/Sink      38       45
[ ]  60
[ ]  54
[ ]  Stall*        33
[ ]  Stall*         31       37
[ ]  39       47
[ ]  44
TAKEOFF
LAND
[ ]  Altimeter + radio .... SET
[ ]  Undercarriage .... CHECK
[ ]  Belts  + passenger brief .... BRIEFED
[ ]  Speed    50(47solo) + ½ w .... CHECK
[ ]  Control     trim off + Xwind .... CHECK
[ ]  Trim .... CHECK
[ ]  Cable .... CHECK
[ ]  Airbrakes .... CHECK
[ ]  Canopy .... CHECK
[ ]  Look out!    radio call .... PERFORM
[ ]  Dive Brakes .... CHECK
[ ]  Landing .... PERFORM
[ ]  I P-
[ ]  Direction of Wind .... CHECK
[ ]  1000'-800'
[ ]  Emergency Takeoff. forward to right .... PERFORM
[ ]  Abeam T P-     600'-500'
[ ]  200< forward to right .... PERFORM
[ ]  Base-
[ ]  200> 50mph 45ºbank .... PERFORM
[ ]  500'-400'
[ ]  180º turn to runway .... PERFORM
[ ]  Final-
[ ]  300'-200'
[ ]  Flair 5'-3'
[ ]  Vref 43 (41solo)
[ ]  Slack .... Yaw Away!
[ ]  Release rope .... Clear R & L  90ºR turn + check
[ ]  Stall* .... Test speed into and with wind
[ ]  Spin .... Neutral stick, top rudder, nose down
[ ]  Landing Stall .... Top rudder! Nose Down! Quickly!
[ ]  Speed to Fly     L/D + ½ HeadW        TailW   L/D
[ ]  ↔ M/S
WEIGHT  ARM  MOMENT
[ ]  SGS 2-33      612          x     96.12    58825
[ ]  F Pilot           _______   x     43.8    _________
[ ]  R Pilot          _______   x    74.7    _________
[ ]  Ballast          19.5 (op.)  x    14.7    286.65
[ ]  Total             _______   __________/W
[ ]  Max            1040lbs    CG 78.2↔86.1

Preflight
[ ]  N1178S
PREFLIGHT PREP:
[ ]  Open canopy pull tow hook release .... RELEASE
[ ]  Canopy Closed .... CHECK
[ ]  Remove Aileron locks .... REMOVE
[ ]  Lower Tail and retie .... LOWER/RETIE
[ ]  Remove rudder lock .... REMOVE
[ ]  Untie wing tips .... UNTIE
FRONT COCKPIT:
[ ]  Canopy - Condition & Secure .... CHECK
[ ]  ARROW .... CHECK
[ ]  Instruments and radio .... CHECK
[ ]  Controls - Free and correct .... CHECK
[ ]  Spoilers - check and leave open .... CHECK/OPEN
[ ]  Trim - operational .... CHECK
[ ]  Cables & Bolts - secure .... CHECK
[ ]  Belts and Harness .... CHECK
[ ]  Rudder Pedals - Adjust/check .... ADJUST/CHECK
[ ]  Ballast - Secure or remove .... SECURE/REMOVE
[ ]  Canopy Closed & Locked .... CLOSED/LOCKED
REAR COCKPIT + FUSELAGE INTERIOR:
[ ]  Canopy/Door - Condition .... CHECK
[ ]  Seat Cushions (Secure for solo) .... SECURE
[ ]  Belts & Harness .... CHECK
[ ]  Loose Equipment - Remove/Stow .... REMOVE/STOW
[ ]  Cables & Bolts .... CHECK
[ ]  Wing Connections .... CHECK
[ ]  Control Connections .... CHECK
[ ]  Cotter Pins - 6 .... CHECK
[ ]  Linkage .... CHECK
[ ]  Canopy Closed & Locked .... CLOSED/LOCKED
RIGHT WING:
[ ]  Struts & Bolts & Pins .... CHECK
[ ]  Leading Edge .... CHECK
[ ]  Wing Surface .... CHECK
[ ]  Outrigger Wheel .... CHECK
[ ]  Aileron .... CHECK
[ ]  Spoiler .... CHECK
[ ]  Trailing Edge .... CHECK
TAIL:
[ ]  Right Fuselage Skin .... CHECK
[ ]  Vertical Stabilizer .... CHECK
[ ]  Rudder and Hinge pins .... CHECK
[ ]  Horizontal Stabilizer .... CHECK
[ ]  Elevator and Hinge pins .... CHECK
[ ]  Control Cables/Push Rods .... CHECK
[ ]  Untie tail .... UNTIE
[ ]  Tail Fairing & Wheel .... CHECK
[ ]  Inspection Plates .... CHECK
[ ]  Left Fuselage Skin .... CHECK
LEFT WING:
[ ]  Left Wing: Repeat as per right wing in reverse 7-1 .... CHECK
NOSE SECTION:
[ ]  Pitot Static System .... CHECK
[ ]  Static Port - Clear .... CHECK
[ ]  Yaw String .... CHECK
[ ]  Tow hook release, skid, and wheel .... CHECK
[ ]  Fabric/Glass .... CHECK
WALK AROUND FINAL CHECK
[ ]  IMSAFE + Passenger Brief .... PERFORM
[ ]  Untie remaining ropes and move glider to holding area .... PERFORM
TOW PLANE/CREW:
[ ]  Instructions, Altitude & Direction .... BRIEFED
[ ]  Signals and Radio checks .... CHECK
[ ]  Check Tow Rope .... CHECK
RUNWAY:
[ ]  Traffic check and radio call .... PERFORM
[ ]  Position tow plane and glider for tow .... POSITION
[ ]  Tow release checks .... CHECK
[ ]  ABCs .... CHECK
NOTE: Use of this check list is solely at "Users risk". Authors assume no liability for any information thus contained.
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