Schweizer SGS 2-33A — Normal Procedures and Launch Emergencies
NOT FOR FLIGHT — source fidelity: not_applicable | operational review: none | completeness: partial | 1 unresolved safety defect(s)
safety_defect: No airspeeds or weight limits. Club and site procedures for signals, release points and pattern entry vary and override anything here.
content_gap: Aerotow only. No winch or auto-tow launch procedures, and no spin recovery section.

Daily and Preflight Inspection
[ ]  Canopy and latches .... CONDITION, SECURE
[ ]  Controls .... FREE, FULL TRAVEL, CORRECT SENSE
[ ]  Control connections and safeties .... CHECKED
[ ]  Spoilers .... OPERATE, LOCK CLOSED
[ ]  Tow release .... OPERATES AND RESETS
[ ]  Wings, fuselage, tail surfaces .... NO DAMAGE, FABRIC INTACT
[ ]  Tailwheel or skid, main wheel and tire .... CONDITION
[ ]  Pitot and static .... UNOBSTRUCTED
[ ]  Ballast and placards .... CORRECT FOR OCCUPANTS

Pre-Launch
[ ]  Straps .... TIGHT, ALL OCCUPANTS
[ ]  Instruments .... ALTIMETER SET, ZEROED AS REQUIRED
[ ]  Controls .... FREE, CORRECT
[ ]  Canopy .... CLOSED AND LOCKED
[ ]  Trim .... SET
[ ]  Spoilers .... CLOSED AND LOCKED
[ ]  Tow rope and weak link .... CORRECT, ATTACHED
[ ]  Wind and traffic .... CHECKED
[ ]  Launch emergency plan .... BRIEFED ALOUD
State the plan for a rope break below 200 feet, between 200 feet and pattern altitude, and above pattern altitude, and the landing option for each.
[ ]  Wing runner and tow pilot .... READY, SIGNAL GIVEN

Rope Break Below 200 Feet  [EMERGENCY]
Tow rope breaks or tow is released below approximately 200 feet AGL
WARNING: Do not attempt a turn back to the runway from low altitude. Land ahead, accepting whatever is in front of the glider.
[ ]  Nose [MEMORY] .... LOWER TO APPROACH ATTITUDE
[ ]  Tow release [MEMORY] .... PULL, TWICE
[ ]  Spoilers [MEMORY] .... AS REQUIRED
[ ]  Land straight ahead

Rope Break At or Above Pattern Altitude  [ABNORMAL]
Tow failure with sufficient height to fly a pattern
[ ]  Tow release [MEMORY] .... PULL, TWICE
[ ]  Airspeed .... ESTABLISH BEST GLIDE
[ ]  Landing area .... SELECTED
[ ]  Pattern .... FLOWN, ADJUSTED FOR HEIGHT
GO TO: Continue with the normal approach and landing checklist.

Approach and Landing
[ ]  Straps .... TIGHT
[ ]  Landing area .... CONFIRMED CLEAR
[ ]  Airspeed .... APPROACH SPEED SET FOR CONDITIONS
[ ]  Spoilers .... USED TO CONTROL GLIDE PATH
NOTE: Plan to land long rather than short. Undershooting is not recoverable in a glider.

After Landing
[ ]  Maintain wings level with aileron until the glider stops
[ ]  Spoilers .... OPEN
[ ]  Canopy .... AS REQUIRED
[ ]  Clear the runway and report clear
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