Yakovlev Yak-12M — YAK_12M_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

External
[ ]  Kick the tyres, nothing about to fall off etc.
[ ]  Oil level > 8 litres.
[ ]  Fuel levels OK.
[ ]  Turn engine 9 blades; watch for the oil.

Internal / starting
[ ]  All switches off, mags off etc.
[ ]  Fuel OK.
[ ]  Air on.
[ ]  Brakes on.
[ ]  Fuel on. .... ON
[ ]  Mixture rich. .... RICH
[ ]  Close oil cooler.
[ ]  Close carb heat.
[ ]  Open Gills.
[ ]  Flaps up.
FOR COLD START;
[ ]  If you have an assistant, 9 blades, 1 prime each.
[ ]  Otherwise, 8 primes, suck in, then 2 more.
FOR WARM START,
[ ]  1 prime per 10° below 100 cylinder head temp.
[ ]  Master switch on.
[ ]  Generator on.
[ ]  DC converter.
[ ]  Starter on.
[ ]  Set throttle.
[ ]  Press starter, when engine turns correct way, mags on both.
[ ]  When engine fires, set throttle and prime as necessary.
[ ]  Set 1000 RPM. .... 1000 RPM
[ ]  Close Gills until cylinder head temp rises, then open as necessary.
[ ]  Open oil cooler as necessary.

Before Taxi
[ ]  Switches on as necessay.
[ ]  Radio on and set.
[ ]  Set DI to compass
[ ]  Set altimeter.
[ ]  Uncage artificial horizon.
[ ]  Do not taxi until oil temp in green.

Taxi
NOTE: Note; tail wheel unlocked when stick forward.
[ ]  Check brakes and steering.
[ ]  Check pneumatic pressure maintained.
[ ]  Check turn and slip move correctly.
[ ]  Check DI moves correctly.

Engine checks
[ ]  Oil temp in green.
[ ]  Cylinder head temp in green.
[ ]  Set 2000 RPM .... 2000 RPM
[ ]  Check mags.
[ ]  Exercise prop.
[ ]  Check carb heat.
[ ]  Set idle; engine continues to run.
[ ]  Set 1000 RPM. .... 1000 RPM

Pre take off vital checks
[ ]  Mags on both.
[ ]  Trim set.
[ ]  Flaps to 15° .... 15°
[ ]  Fuel on and sufficient.
[ ]  Mixture fully rich.
[ ]  Starter covered.
[ ]  Primer locked.
[ ]  Prop fully fine.
[ ]  Oil temp green.
[ ]  Cylinder head temp green.
[ ]  Set DI to compass.
[ ]  Switches on as necessary.
[ ]  Controls full and free.
[ ]  Hatches and harness’ secure.

Take off
[ ]  Set full power, then back to 7.5 boost.
[ ]  Set prop to 2000 RPM. .... 2000 RPM
[ ]  Take off with tail up or 3 point.

Climb
[ ]  boost, 2000 RPM.
[ ]  Flaps up above 300 feet.

Cruise
[ ]  boost, 1860 RPM, no flaps.

Descent
[ ]  Reduce throttle.
[ ]  Flaps extend below 140kmh
[ ]  Final approach 110kmh, Prop to fine
NOTE: Note land with stick back to ensure tail wheel locked - risk of ground loops.

Close down
[ ]  Brakes on.
[ ]  Set 1000 RPM .... 1000 RPM
[ ]  Check mags.
[ ]  Flaps up.
[ ]  Close carb heat.
[ ]  Unnecessary electrics off.
[ ]  Set idle.
[ ]  Mags off.
[ ]  Open gill flaps.
[ ]  Electrics off.
[ ]  Close pneumatic valve.
[ ]  Stick free and brakes off for manoeuvring.
[ ]  Drain water trap
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