Yakovlev Yak 52 — yak52_yak52shortch
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

EXTERNAL
[ ]  Fuel quantity
[ ]  Oil Quantity, min 8 lts
[ ]  Prop alignment marks "0"
[ ]  Prop Area clear
[ ]  Cowl Shutters
[ ]  Fuselage FOD
[ ]  Oil Leaks
[ ]  Gear Struts
[ ]  Cowl Latches
[ ]  Pitot cover .... OFF
[ ]  Static Ports
[ ]  Flaps
[ ]  Drain Fuel
[ ]  Control Surfaces
[ ]  Ail Bearings
[ ]  Oil Cooler Cover
[ ]  Manifold drain tap .... shut
[ ]  Configure cockpits

REAR
[ ]  Mag Control UP (1st cabin)
[ ]  Gear .... NEUTRAL
[ ]  Flaps .... NEUTRAL
[ ]  Intsr. Switches .... DOWN
[ ]  Mags .... OFF
[ ]  Brake Override .... OFF
[ ]  Parachute Secured
[ ]  Straps Tied and Secure

FRONT
[ ]  Mags .... OFF (0)
[ ]  All Switches .... OFF
[ ]  Gear .... DOWN & Latched
[ ]  Brakes .... ON
[ ]  Main air supply .... ON
[ ]  Prime as required (cyls)
[ ]  Pull through blades as req.
WARNING: Do not touch the propeller if the engine is hot!
WARNING: TREAT PROP AS LIVE!
[ ]  Rear Mags .... 1+2
[ ]  Rear canopy .... CLOSED

STARTING
[ ]  Air supply Re-check
[ ]  Air supply .... ON
[ ]  Brakes re-check
[ ]  Brakes .... ON
[ ]  Master switch .... ON Generator ON
[ ]  Ignition .... ON Engine Instruments ON
[ ]  U/C switch .... ON
[ ]  Throttle .... SET
[ ]  Prop .... FINE
[ ]  Fire valve .... ON
[ ]  Enunciator lights .... TEST
[ ]  Carb heat .... OFF
[ ]  Shutters .... OPEN
[ ]  Prime LEFT Fuel pressure
[ ]  Prime right as req'd
[ ]  Check behind "Clear prop"
[ ]  Press starter
[ ]  Mags to BOTH (1+2)
[ ]  Prime as req'd then lock
WARNING: OIL PRESSURE!!!
[ ]  Warm up at .... 40-45%
[ ]  Cooling gills .... CLOSED Electrical systems ON

WARM UP
[ ]  Monitor temps and Pressures
[ ]  Set cooling controls as required
[ ]  Switch on and test avionics

POWER CHECKS
[ ]  Brakes .... ON
[ ]  Clear behind, T's & P's
[ ]  Shutters As required
[ ]  Power .... 70%
[ ]  Brakes holding
[ ]  Exercise Prop .... (54%)
[ ]  Mags .... (3% max drop)
[ ]  T's & P's .... CHECK
[ ]  *Ammeter Charging & 28v
[ ]  *Carb heat 1% RPM, + carb temp inc.
[ ]  Idle .... 28%
[ ]  Set .... 35%
NOTE: * (can do at 60%)

VITAL ACTIONS — WORK LEFT TO RIGHT
[ ]  Air .... ON
[ ]  Electric's .... ON
[ ]  Trimmer .... SET
[ ]  Flaps .... UP
[ ]  Prop .... FINE
[ ]  Fuel .... ON
[ ]  Lights .... PTT
[ ]  Mags .... 1+2
[ ]  Instruments .... Check
[ ]  Fuel Contents
[ ]  Primer .... Neutral
[ ]  Shutters .... Open & locked
[ ]  Carb heat .... Cold
[ ]  Controls .... Full Free
[ ]  Harnesses .... Secure
[ ]  Canopy As req.
[ ]  Strobes .... ON
[ ]  Transponder .... ON

TAKEOFF
[ ]  VR .... 100kph
[ ]  Climb .... 170 kph
[ ]  Gear .... UP
[ ]  Power to 82%, 80 cms or as req.
[ ]  T's & P's .... Check

BEFORE LANDING
[ ]  Power to 70% & 40 cms
[ ]  Abeam touchdown area
[ ]  200 kph GEAR .... DOWN, check lights and poles.
[ ]  170 kph Flaps
[ ]  Approach .... 150kph
[ ]  PUFA CHECK on finals

AFTER LANDING
[ ]  Taxi clear of r'way & STOP.
[ ]  Strobes & TX .... OFF
[ ]  FLAPS Identify and raise
[ ]  Shutters .... Open
[ ]  Converters .... OFF

SHUT DOWN
[ ]  Cool engine to 150 CHT
[ ]  Electric's .... OFF
[ ]  Mags .... OFF
[ ]  Air tap & shutters Close
[ ]  Water drain. Bleed
[ ]  Control locks. As req.
[ ]  Manifold drain .... OPEN

USE ONLY AS A GUIDELINE
NOTE: THIS IS NOT AN APPROVED CHECKLIST.
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