Bellanca 8GCBC Scout — Sam_Dawson_8gcbc_inflight_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Turn- Time-Twist-Tap-Throttle-Talk" item count differs between passes (4 vs 1); verify nothing was dropped.
content_gap: Section "Turn-Time-Twist-Throttle-Talk" item count differs between passes (4 vs 1); verify nothing was dropped.

Final Before Take Off Check
[ ]  1. Heading .... Check aligned w/ runway
[ ]  2. Altimeter .... Field elevation
[ ]  3. Transponder .... ON
[ ]  4. Time .... Noted
[ ]  5. Strobes, lights .... All on
[ ]  6. Landing & TO lights .... On when cleared for Takeoff

Climb Check
[ ]  1. Throttle .... FULL OPEN
[ ]  2. Mixture .... Lean
[ ]  3. Airspeed .... 70-85 MPH

Cruise
[ ]  1. Level Off .... TRIM
[ ]  2. Airspeed .... ACCELERATE
[ ]  3. Power .... SET to cruise
[ ]  4. Mixture .... LEAN when below 75%
[ ]  5. Taxi/Landing Lights .... Off

In Range-Descent
[ ]  1. ATIS/AWOS/ASOS .... Received
[ ]  2. Altimeter .... Set
[ ]  4. Seat Belts .... secured
[ ]  6. Mixture .... SET
[ ]  7. Landing Light/Taxi Light .... ON
[ ]  8. Avionics .... SET
[ ]  9. Approach Briefing .... Complete

Turn-Time-Twist-Throttle-Talk
NOTE: Vx-58, Vy-80, Cruise Climb- 75-80, Va-118
NOTE: Vref-70-75, Vref short- 60, Vfe- 101,
NOTE: Vfret- 60 (all speeds MPH)
NOTE: 14 July 2007 Blackhawk Aviation, El Paso, TX

Approach Brief
[ ]  Approach .... Type, Runway
[ ]  Frequency .... Set, ID
[ ]  Final Approach Course .... CDI Set
[ ]  FAF
[ ]  DH/MDA
[ ]  Approach Lights/PAPI/VASI .... Pilot activated?
[ ]  TDZE, HAT/HAA
[ ]  MAP
[ ]  Missed Approach
[ ]  Notes
[ ]  Runway exit/taxi plan
[ ]  Terrain
[ ]  Min. Alt., MAP & Climb Out .... Complete

Before Landing
[ ]  1. Seat Belts .... Fastened
[ ]  2. Mixture .... RICH
[ ]  3. Breaks .... CHECK FIRM
[ ]  4. Approach Speed .... 70-75 MPH

GO AROUND
[ ]  1. Throttle .... Full
[ ]  2. Carburetor Heat .... Cold
[ ]  3. Wing Flaps .... 20° Immediately
[ ]  4. Climb Speed .... 62 KIAS
[ ]  5. Wing Flaps .... 10° (until obstacles clear), RETRACT (safe altitude & 60 KIAS)

After Landing
[ ]  1. Transponder .... Stby
[ ]  3. Strobes/lights .... Off as necessary
[ ]  4. Electric Fuel Pump .... OFF
[ ]  5. Taxi Clearance .... Obtain

Turn- Time-Twist-Tap-Throttle-Talk
NOTE: Vx-58, Vy-80, Cruise Climb- 75-80, Va- 118,
NOTE: Vref-70-75, Vref short- 60, Vfe-101, Vfret-
NOTE: 60 (all speeds MPH)
NOTE: 14 July 2007  Blackhawk Aviation, El Paso, Texas
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