Bellanca 8KCAB Decathlon — Sam_Dawson_8kcab_ground_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Shutdown and Securing" item count differs between passes (14 vs 13); verify nothing was dropped.
content_gap: Section "Starting Engine" item count differs between passes (10 vs 13); verify nothing was dropped.
content_gap: Section "Taxi" item count differs between passes (3 vs 2); verify nothing was dropped.

Before Starting Engine
[ ]  Preflight Inspection .... Complete
[ ]  CRM/Passenger Briefing .... Complete
[ ]  Seats and Seat Belts .... Adjust & Lock
[ ]  Fuel Shut-Off Valve .... ON
[ ]  Brakes .... Set
[ ]  Alternate Air .... COLD
[ ]  Electrical and Radio Switches .... OFF
[ ]  Propeller Control .... FULL INCREASE
[ ]  Circuit Breakers .... Check In

Starting Engine
[ ]  Master Switch .... On
[ ]  Engine Prime (as Required) .... Mixture- RICH / Throttle- ¼-½” / Fuel Pump- ON until fuel pressure; then OFF
[ ]  Mixture .... IDLE CUT OFF
[ ]  Throttle .... ½-1” Open
[ ]  Magneto Switches .... BOTH
[ ]  Propeller Area .... CLEAR
[ ]  Starter .... ENGAGE
[ ]  Mixture .... FULL RICH
[ ]  Throttle .... 1000-2000 RPM
[ ]  Oil Pressure .... CHECK

Before Taxi
[ ]  Mixture .... Lean for taxi
[ ]  Throttle .... 1000 RPM
[ ]  Electrical and Radio Switches .... On as needed
[ ]  ATIS / AWOS .... Receive
[ ]  Clearance .... Obtain
[ ]  Avionics / Transponder .... Set / STBY
[ ]  Flight Instruments .... Check & Set
[ ]  Engine Instruments .... Check

Taxi
[ ]  Brakes & Steering .... Check
[ ]  Flight Instruments .... Check
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Before Takeoff
[ ]  Seat Belts .... Secured
[ ]  Flight Controls .... Free & Correct
[ ]  Clock .... Check
[ ]  Fuel Quantity .... Check
[ ]  Flight Instruments .... Check & Set
[ ]  Radios / Avionics .... Set for Departure
[ ]  Fuel Shut off Valve .... ON
[ ]  Elevator Trim .... Check / Set
[ ]  Mixture .... Enrich
[ ]  Throttle .... 1800 RPM
[ ]  Mixture .... Set for Takeoff
[ ]  Magnetos .... Check (-175±50)
[ ]  Propeller .... Check (-300-500)
[ ]  Engine Instruments / Ammeter .... Check
[ ]  Vacuum .... Green Arc
[ ]  Throttle .... Idle / 1000 RPM
[ ]  Electrical Fuel Pump .... ON
[ ]  Cabin Doors .... Closed & Locked
[ ]  Lights (except taxi/takeoff) .... ON

Shutdown and Securing
[ ]  Avionics .... Off
[ ]  Exterior Lights (except beacon) .... Off as Required
[ ]  Throttle .... 1500 RPM
[ ]  Mixture .... Lean for 15 secs.
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... Idle Cut Off
[ ]  Magneto Switches .... Off
[ ]  Master Switch .... Off
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Controls .... Secure w/ lapbelt
[ ]  Post Flight Inspection .... Accomplish
[ ]  Internal and External Covers .... Install
[ ]  Tie downs and Chocks .... Install
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