Bellanca 8KCAB Decathlon — Sam_Dawson_8kcab_InFlight_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "After Landing" item count differs between passes (8 vs 4); verify nothing was dropped.
content_gap: Section "In Range-Descent" item count differs between passes (9 vs 7); verify nothing was dropped.
content_gap: Section "Turn-Time-Twist-Throttle-Talk" item count differs between passes (2 vs 3); verify nothing was dropped.

Final Before Take Off Check
[ ]  Heading .... Check aligned w/ runway
[ ]  Altimeter .... Field elevation
[ ]  Transponder .... ON
[ ]  Time .... Noted
[ ]  Strobes, lights .... All on
[ ]  Landing & TO lights .... On when cleared for Takeoff

Climb Check
[ ]  Throttle .... FULL OPEN
[ ]  Propeller Control .... FULL INCREASE
[ ]  Throttle .... Full
[ ]  Mixture .... Lean
[ ]  Airspeed .... 70-85 MPH
[ ]  Electrical Fuel Pump .... OFF after safe alt.

Cruise
[ ]  Level Off .... TRIM
[ ]  Airspeed .... ACCELERATE
[ ]  Power .... SET to cruise
[ ]  Mixture .... LEAN when below 75%
[ ]  Taxi/Landing Lights .... Off

In Range-Descent
[ ]  ATIS/AWOS/ASOS .... Received
[ ]  Altimeter .... Set

[ ]  Seat Belts .... secured

[ ]  Mixture .... SET
[ ]  Landing Light/Taxi Light .... ON
[ ]  Avionics .... SET
[ ]  Approach Briefing .... Complete

Turn-Time-Twist-Throttle-Talk
NOTE: Vx-58, Vy-80, Cruise Climb- 75-80, Va-121 (normal) 132(acrobatic), Vref-70-75, Vref short- 60 (all speeds MPH)
NOTE: 11 July 2007 Blackhawk Aviation, El Paso, TX

Approach Brief
[ ]  Approach
[ ]  Frequency
[ ]  Final Approach Course
[ ]  FAF
[ ]  DH/MDA
[ ]  Approach Lights/PAPI/VASI
[ ]  TDZE, HAT/HAA
[ ]  MAP
[ ]  Missed Approach
[ ]  Notes
[ ]  Runway exit/taxi plan
[ ]  Terrain
[ ]  Min. Alt., MAP & Climb Out

Before Landing
[ ]  Seat Belts .... Fastened
[ ]  Propeller .... FULL increase
[ ]  Mixture .... RICH
[ ]  Electrical Fuel Pump .... ON
[ ]  Breaks .... CHECK FIRM
[ ]  Approach Speed .... 70-75 MPH

GO AROUND  [ABNORMAL]
[ ]  Throttle .... Full
[ ]  Carburetor Heat .... Cold
[ ]  Wing Flaps .... 20° Immediately
[ ]  Climb Speed .... 62 KIAS
[ ]  Wing Flaps .... 10° (until obstacles clear), RETRACT (safe altitude & 60 KIAS)

After Landing
[ ]  Transponder .... Stby

[ ]  Strobes/lights .... Off as necessary
[ ]  Electric Fuel Pump .... OFF
[ ]  Taxi Clearance .... Obtain
NOTE: Turn-Time-Twist-Tap-Throttle-Talk
NOTE: Vx-58, Vy-80, Cruise Climb- 75-80, Va-121 (normal) 132 (acrobat), Vref-70-75, Vref short- 65 (all speeds MPH)
NOTE: 11 July 2007 Blackhawk Aviation, El Paso, Texas
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