Cessna 152 — Matthew_Kudija_Cessna_152_NORMAL_PROCEDURES
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "After Takeoff" item count differs between passes (9 vs 3); verify nothing was dropped.
content_gap: Section "Before Taxi" item count differs between passes (5 vs 4); verify nothing was dropped.
content_gap: Section "Engine Start" item count differs between passes (21 vs 20); verify nothing was dropped.
content_gap: Section "Landing" item count differs between passes (16 vs 15); verify nothing was dropped.
content_gap: Section "Maneuvers" item count differs between passes (27 vs 23); verify nothing was dropped.
content_gap: Section "Takeoff" item count differs between passes (34 vs 31); verify nothing was dropped.
content_gap: Section "Taxiing" item count differs between passes (3 vs 2); verify nothing was dropped.

Engine Start
BEFORE STARTING
[ ]  Preflight .... COMPLETE
[ ]  Seat Position .... LOCK
[ ]  Seatbelts .... ON
[ ]  Fuel Shutoff .... ON
[ ]  Radios .... OFF
[ ]  Brakes .... SET
[ ]  Circuit Breakers .... IN

STARTING ENGINE
[ ]  Mixture .... RICH
[ ]  Carb Heat .... COLD
[ ]  Primer .... PRIME
[ ]  Throttle .... ¼”
[ ]  Master .... ON
[ ]  Beacon .... ON
[ ]  Radios .... OFF
[ ]  Area .... CLEAR
[ ]  Ignition .... ENGAGE
[ ]  Throttle .... 1000 RPM
[ ]  Oil Press .... IN GREEN

Before Taxi
[ ]  ATIS .... 120.6
[ ]  Transponder .... SBY
[ ]  Nav Lights .... ON
[ ]  Landing Lights .... ON
[ ]  Flaps .... UP

Taxiing
[ ]  Clearance .... 121.6
[ ]  Controls .... SET FOR WIND
[ ]  Brakes .... STOP TO CHECK

Takeoff
BEFORE TAKEOFF
[ ]  Cabin Doors .... CLOSED
[ ]  Windows .... CLOSED
[ ]  Flight Controls .... CORRECT
[ ]  Elevator Trim .... T.O.
[ ]  Flight Inst. .... ALT, COMPASS
[ ]  Comm/VOR .... SET
[ ]  All Lights .... ON

RUN UP
[ ]  Fuel Shutoff .... ON
[ ]  Mixture .... RICH
[ ]  Brake .... SET
[ ]  Throttle .... 1700 RPM
[ ]  Mags .... CHECK
[ ]  Carb Heat .... ON>OFF
[ ]  Vacuum .... IN GREEN
[ ]  Throttle .... IDLE
[ ]  Carb Heat .... ON>OFF
[ ]  Throttle .... 1000 RPM
[ ]  Friction Lock .... ADJUST
[ ]  Alternator .... OFF>ON
[ ]  Transponder .... ALT

TAKEOFF
[ ]  Tower .... 124.0
[ ]  Strobe .... ON
[ ]  Flaps .... AS DESIRED
[ ]  Carb Heat .... OFF
[ ]  Elevator Trim .... SET
[ ]  Heading Indic .... SET
[ ]  Engine Instrum .... CK
[ ]  Rotate .... 50
[ ]  Climb .... 65-75

After Takeoff
[ ]  Airspeed .... 65-75
[ ]  Flaps .... RETRACT
[ ]  Landing Light .... OFF
AT CRUISE
[ ]  Landing Light .... OFF
[ ]  Attitude .... LEVEL
[ ]  Airspeed .... AS DESIRED
[ ]  Heading Indic .... ALIGN
[ ]  Mixture .... LEAN ABOVE 3000’

Landing
PRE-LANDING
[ ]  Seatbelts .... ON
[ ]  Mixture .... RICH
[ ]  Carb Heat .... ON
[ ]  Fuel Shutoff .... ON
[ ]  Landing Light .... ON
[ ]  Downwind .... 70
[ ]  Final .... 60-70

POST-LANDING
[ ]  Clear of Runway
[ ]  Flaps .... RETRACT
[ ]  Carb Heat .... OFF
[ ]  Elevator Trim .... TO
[ ]  Transponder .... SBY
[ ]  Strobe .... OFF

Engine Shutdown
[ ]  Radios .... ALL OFF
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... IDLE CUTOFF
[ ]  Ignition .... OFF
[ ]  All Lights .... OFF
[ ]  Master Switch .... OFF

Securing Airplane
[ ]  Control Lock .... SET
[ ]  Tiedowns .... ON
[ ]  Electrical .... ALL OFF
[ ]  Master .... OFF
[ ]  Flight Plan .... CLOSE

Maneuvers
BEFORE MANEUVERS
[ ]  Clear Area
[ ]  Altitude .... 1500 AGL
[ ]  Configure

SLOW FLIGHT/STALLS
[ ]  Power/Carb Heat
[ ]  Pitch
[ ]  Flaps

STALL RECOVERY
[ ]  Power/Carb Heat
[ ]  Pitch for Horizon
[ ]  Flaps Up

SAFE FLIGHT CHECKLIST
[ ]  Pilot
[ ]  Aircraft
[ ]  Weather
[ ]  Stress
[ ]  I .... ILLNESS
[ ]  M .... MEDICATION

[ ]  S .... STRESS
[ ]  A .... ALCOHOL
[ ]  F .... FATIGUE
[ ]  E .... EMOTION
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