Cessna 152 — Sam_Dawson_152n_ground_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Before Starting Engine
[ ]  Preflight Inspection .... Complete
[ ]  CRM/Passenger Briefing .... Complete
[ ]  Seats and Seat Belts .... Adjust & Lock
[ ]  Brakes .... Test & Set
[ ]  Fuel Selector .... ON
[ ]  Mixture .... Full Rich
[ ]  Throttle .... 1/2 inch
[ ]  Carburetor Heat .... Cold
[ ]  Avionics Master Switch .... Off
[ ]  Electrical Equipment .... Off
[ ]  Circuit Breakers .... Check In

Starting Engine
[ ]  Prime .... As Required
[ ]  Master Switch .... On
[ ]  Exterior Lights .... As Required
[ ]  Propeller Area .... Clear
[ ]  Ignition Switch .... Start
[ ]  Throttle .... 1000-1200 RPM
[ ]  Oil Pressure / Ammeter .... Check

Before Taxi
[ ]  Flaps .... Take Off Position
[ ]  Mixture .... Lean
[ ]  Throttle .... 1000 RPM
[ ]  Avionics Master (Radios) .... On
[ ]  ATIS / AWOS .... Receive
[ ]  Clearance .... Obtain
[ ]  Avionics / Transponder .... Set / STBY
[ ]  Flight Instruments .... Check & Set
[ ]  Engine Instruments .... Check

Taxi
[ ]  Brakes & Steering .... Check
[ ]  Flight Instruments .... Check

Before Takeoff
[ ]  Cabin Doors .... Closed & Locked
[ ]  Seats / Seat Belts .... Upright & Secured
[ ]  Flight Controls .... Free & Correct
[ ]  Clock .... Check
[ ]  Fuel Quantity .... Check
[ ]  Engine Instruments .... Check
[ ]  Flight Instruments .... Check & Set
[ ]  Radios / Avionics .... Set for Departure
[ ]  Fuel Selector .... ON
[ ]  Elevator Trim .... Check / Set
[ ]  Flaps .... Set for Takeoff
[ ]  Mixture .... Enrichen
[ ]  Throttle .... 1700 RPM
[ ]  Mixture .... Set for Takeoff
[ ]  Carb Heat .... Check
[ ]  Magnetos .... Check (±125/50)
[ ]  Engine Instruments / Ammeter .... Check
[ ]  Vacuum .... Green Arc
[ ]  Throttle .... Idle / 1000 RPM
[ ]  Departure Briefing .... Complete - Type T/O, Vr-, Vy-, Vx-, Emerg. Altitude

Shutdown and Securing
[ ]  Avionics Master Switch .... Off
[ ]  Exterior Lights (except beacon) .... Off
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... Idle Cut Off
[ ]  Magneto Switch .... Off
[ ]  Battery and Alternator .... Off
[ ]  Gust Lock .... Install
[ ]  Post Flight Inspection .... Accomplish
[ ]  Internal and External Covers .... Install
[ ]  Tie downs and Chocks .... Install
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