Cessna 182P Skylane — chris_leary_cessna182p_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

EXTERIOR INSPECTION
[ ]  AROW DOCS
[ ]  Plug in Headsets
[ ]  Remove Wheel Lock
[ ]  Master .... ON
[ ]  Gyros .... LISTEN
[ ]  Lights .... ON
[ ]  Pito Heat .... ON
[ ]  Flaps .... LOWER
[ ]  1) Lights .... CHECK
[ ]  2) Pito Tube .... CHECK
[ ]  Master .... OFF
LEFT
[ ]  Static Port .... CHECK
[ ]  Fuel Strainer .... CHECK
[ ]  Aileron .... CHECK
[ ]  Flap .... CHECK
[ ]  Strut / LDG Gear .... CHECK
[ ]  Fuselage .... CHECK
[ ]  Antennas .... CHECK
[ ]  H Stabaliser .... CHECK
[ ]  Elevator .... CHECK
[ ]  Rudder .... CHECK
RIGHT
[ ]  Fuselage .... CHECK
[ ]  Strut / LDG Gear .... CHECK
[ ]  Flap .... CHECK
[ ]  Aileron .... CHECK
[ ]  Fuel Strainer .... CHECK
[ ]  Static Port .... CHECK
[ ]  Oil .... CHECK
[ ]  Cowl flap .... CHECK
FRONT
[ ]  Nose / Prop .... CHECK
[ ]  Air Vents .... CHECK
[ ]  Nose Gear .... CHECK
NOTE: CHECK FUEL

PRE START CHECK LIST
NOTE: GET IN
[ ]  Adjust Seat
[ ]  Seat Belt
[ ]  Lap Board
[ ]  Close Door  (open window)
[ ]  Parking Break .... ON
[ ]  Avionics / Lights .... OFF
[ ]  Strobe .... ON
[ ]  Circuit Breakers .... IN
[ ]  Fuel Selector .... BOTH
[ ]  Cowl Flaps .... OPEN (closed cold)
[ ]  Trim (both) .... T/O
[ ]  Carb Heat .... IN/OFF
[ ]  Prime (as needed) .... (2/3 ish)
NOTE: ^ - In and locked

ENGINE START
[ ]  Visual .... CLEAR
[ ]  Master .... ON
[ ]  Flaps .... UP
[ ]  Mix/Prop .... IN
[ ]  Throttle .... 1/4 IN
[ ]  YELL  CLEAR .... CLEAR
[ ]  Starter .... ENGAGE
[ ]  Tach .... 1000 RPM
[ ]  Oil Pres. / Gages .... GREEN
[ ]  Lights .... ON
[ ]  Avionics Switch .... ON
[ ]  ATIS
[ ]  FREQUENCIES: -Ground, -ATC, -Flight Following
NOTE: CHECK  FUEL  GAGES
NOTE: TAXI >
NOTE: CHECK   BREAKS

RUN UP
[ ]  Parking Break .... SET
[ ]  Doors/Windows .... LOCKED
[ ]  Flight Controls .... FREE
[ ]  Insruments .... GREEN
[ ]  Auto Pilot .... OFF
[ ]  Mixture .... IN / FULL
[ ]  Fuel Selector .... BOTH
[ ]  Cowel Flaps .... OPEN
[ ]  Throttle .... 1700 RPM
[ ]  Magnetos  L/R (150 RPM drop max) .... CHECK
[ ]  Carb Heat .... CYCLE
[ ]  Prop .... CYCLE (3times)
[ ]  Ammeter .... CHECK charge
[ ]  Vacuum .... CHECK
[ ]  Throttle .... IDOL
[ ]  Flaps .... 10*
[ ]  Carb Heat .... IN
[ ]  Trim .... SET
[ ]  FREQUENCIES  /  CLOCK
[ ]  Heading Bug .... SET
[ ]  VOR .... SET
[ ]  Figure 7 visual check .... FLOOR – DASH
[ ]  HOLD SHORT – GET CLEARANCE
[ ]  LIGHTS  / CAMERA  / ACTION
[ ]  Landing Light .... ON
[ ]  Transponder .... ON
[ ]  FULL Power .... (Glance Instruments)

TAKE OFF / CLIMB
[ ]  Rotate     Vr .... 50kts / 60mph
[ ]  Climb           Vy .... 80kts / 90mph (rt. rudr)
[ ]  (Climb)           Vx .... (60kts / 70mph) 20* Flaps
NOTE: ----Lift Off----
[ ]  Touch Breaks .... LIFT OFF
[ ]  Landing Gear .... RETRACT
NOTE: ---500 AGL---
[ ]  FLAPS .... UP
[ ]  LANDING LIGHTS .... OFF
[ ]  ENROUTE CLIMB .... 100KTS/110MPH
[ ]  TRIM .... TRIM

CRUISE    (140 kts / 150mph)
[ ]  1) THROTTLE .... SET 22” – 24” MP
[ ]  2) PROP .... SET 2200 – 2400 RPM
CAUTION: avoid low RPM with high MP
[ ]  OPEN FLIGHT PLAN
[ ]  VOR .... SET
NOTE: [4000 ft or higher]
[ ]  Mixture .... SET/LEAN
[ ]  Carb Heat .... Still OFF
[ ]  Cowl Flaps .... CLOSED
[ ]  Headings: N E .... ODD + 500
[ ]  Headings: S W .... EVEN + 500

DECENT  /  APPROACH
[ ]  ATIS .... 10 miles out
[ ]  ATC / TRAFFIC .... 8 miles out
[ ]  Altimeter .... ADJUST
[ ]  AIRSPACE .... 5 miles out

BEFORE LANDING CHECKLIST
[ ]  Seat Belts .... FASTEN
[ ]  Fuel Selector .... BOTH
[ ]  MIX / PROP .... IN / FULL
[ ]  Master/Mags .... ON
[ ]  Engine Gages .... Green
[ ]  Auto Pilot .... OFF
NOTE: Enter pattern at TPA (don’t decend into it)
NOTE: Power for climb/decend, Pitch for speed
DOWNWIND ......,,,,,,,,,,,,TPA
[ ]  Power/Speed .... ADJUST 130kts / 140mph
[ ]  Flaps .... 10*
[ ]  LANDING GEAR .... DOWN   GREEN
[ ]  Abeam touchdown .... 15” MP
[ ]  Carb Heat .... ON
TURN  BASE ..................700  FT AGL
[ ]  Power/Speed .... ADJUST 95  kts
[ ]  Flaps .... 20*
[ ]  VSI .... 500 fpm
TURN  FINAL ...............500  FT AGL
[ ]  Flaps .... FULL*
[ ]  Power/Speed .... ADJUST 80  kts
[ ]  VSI .... 500 fpm
NOTE: [RUDDER CONTROL]
NOTE: [WATCH "P" FACTOR]
[ ]  Pull Throttle when the runway is made

GO AROUND
[ ]  Full Throttle
[ ]  Flaps .... 10*
[ ]  Carb Heat .... IN / OFF
[ ]  Cowl Flaps .... OPEN

AFTER LANDING CHECKLIST
[ ]  Flaps .... RETRACT
[ ]  Carb Heat .... IN / OFF
[ ]  Landing Light .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Trim .... T/O

SHUT DOWN
[ ]  Carb Heat .... OFF
[ ]  Avionics Switch .... OFF
[ ]  Mix, Mags, Master .... CUT / OFF
[ ]  Lights / Fuel Pump .... OFF
[ ]  Cowl Flaps .... CLOSED
NOTE: Readings: [HOBBS/TACH]

READINGS
[ ]  Vr .... 50kts / 60mph
[ ]  Vs .... 50kts / 60mph
[ ]  Full flaps .... 40kts / 50mph
[ ]  Vso   LGD Gear .... 50kts / 60mph
[ ]  Vs1 .... 55kts / 65mph
[ ]  Vy .... 80kts / 90mph
[ ]  Vx .... 60kts / 70mph
[ ]  Vfe .... 95kts / 110mph
[ ]  Va .... 110kts / 125mph
[ ]  Vno .... 140kts / 160mph
[ ]  Vne .... 175kts / 195mph
[ ]  MAX GROSS WEIGHT .... 2950 lbs.
NOTE: Models after “P”         3100 lbs.
[ ]  APPROACH SPEED Flaps Up .... 75kts / 85mph
[ ]  APPROACH SPEED Flaps Down .... 65kts / 75mph

ENGINE FAILURE / TAKE OFF ROLL  [EMERGENCY]
[ ]  Throttle .... CLOSED
[ ]  Breaks .... ON
[ ]  Mix, Mags, Master .... CUT / OFF

ENGINE FAILURE / TAKE OFF  [EMERGENCY]
[ ]  Pitch Best Glide .... 70kts
[ ]  Mix, Mags, Master .... CUT / OFF

ENGINE FAILURE / IN FLIGHT  [EMERGENCY]
[ ]  Best Glide .... 70kts
[ ]  Best Field
[ ]  Carb Heat .... ON
[ ]  Mix, Mags, Master .... ON
[ ]  Fuel Selector .... BOTH
[ ]  RESTART !
NOTE: NO:
[ ]  Mix, Mags, Master .... CUT / OFF
[ ]  Seat Belt .... ON

ENGINE FIRE AT START UP  [EMERGENCY]
[ ]  Keep Cranking
NOTE: IF STARTS
[ ]  Throttle .... 1800rpm
[ ]  Mix, Mags, Master .... OFF
NOTE: IF NO START
[ ]  Throttle .... FULL
[ ]  Mix .... CUT OFF
[ ]  Mags .... keep cranking
[ ]  GET GAS OUT OF LINE
[ ]  Mix, Mags, Master .... CUT / OFF
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