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Before Start
[ ]  Fasten Belts .... ON
[ ]  External Lights .... AS REQUIRED
[ ]  APU .... AS REQUIRED
[ ]  Flaps Bit .... CHECKED
[ ]  Air Conditioning .... AS REQUIRED
[ ]  Radio Master .... ON
[ ]  Instruments .... SET / X-CHECKED
[ ]  Radios/Radar/XPDR .... SET / STAND BY
[ ]  Fuel Totalizer .... SET
[ ]  Fuel Quantity .... CHECKED

Before Start 2
[ ]  Flight Recorder .... SET
[ ]  Power Levers .... GRD IDLE
[ ]  Condition Levers .... FUEL CUT OFF
[ ]  Press sys .... SET
[ ]  Parking Brake .... ON
[ ]  Flight Idle Stop CB .... CHECKED

Cleared to Start
[ ]  Windows .... CLOSED
[ ]  Door Lights .... OFF
[ ]  Rotating Beacon .... ON
[ ]  Fuel Pumps .... AS REQUIRED
[ ]  Radio Master .... OFF

After Start
[ ]  Electrical .... CHECKED / SET
[ ]  APU .... AS REQUIRED
[ ]  Fuel .... CHECHED / SET

After Start 2
[ ]  Auto Feather .... TESTED / ON
[ ]  Prop sync .... ON
[ ]  EEC .... CHECKED / TO or ON
[ ]  Hydraulic Power .... CHECKED / AUTO
[ ]  Ice/Rain Protection .... AS REQUIRED
[ ]  Pitot Static .... ON
[ ]  Air Conditioning .... SET
[ ]  Radio Master .... ON

Taxi
[ ]  Taxi Light .... ON
[ ]  Condition Levers .... FEATHER ONCE
[ ]  Take-off Data .... CHECKED
[ ]  Elev & Aileron Trim .... SET
[ ]  Take-off Briefing .... COMPLETED
[ ]  Flaps .... 15°
[ ]  Flight Controls .... CHECKED
[ ]  Cabin .... CLEAR

Cleared into Position
[ ]  Cab. ATT. Advisory .... GIVEN
[ ]  Landing Lights .... ON
[ ]  Strobe Lights .... ON
[ ]  Air Conditioning .... AS REQUIRED
[ ]  Transponder .... ALT
[ ]  Condition Levers .... MAX RPM
[ ]  Rudder Trim .... SET

After Take-off
[ ]  Gear .... UP - NO LIGHTS
[ ]  Flaps .... ZERO
[ ]  APU .... OFF or AS REQUIRED
[ ]  Auto Feather .... OFF
[ ]  Air Conditioning .... SET
[ ]  Altimeters .... 1013
[ ]  Pressurisation .... CHECKED
[ ]  Fasten Belts .... AS REQUIRED
[ ]  Landing Lights .... OFF

Descend
[ ]  W/S Heat .... AS REQUIRED
[ ]  W/S Defog .... ON
[ ]  Air Conditioning .... AS REQUIRED
[ ]  Landing Data .... CHECK
[ ]  Pressurization .... SET
[ ]  Approach Briefing .... COMPLETED
[ ]  Fasten Belts .... ON
[ ]  Landing Lights .... ON

Approach
[ ]  APU .... AS REQUIRED
[ ]  Autofeather .... ON
[ ]  Air Conditioning .... AS REQUIRED
[ ]  Altimeters .... SET
[ ]  Instruments & Radios .... SET
[ ]  Pressurization .... CHECKED
[ ]  Cab. Att. Advisory .... GIVEN

Before Landing
[ ]  W/S Heat .... AS REQUIRED
[ ]  Radar .... AS REQUIRED
[ ]  Gear .... DOWN - GREEN
[ ]  Flaps .... CHECKED - °/c Vref
[ ]  Condition Levers .... MAX RPM
[ ]  Yaw Damper .... OFF
[ ]  Cabin .... CLEAR

After Landing
[ ]  Landing Lights .... OFF
[ ]  Strobe Lights .... OFF
[ ]  Fuel Pumps .... AS REQUIRED
[ ]  Auto Feather .... OFF
[ ]  Prop sync .... OFF
[ ]  Ice/Rain Protection .... OFF
[ ]  Radar .... STANDBY
[ ]  Transponder .... STANDBY
[ ]  Trim Controls .... ZERO
[ ]  Pressurzation .... CHECKED
[ ]  Flaps .... ZERO

Shut-Down
[ ]  Inverters .... AS REQUIRED
[ ]  Main/Aux Generator .... OFF
[ ]  Fasten Belts .... OFF
[ ]  Emerg Lights .... AS REQUIRED
[ ]  External Lights .... AS REQUIRED
[ ]  Electric Hydraulic Pumps .... OFF
[ ]  Air Conditioning .... AS REQUIRED
[ ]  Stanby Horizon .... AS REQUIRED
[ ]  Back-up Battery .... AS REQUIRED
[ ]  Radio Master .... AS REQUIRED

Shut-Down 2
[ ]  Power Levers .... GRD IDLE
[ ]  Condition Levers .... FUEL CUT OFF
[ ]  Parking Brake .... ON
[ ]  PWR Select .... AS REQUIRED
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