Lancair 320 — L320-3 - Climb Checklist
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Climb Checklist
[ ]  Power .... 25"Hg, 2,500 RPM
[ ]  Flaps & Gear .... CHECK
NOTE: Cruise Climb 125 KIAS. Check power in climb, adjust Mixture for 10.0 GPH hot days, 9.5 GPH cool days. Max 1400( EGT.

Cruise Checklist
[ ]  Power .... 22"Hg, 2,400 RPM
[ ]  Mixture .... ADJUST
[ ]  Fuel .... TIME & MANAGE
NOTE: At 8,500 MSL, normal EGT = 1400(, FF = 7.6 GPH.

Descent Checklist
[ ]  Power .... 14"Hg, 2,300 RPM
[ ]  Mixture .... INCR. AS REQUIRED
[ ]  Approach Briefing .... COMPLETE
NOTE: Descent Planning: 4 to 1, + 5 Miles to decelerate.

Before Landing Checklist
[ ]  Mixture .... FULL RICH
[ ]  Prop .... HIGH RPM
[ ]  Gear [120 KIAS] .... DOWN, 3 GREEN
[ ]  Flaps [100 KIAS] .... AS REQUIRED
[ ]  Landing Clearance .... RECEIVED
NOTE: Approach Speed 75 - 80 KIAS Full Flaps. MFA Additive:  ½ Headwind + All Gusts Up To 90 KIAS.
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