Lancair 320 — L320-4 - After Landing Checklist
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After Landing Checklist
[ ]  Strobe Lights .... OFF
[ ]  Flaps .... UP
[ ]  Pitot Heat .... OFF
[ ]  Transponder .... STBY, 1200

Shut Down Checklist
[ ]  Electrical Switches .... OFF
[ ]  Avionics & GPS .... OFF
[ ]  Alternator & Avionics Master .... OFF
[ ]  Mixture .... CUTOFF
[ ]  Magneto Switches .... OFF
[ ]  Fuel Totalizer .... Note Fuel Remaining
[ ]  Cockpit Lights .... OFF
[ ]  Flaps .... DOWN
[ ]  Master Switch .... OFF
[ ]  Control Sticks .... SECURE
[ ]  Flight Log .... NOTE
[ ]  Canopy .... LOCK
NOTE: Attach Tow Bar and Cover. Insert Cowl Plugs after engine cools.
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