Mooney M20R Ovation 2 — Johnathan_Celso_MooneyM20R_Ovation2_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Before Takeoff" item count differs between passes (18 vs 19); verify nothing was dropped.
content_gap: Section "Descent" item count differs between passes (4 vs 5); verify nothing was dropped.
content_gap: Section "Landing" item count differs between passes (19 vs 17); verify nothing was dropped.
content_gap: Section "Securing Aircraft" item count differs between passes (10 vs 11); verify nothing was dropped.
content_gap: Section "Starting Engines" item count differs between passes (20 vs 21); verify nothing was dropped.

Preflight Inspection
CABIN
[ ]  A.R.R.O.W. .... Check
[ ]  Control Lock .... Remove
[ ]  Alternate Static Air .... Off
[ ]  Gear Selector .... Down
[ ]  Ignition Switch .... Off
[ ]  Master Switch .... On
[ ]  Fuel Quantity .... Check
[ ]  Battery Voltage .... Check
[ ]  Standby Vacuum .... Check
[ ]  Pitot Heat .... Check
[ ]  Trim .... Neutral
[ ]  Flaps .... Down/Check
[ ]  Master Switch .... Off
[ ]  Fire Extinguisher .... Charged/Secure
FUSELAGE/TAIL
[ ]  Skin/Windows .... Check
[ ]  Antennas .... Check
[ ]  Beacon/Strobe Lights .... Check
[ ]  Access Panels .... Secure
[ ]  Static Ports .... Check
[ ]  Static Drain Valve .... Push
[ ]  Fresh Air Vent .... Check
[ ]  Elevator/Rudder .... Inspect
[ ]  Tiedown .... Remove
LEFT WING
[ ]  Aileron/Flap .... Inspect
[ ]  Nav/Strobe/Recog Lights .... Check
[ ]  Pitot Tube Cover .... Check
[ ]  Pitot Tube .... Check
[ ]  Pitot Drain Valve .... Push
[ ]  Landing/Taxi Lights .... Check
[ ]  Stall Warning Vane .... Check
[ ]  Main Gear/Wheel .... Check
[ ]  Fuel Sumps .... Test
[ ]  Fuel Tank/Cap/Vent .... Check
[ ]  Wheel Chocks/Tiedown .... Remove
NOSE
[ ]  Air Inlets .... Check
[ ]  Engine Oil/Cap .... Check
[ ]  Engine Cowl .... Secure
[ ]  Propeller/Spinner .... Check
[ ]  Air Intakes .... Check
[ ]  Exhaust Pipes .... Check
[ ]  Nose Gear/Wheel .... Check
RIGHT WING
[ ]  Wheel Chocks/Tiedown .... Remove
[ ]  Fuel Sumps .... Test
[ ]  Fuel Tank/Cap/Vent .... Check
[ ]  Main Gear/Wheel .... Check
[ ]  Landing/Taxi Lights .... Check
[ ]  Nav/Strobe/Recog Lights .... Check
[ ]  Aileron/Flap .... Inspect
[ ]  Baggage Door .... Close/Lock

Before Starting Engine
[ ]  Preflight Inspection Completed
[ ]  Passengers .... Briefed
[ ]  Seatbelts .... Fastened
[ ]  Cabin Door .... Closed/Locked
[ ]  Parking Brake .... Set
[ ]  Fuel Selector .... Right Tank
[ ]  Gascolator .... Drain (5 Sec)
[ ]  Fuel Selector .... Left Tank
[ ]  Gascolator .... Drain (5 Sec)
[ ]  Gear Selector .... Down
[ ]  Circuit Breakers .... In
[ ]  Electrical Equipment .... Off
[ ]  Radio Master Switch .... Off
[ ]  Ignition Switch .... Off
[ ]  Alternate Air .... Off
[ ]  Propeller .... Full High
[ ]  Mixture .... Idle Cutoff
[ ]  Master Switch .... On
[ ]  Alternator .... On
[ ]  Rotating Beacon .... On

Starting Engines
NORMAL
[ ]  Throttle .... Open 1/4”
[ ]  Prime (Omit If Hot)
[ ]  Mixture .... Full Rich
[ ]  Boost Pump .... On (5 Sec)
[ ]  Mixture .... Idle Cutoff
[ ]  Propeller Area .... Clear
[ ]  Ignition Switch .... Both
[ ]  Starter .... Engage
[ ]  Mixture .... Enrich
[ ]  Throttle .... 1000 RPM
FLOODED
[ ]  Throttle .... Full Open
[ ]  Mixture .... Idle Cutoff
[ ]  Propeller Area .... Clear
[ ]  Ignition Switch .... Both
[ ]  Starter .... Engage
[ ]  Throttle .... Reduce
[ ]  Mixture .... Enrich
[ ]  Throttle .... 1000 RPM

Before Taxi
[ ]  Oil Pressure .... Check
[ ]  Mixture .... Lean
[ ]  Flaps .... Up
[ ]  Annunciator Panel .... Test
[ ]  ELT .... Arm
[ ]  Radio Master Switch .... On
[ ]  Transponder .... Standby
[ ]  Avionics .... Test/Set
[ ]  Clearance .... Obtain

Taxi
[ ]  Parking Brake .... Release
[ ]  Nav/Taxi Lights .... As Required
[ ]  Brakes/Steering .... Check
[ ]  Flight Instruments .... Check

Before Takeoff
[ ]  Parking Brake .... Set
[ ]  Fuel Selector .... Fullest Tank
[ ]  Mixture .... Full Rich
[ ]  Throttle .... 2000 RPM
[ ]  Magnetos .... Check
[ ]  Propeller .... Cycle
[ ]  Vacuum/Ammeter .... Check
[ ]  Engine Gauges .... Check
[ ]  Annunciator Panel .... Check
[ ]  Throttle .... 1000 RPM
[ ]  Flight Instruments .... Set
[ ]  Flight Controls .... Free/Correct
[ ]  Trim/Flaps .... Set Takeoff
[ ]  Boost Pump .... On
[ ]  Strobe/Recog Lights .... On
[ ]  Landing Lights .... As Required
[ ]  Transponder .... On/Altitude
[ ]  Parking Brake .... Release

Takeoff
NORMAL
[ ]  Throttle .... Full Open
[ ]  Rotate .... 67 KIAS
[ ]  Gear Selector .... Up
[ ]  Climb Speed .... 105 KIAS
[ ]  Flaps .... Up
[ ]  Boost Pump/Excess Lights .... Off
SHORT FIELD
[ ]  Brakes .... Apply
[ ]  Throttle .... Full Open
[ ]  Rotate .... 67 KIAS
[ ]  Climb Speed .... 85 KIAS
[ ]  Obstacles .... Clear
[ ]  Gear Selector .... Up
[ ]  Climb Speed .... 105 KIAS
[ ]  Flaps .... Up
[ ]  Boost Pump/Excess Lights .... Off

Climb
[ ]  Power .... Max MP/2500 RPM
[ ]  Mixture .... 100° Rich EGT
[ ]  Climb Speed .... 120 KIAS
[ ]  Trim .... Set

Cruise
[ ]  Power .... As Desired
[ ]  Mixture .... 50° Rich EGT
[ ]  Trim .... Set
[ ]  Fuel Selector .... Switch Tanks

Descent
[ ]  Power .... 20” MP/2000 RPM
[ ]  Mixture .... 25° Rich EGT
[ ]  Speed Brakes .... As Required
[ ]  Trim .... Set

Before Landing
[ ]  Seatbelts .... Fastened
[ ]  Fuel Selector .... Fullest Tank
[ ]  Parking Brake .... Released
[ ]  Propeller .... Full High
[ ]  Mixture .... Full Rich
[ ]  Flaps .... As Desired
[ ]  Approach Speed .... 90-100 KIAS
[ ]  Trim .... Set
[ ]  Boost Pump .... On
[ ]  Landing/Taxi Lights .... As Required

Landing
NORMAL
[ ]  Flaps .... Down
[ ]  Gear Selector .... Down/Check
[ ]  Approach Speed .... 80 KIAS
[ ]  Trim .... Set
[ ]  Touchdown .... Main Wheels First
[ ]  Throttle .... Idle
[ ]  Brakes .... Apply
[ ]  Flaps .... Up
SHORT FIELD
[ ]  Flaps .... Down
[ ]  Gear Selector .... Down/Check
[ ]  Speed Brakes .... Extended
[ ]  Approach Speed .... 75 KIAS
[ ]  Trim .... Set
[ ]  Touchdown .... Main Wheels First
[ ]  Throttle .... Idle
[ ]  Brakes .... Apply
[ ]  Flaps .... Up

Balked
[ ]  Throttle .... Full Open
[ ]  Positive Climb Rate .... Check
[ ]  Speed Brakes .... Retracted
[ ]  Flaps .... Set Takeoff
[ ]  Climb Speed .... 85 KIAS
[ ]  Obstacles .... Clear
[ ]  Gear Selector .... Up
[ ]  Climb Speed .... 105 KIAS
[ ]  Flaps .... Up

After Landing
[ ]  Landing/Strobe/Recog Lights .... Off
[ ]  Speed Brakes .... Retract
[ ]  Boost Pump .... Off
[ ]  Flaps .... Up
[ ]  Transponder .... Standby

Securing Aircraft
[ ]  Brakes .... Apply
[ ]  ELT .... Disarm
[ ]  Electrical Equipment .... Off
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... Idle Cutoff
[ ]  Engine .... Shutdown
[ ]  Ignition Switch .... Off
[ ]  Master Switch .... Off
[ ]  Alternator .... Off
[ ]  Locks/Chocks/Tiedowns .... Install

Close Flight Plan
[ ]  Close Flight Plan
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