Piper PA-24-250 Comanche — Mike_Tidmarsh_N84VK_WB_08_01_05
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content_gap: Section "Weight & Balance" item count differs between passes (67 vs 19); verify nothing was dropped.

Weight & Balance
WEIGHT & BALANCE FOR N84VK
NOTE: Modified by: Mike Tidmarsh - Date: 08/01/2005
[ ]  Basic Empty Wt .... 1879
[ ]  Basic Empty Wt — Lever Arm: 82.7
[ ]  Basic Empty Wt — Moment: 155393.30000000002
[ ]  Pilot .... 0
[ ]  Pilot — Weight (stone): 0
[ ]  Pilot — Weight (lbs): 0
[ ]  Pilot — Total Weight (lbs): 0
[ ]  Pilot — Lever Arm: 84.8
[ ]  Pilot — Moment: 0
[ ]  Front Passenger .... 0
[ ]  Front Passenger — Weight (stone): 0
[ ]  Front Passenger — Weight (lbs): 0
[ ]  Front Passenger — Total Weight (lbs): 0
[ ]  Front Passenger — Lever Arm: 84.8
[ ]  Front Passenger — Moment: 0
[ ]  Rear Passenger 1 .... 0
[ ]  Rear Passenger 1 — Weight (stone): 0
[ ]  Rear Passenger 1 — Weight (lbs): 0
[ ]  Rear Passenger 1 — Total Weight (lbs): 0
[ ]  Rear Passenger 1 — Lever Arm: 118.5
[ ]  Rear Passenger 1 — Moment: 0
[ ]  Rear Passenger 2 .... 0
[ ]  Rear Passenger 2 — Weight (stone): 0
[ ]  Rear Passenger 2 — Weight (lbs): 0
[ ]  Rear Passenger 2 — Total Weight (lbs): 0
[ ]  Rear Passenger 2 — Lever Arm: 118.5
[ ]  Rear Passenger 2 — Moment: 0
[ ]  Rear Baggage .... 0
[ ]  Rear Baggage — Lever Arm: 142
[ ]  Rear Baggage — Moment: 0
[ ]  UsbleFuel/Endur .... 0
[ ]  UsbleFuel/Endur — Total Weight (lbs): 0
[ ]  UsbleFuel/Endur — Lever Arm: 90
[ ]  UsbleFuel/Endur — Moment: 0
WEIGHT CHECK
[ ]  Weight Check — Lever Arm: 82.7
[ ]  Weight Check — Total Weight (lbs) .... 1879
[ ]  *** TOTAL *** — Weight (stone) .... 0
[ ]  *** TOTAL *** — Weight (lbs): 0
[ ]  *** TOTAL *** — Total Weight (lbs) .... 1879
[ ]  *** TOTAL *** — Lever Arm: 82.7
[ ]  *** TOTAL *** — Moment: 155393.30000000002
[ ]  Zero Fuel — Total Weight (lbs) .... 1879
[ ]  Zero Fuel — Lever Arm: 82.7
[ ]  Zero Fuel — Moment: 155393.30000000002
[ ]  Fuel — Lever Arm: 84
[ ]  Fuel — Moment: 1200
FUEL
[ ]  Fuel — Lever Arm: 84
[ ]  Fuel — Moment: 1650
[ ]  Full Fuel — Litres .... 212.24
[ ]  Full Fuel — US Gallons .... 56
[ ]  Full Fuel — Weight (lbs) .... 335.3392
[ ]  Full Fuel — Endurance (Hrs) .... 3.858909090909091
[ ]  Tip Tanks — Litres .... 113.7
[ ]  Tip Tanks — US Gallons .... 30
[ ]  Tip Tanks — Weight (lbs) .... 179.64600000000002
[ ]  Tip Tanks — Endurance (Hrs) .... 2.0672727272727274
[ ]  TOTALS: — Litres .... 325.94
[ ]  TOTALS: — US Gallons .... 86
[ ]  TOTALS: — Weight (lbs) .... 514.9852000000001
[ ]  TOTALS: — Endurance (Hrs) .... 5.926181818181819
[ ]  Lbs per Litre
[ ]  Lbs per Litre .... 1.58
[ ]  Calculator .... 0
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