Piper PA-28-161 Warrior II — paul_fawcett_warriorchecklist18
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "After Landing" item count differs between passes (3 vs 8); verify nothing was dropped.
content_gap: Section "Before Takeoff" item count differs between passes (23 vs 14); verify nothing was dropped.

Preflight Inspection
COCKPIT
[ ]  Electrical Equip. .... Off
[ ]  Avionics Master .... Off
[ ]  Circuit Breakers .... In
[ ]  Master Switch .... On
[ ]  Annunciators .... Chk on
[ ]  Turn Coordinator .... Chk flag
[ ]  Fuel Gauges .... Chk qty.
[ ]  Fuel Selector .... Low tank
[ ]  Static/Pitot .... Drain
[ ]  Fuel Pump - On .... Chk press.
[ ]  Lights .... Chk
[ ]  Master Switch .... Off
[ ]  Trims .... Chk
[ ]  Flaps .... Down
[ ]  Aircraft Docs .... AROW
RIGHT WING
[ ]  Flap .... Chk
[ ]  Aileron .... Chk
[ ]  Wingtip / lights .... Chk
[ ]  Leading edge .... Chk clean
[ ]  Fuel quantity .... Chk
[ ]  Fuel vent .... Clear
[ ]  Fuel strainer .... Sample
[ ]  Landing gear/tire .... Chk
[ ]  Air inlet .... Clear
NOSE
[ ]  Engine condition R .... Chk
[ ]  Oil quantity .... Chk
[ ]  Prop and spinner .... Chk
[ ]  Alternator belt .... Chk
[ ]  Air inlets .... Clear
[ ]  Exhaust stacks .... Chk
[ ]  Landing light .... Chk
[ ]  Nose gear, tire .... Chk
[ ]  Engine condition L .... Chk
[ ]  Brake reservoir .... Chk
LEFT WING
[ ]  As per right wing plus:
[ ]  Pitot / static mast .... Clear
[ ]  Stall horn .... Chk audio
[ ]  Nose fuel drain .... Chk (2x)
FUSELAGE & EMPENNAGE
[ ]  Antennas .... Chk
[ ]  Air inlet .... Chk
[ ]  Stabilator & trim .... Chk
[ ]  Jackscrew .... Chk
[ ]  Rudder / stab stops .... Chk
[ ]  Roll & "Big picture" .... Chk

Before Start
[ ]  Hobbs Time .... Record
[ ]  Charts .... Available
[ ]  Seats .... Adjust & lock
[ ]  Restraints .... Fastened
[ ]  Radio and elect. .... Off

Engine Start
[ ]  Brakes .... Set
[ ]  Carb heat .... Off
[ ]  Mixture .... Full rich
[ ]  Master switch .... On
[ ]  Fuel pump .... On
[ ]  Prime .... 3 times
[ ]  Tail beacon .... On
[ ]  Propellor .... Clear!
[ ]  Starter .... Engage
[ ]  Throttle .... Pump twice
[ ]  Throttle .... 1000 RPM
[ ]  Oil temperature .... Chk
[ ]  Oil pressure .... Chk
[ ]  Ammeter .... Chk
[ ]  Vacuum .... Chk
[ ]  Annunciators .... Out
[ ]  Mixture .... Lean for taxi
[ ]  Fuel pump off .... Chk press.

Before Taxi
[ ]  Flaps .... Up
[ ]  Avionics .... On
[ ]  Transponder .... 1200, stdby
[ ]  ATIS .... Copy
[ ]  Altimeter .... Set & chk
[ ]  Hdg indicator .... Set
[ ]  Parking brake .... Release
[ ]  Ground control .... Clearance

Taxi
[ ]  Brakes .... Chk R & L
[ ]  Turn coord. .... Chk in turn
[ ]  Directional gyro .... Chk in turn
[ ]  Compass .... Chk in turn
[ ]  Attitude indic. .... No D in turn

Run-Up
[ ]  Brakes .... Set
[ ]  Mixture .... Full rich
[ ]  Fuel pump .... On
[ ]  Fuel selector .... Switch tank
[ ]  Fuel pump - Off .... Chk press.
[ ]  Throttle .... 2000 RPM
[ ]  Magnetos .... <175, <50 dif
[ ]  Vacuum .... Chk (4.9-5.1)
[ ]  Annunciators .... Test
[ ]  Engine instr. .... In green
[ ]  Carb heat on .... Chk drop
[ ]  Throttle .... idle
[ ]  Carb heat .... Off
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... As required

Before Takeoff
[ ]  Circuit breakers .... Chk in
[ ]  Flight instr. .... Chk & set
[ ]  Comm. radio .... Set tower
[ ]  Pitot heat .... Load test
[ ]  Primer .... In & locked
[ ]  Flaps .... Set
[ ]  Trims .... Set both
[ ]  Controls .... Free & crct
[ ]  Doors / window .... Secured
[ ]  Seats belts .... Secured
[ ]  Briefing .... Complete
[ ]  Air conditioner .... Off
[ ]  Autopilot .... Off
[ ]  Tower .... Clearance
[ ]  Cleared for Takeoff
[ ]  Brakes .... Off
[ ]  Lights .... On
[ ]  Camera .... Xpdr ALT
[ ]  Action
[ ]  Mixture .... Full rich
[ ]  Fuel pump .... On
[ ]  Compass & DG .... Chk rwy hdg.
[ ]  Time off .... Noted

After Takeoff
[ ]  Flaps .... Up
[ ]  Fuel pump .... Off - chk pres.

Cruise
[ ]  Landing lights .... Off
[ ]  Throttle .... As req.
[ ]  Mixture .... Leaned

Approach
[ ]  Comm. radios .... Set
[ ]  Flight instrmts. .... Chk & set
[ ]  Fuel selector .... Best tank
[ ]  Fuel pump .... On
[ ]  Mixture .... Full rich
[ ]  Landing light .... On
[ ]  Brakes .... Chk
[ ]  Seats belts .... Secured

After Landing
[ ]  Throttle .... 1000 RPM
[ ]  Transponder .... Standby
[ ]  Carb heat .... Off

Shutdown
[ ]  Comm. radio .... Monitor 121.5
[ ]  Avionics .... Off
[ ]  Electr. equip. .... Off
[ ]  Throttle .... Idle
[ ]  Magnetos .... Chk GND
[ ]  Throttle .... 1200 RPM
[ ]  Mixture .... Idle Cutoff
[ ]  Magnetos/keys .... Off & out
[ ]  Master switch .... Off!!!!
[ ]  Hobbs/Tach .... Record

Speeds
[ ]  Vr .... 55
[ ]  Vx .... 63
[ ]  Vy .... 79
[ ]  Climb .... 87
[ ]  Vs .... 50
[ ]  Vso .... 44
[ ]  Va .... 88-111
[ ]  Vfe .... 103
[ ]  Vno .... 126
[ ]  Vne .... 160
[ ]  Glide .... 73
[ ]  Max dem.XW .... 17
[ ]  Vapp (flaps) .... 63

Airports and Frequencies
PAO
[ ]  ATIS .... 120.6
[ ]  GND .... 125.0
[ ]  TWR .... 118.6
SQL
[ ]  ATIS .... 125.9
[ ]  GND .... 121.6
[ ]  TWR .... 119.0
HAF
[ ]  UNICOM .... 122.8
LVK
[ ]  ATIS .... 119.65
[ ]  GND .... 121.6
[ ]  TWR .... 118.1

Engine Failure  [EMERGENCY]
[ ]  Altitude for restart??
NO
[ ]  Glide .... 73 Kts
[ ]  Landing Site .... Select
[ ]  Mixture .... Cut-off
[ ]  Master Switch .... Off
[ ]  Magnetos .... Off
[ ]  Fuel Selector .... Off
YES
[ ]  Fuel Selector .... Opp. tank
[ ]  Fuel Pump .... On
[ ]  Carb Heat .... On
[ ]  Mixture .... Full rich
[ ]  Throttle .... Adjust
[ ]  Primer .... Locked
[ ]  Magnetos .... Check
[ ]  Glide .... 73 Kts
[ ]  Engine restarted?
NO
[ ]  Mayday .... Transmit
[ ]  Transponder .... 7700
[ ]  Mixture .... Cut-off
[ ]  Fuel Selector .... Off
[ ]  Magnetos .... Off
[ ]  Master Switch .... Off

Engine Fire During Start  [EMERGENCY]
[ ]  Starter .... Engage
[ ]  Mixture .... Cut-off
[ ]  Throttle .... Open
[ ]  Fuel Pump .... Off
[ ]  Fuel Selector .... Off
WARNING: Evacuate if fire continues!

Engine Fire During Taxi  [EMERGENCY]
[ ]  Airplane .... Stop
[ ]  Mixture .... Cut-off
[ ]  Fuel Selector .... Off
[ ]  Master switch .... Off
WARNING: Evacuate Aircraft

Engine Fire In Flight  [EMERGENCY]
[ ]  Mixture .... Cut-off
[ ]  Fuel selector .... Off
[ ]  Glide .... 73 Kts
[ ]  Mayday .... Transmit
[ ]  Transponder .... 7700
[ ]  Magnetos .... Off
[ ]  Master switch .... Off

Cabin Fire in Flight  [EMERGENCY]
[ ]  Master switch .... Off
[ ]  Electrical equip. .... Off
[ ]  Cabin heater .... Off
[ ]  Vents .... Open

Low Fuel Pressure  [EMERGENCY]
[ ]  Fuel pump .... On
[ ]  Fuel selector .... Opp. tank

Engine Roughness  [EMERGENCY]
[ ]  Carb heat .... On
[ ]  Still rough after 1 min?
[ ]  Carb heat .... Off
[ ]  Mixture .... Adjust
[ ]  Fuel pump .... On
[ ]  Fuel selector .... Opp. tank
[ ]  Engine instr. .... Chk
[ ]  Magnetos .... Chk

Loss of Oil Pressure or High Oil Temperature  [EMERGENCY]
WARNING: Land as soon as possible
WARNING: Prepare for engine failure

Spin Recovery  [EMERGENCY]
[ ]  Throttle .... Idle
[ ]  Ailerons .... Neutral
[ ]  Rudder .... Against spin
[ ]  Yoke .... Full forward
[ ]  Rotation stopped?
[ ]  Rudder .... Neutral
[ ]  Yoke .... Neutral
[ ]  Pitch .... Level
[ ]  Throttle .... As required

Electrical Failure  [EMERGENCY]
[ ]  Ammeter .... Verify inop.
[ ]  Load is zero?
[ ]  Alternator .... Off
[ ]  Electrical load .... Minimize
[ ]  Alt. circ. brkr. .... Chk & reset
[ ]  Alternator .... On
[ ]  Power not restored?
[ ]  Alternator .... Off
[ ]  Electrical load .... Minimize
WARNING: Land as soon as possible

Electrical Overload  [EMERGENCY]
[ ]  Alternator .... Off
[ ]  Battery .... On
[ ]  Loads reduced?
[ ]  Electrical load .... Minimize
WARNING: Land as soon as possible
[ ]  Not reduced?
[ ]  Alternator .... Off
[ ]  Battery .... As required
WARNING: Essential equipment only!

Carburetor Icing  [EMERGENCY]
[ ]  Carb heat .... On
[ ]  Mixture .... Adjust

Emergency Frequencies  [EMERGENCY]
[ ]  Frequency .... 121.5
[ ]  Transponder .... 7700

Xwind Component
[ ]  0.5 .... 30 deg.
[ ]  0.7 .... 45 deg.
[ ]  0.9 .... 60 deg.
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