Piper PA-28-181 Archer II_III — carl_kintanar_archer_2_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Cockpit
[ ]  Weight/Balance .... IN LIMITS
[ ]  Line Box .... LOCKED
[ ]  Parking Brake .... SET
[ ]  Control Lock .... REMOVE
[ ]  Ignition .... OFF
[ ]  Ignition Key .... ON DASH
[ ]  Mag Compass .... CHECK
[ ]  Hobbs .... RECORD
[ ]  Tach .... VERIFY
[ ]  Transponder .... OFF
[ ]  Fan .... OFF
[ ]  Pitot Heat .... OFF
[ ]  All Lights .... OFF
[ ]  Avionics .... OFF
[ ]  Master Switch .... ON
[ ]  Annunciator Panel .... TEST
[ ]  Fuel Quantity .... CHECK
[ ]  Exterior Lights .... CHECK
[ ]  Master Switch .... OFF
[ ]  Flaps .... 10 deg
[ ]  Pitot/Static Drains .... CLOSE
[ ]  Aircraft Documents .... ON BOARD

Exterior Inspection
[ ]  Right Flap .... CHECK
[ ]  Aileron .... CHECK
[ ]  Fuel Quantity .... CHECK
[ ]  Tie Down .... REMOVE
[ ]  Fuel Sump .... SAMPLE
[ ]  Fuel Vent .... CLEAR
[ ]  Wing Leading Edge .... CHECK
[ ]  Air Inlet .... CHECK
[ ]  Wheel/Brake .... CHECK
[ ]  Chocks .... REMOVE
[ ]  Engine Oil Level .... MIN 5 qts
[ ]  Right Cowling .... SECURE
[ ]  Propeller/Spinner .... CHECK
[ ]  Engine Air Intake .... CLEAR
[ ]  Alternator Belt .... CHECK
[ ]  Landing Light .... CHECK
[ ]  Carb Air Filter .... CHECK
[ ]  Nose Gear .... CHECK
[ ]  Nose Chocks .... REMOVE
[ ]  Left Cowling .... SECURE
[ ]  Fuel Strainer (Nose) .... SAMPLE
[ ]  Wing Leading Edge .... CHECK
[ ]  Air Inlet .... CHECK
[ ]  Fuel Quantity .... CHECK
[ ]  Tie Down .... REMOVE
[ ]  Fuel Sump .... SAMPLE
[ ]  Wheel/Brake .... CHECK
[ ]  Chocks .... REMOVE
[ ]  Pitot/Static Head .... CLEAR
[ ]  Fuel Vent .... CLEAR
[ ]  Stall Opening .... CLEAR
[ ]  Aileron .... CHECK
[ ]  Flap .... CHECK
[ ]  Fuselage Left Side .... CHECK
[ ]  Antennas .... CHECK
[ ]  Elevator .... CHECK
[ ]  Elevator Trim .... CHECK
[ ]  Rudder .... CHECK
[ ]  Rudder Trim .... CHECK
[ ]  Tail Tie Down .... REMOVE
[ ]  Fuselage Right Side .... CHECK

Before Engine Start
[ ]  Flaps .... UP
[ ]  Seats .... ADJUSTED
[ ]  Seatbelts/Shoulder .... FASTENED
[ ]  Master Switch .... ON
[ ]  Anti Collision Lights .... ON
[ ]  Fuel Selector .... LOWEST
[ ]  Parking Brake .... SET
[ ]  Brake .... SET
[ ]  Fuel Pump .... ON
[ ]  Mixture .... RICH
[ ]  Throttle .... ¼” OPEN
[ ]  Prime .... AS REQUIRED
[ ]  Prop Area .... CLEAR!
[ ]  Starter .... ENGAGE
[ ]  Throttle .... 1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Engine Instruments .... CHECK
[ ]  Fuel Pump .... OFF
[ ]  Primer .... LOCKED

Before Taxi
[ ]  Fan .... AS REQUIRED
[ ]  Defrost .... AS REQUIRED
[ ]  Cabin Heat .... AS REQUIRED
[ ]  Pitot Heat .... AS REQUIRED
[ ]  Annunciator .... TEST
[ ]  Avionics .... ON
[ ]  Comm Radios .... SET
[ ]  Rnav/Nav Mode .... SET
[ ]  Nav Radios .... SET
[ ]  Transponder .... STDBY 1200
[ ]  Circuit Breakers .... IN
[ ]  Fuel Selector .... FULLEST
[ ]  ATIS/Weather .... CHECK
[ ]  Taxi Clearance .... AS REQUIRED
[ ]  Parking Brake .... RELEASE
[ ]  Brakes .... CHECK

Before Takeoff
[ ]  Parking Brake .... SET
[ ]  Brakes .... SET
[ ]  Mixture .... RICH
[ ]  Throttle .... 2000 RPM
[ ]  Engine Instruments .... IN LIMITS
[ ]  Suction .... CHECK
[ ]  Ammeter .... CHECK
[ ]  Magnetos .... CHECK
[ ]  Carb Heat .... CHECK
[ ]  Throttle .... IDLE
[ ]  RPM/Oil Pressure .... IN LIMITS
[ ]  Throttle .... 1000 RPM
[ ]  Flight Controls .... FREE / CORRECT
[ ]  Flight Instruments .... CHECK / SET
[ ]  Comm Radios .... SET
[ ]  Flaps .... UP
[ ]  Trim .... SET
[ ]  Takeoff Briefing .... COMPLETE
[ ]  Door and Window .... SECURE
[ ]  Autopilot .... OFF
[ ]  Fuel Pump .... ON
[ ]  Strobes .... ON
[ ]  Landing Light .... ON
[ ]  Transponder .... ALT 1200
[ ]  Parking Brake .... RELEASE
[ ]  Takeoff Clearance .... AS REQUIRED

After Takeoff
[ ]  Flaps .... UP
[ ]  Fuel Pump .... OFF

Cruise
[ ]  Throttle .... CRUISE RPM
[ ]  Mixture .... LEAN
[ ]  Landing Light .... AS REQUIRED
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Selector .... SET
[ ]  Engine Instruments .... CHECK
[ ]  Flight Instruments .... CHECK

Approach
[ ]  ATIS/Weather .... CHECK
[ ]  Comm Radios .... SET
[ ]  Nav Radios .... SET
[ ]  Flight Instruments .... CHECK / SET
[ ]  Engine Instruments .... CHECK
[ ]  Landing Light .... ON
[ ]  Fuel Pump .... ON
[ ]  Mixture .... RICH
[ ]  Fuel Selector .... FULLEST
[ ]  Approach Briefing .... COMPLETE
[ ]  Seats .... ADJUSTED
[ ]  Seat Belts .... FASTENED
[ ]  Autopilot .... OFF

After Landing
[ ]  Transponder .... OFF
[ ]  Fuel Pump .... OFF
[ ]  Landing Light .... OFF
[ ]  Strobes .... OFF
[ ]  Flaps .... UP
[ ]  Taxi Clearance .... AS REQUIRED

Parking
[ ]  Parking Brake .... SET
[ ]  Avionics .... OFF
[ ]  Pitot Heat .... OFF
[ ]  All Lights .... OFF
[ ]  Fan .... OFF
[ ]  Carb Heat .... OFF
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... CUT OFF
[ ]  Master Switch .... OFF
[ ]  Ignition .... OFF

Securing Aircraft
[ ]  Flight Plan .... CLOSED
[ ]  Tie Downs .... SECURE
[ ]  Chocks .... SECURE
[ ]  Door and Window .... SECURE
[ ]  Keys .... SECURE
[ ]  Fuel .... FULL (DPA)
[ ]  Hobbs .... RECORD (DPA)
[ ]  Tach .... RECORD (DPA)
[ ]  Flight Controls .... SECURE (DPA)
[ ]  Extra Oil .... REPLACE (DPA)
[ ]  Fuel Card .... IN LOGBOOK (DPA)
[ ]  Logbook .... LINEBOX? (DPA)
[ ]  Line Box .... LOCKED (DPA)
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